Technology pcb
class com.sun.electric.technology.Technology
shortName=null
techDesc=Printed Circuit Board (eight-layer)
Bits:  NONEGATEDARCS
isScaleRelevant=truepcb.Scale=1270000.0(1270000.0)
pcb.Foundry=NONE(NONE)
pcb.NumMetalLayers=8(8)
pcb.MininumResistance=10.0(10.0)
pcb.GateLengthSubtraction=0.0(0.0)
pcb.Gate Inclusion=false(false)
pcb.Ground Net Inclusion=false(false)
pcb.MaxSeriesResistance=10.0(10.0)
pcb.LogicalEffort.GateCapacitance=0.4(0.4)
pcb.LogicalEffort.WireRatio=0.16(0.16)
pcb.LogicalEffort.DiffAlpha=0.7(0.7)
ResolutionValueForpcb=0.0
TRANSPARENT_1=ff000000
TRANSPARENT_2=ffff0000
TRANSPARENT_3=ff00ff00
TRANSPARENT_4=ff0000ff
TRANSPARENT_5=ffffff00
Layer Signal1 METAL1
	pcb.CIF.Signal1=PC1(PC1)
	pcb.DXF.Signal1=()
	pcb.Skill.Signal1=()
	pcb.Resistance.Signal1=0.0(0.0)
	pcb.Capacitance.Signal1=0.0(0.0)
	pcb.EdgeCapacitance.Signal1=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=1(1)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Signal2 METAL2
	pcb.CIF.Signal2=PC2(PC2)
	pcb.DXF.Signal2=()
	pcb.Skill.Signal2=()
	pcb.Resistance.Signal2=0.0(0.0)
	pcb.Capacitance.Signal2=0.0(0.0)
	pcb.EdgeCapacitance.Signal2=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=2(2)
	color=ffff0000(ff0000)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Signal3 METAL3
	pcb.CIF.Signal3=PC3(PC3)
	pcb.DXF.Signal3=()
	pcb.Skill.Signal3=()
	pcb.Resistance.Signal3=0.0(0.0)
	pcb.Capacitance.Signal3=0.0(0.0)
	pcb.EdgeCapacitance.Signal3=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=3(3)
	color=ff00ff00(ff00)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Signal4 METAL4
	pcb.CIF.Signal4=PC4(PC4)
	pcb.DXF.Signal4=()
	pcb.Skill.Signal4=()
	pcb.Resistance.Signal4=0.0(0.0)
	pcb.Capacitance.Signal4=0.0(0.0)
	pcb.EdgeCapacitance.Signal4=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=4(4)
	color=ff0000ff(ff)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Signal5 METAL5
	pcb.CIF.Signal5=PC5(PC5)
	pcb.DXF.Signal5=()
	pcb.Skill.Signal5=()
	pcb.Resistance.Signal5=0.0(0.0)
	pcb.Capacitance.Signal5=0.0(0.0)
	pcb.EdgeCapacitance.Signal5=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=5(5)
	color=ffffff00(ffff00)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Signal6 METAL6
	pcb.CIF.Signal6=PC6(PC6)
	pcb.DXF.Signal6=()
	pcb.Skill.Signal6=()
	pcb.Resistance.Signal6=0.0(0.0)
	pcb.Capacitance.Signal6=0.0(0.0)
	pcb.EdgeCapacitance.Signal6=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffffff00(ffff00)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Signal7 METAL7
	pcb.CIF.Signal7=PC7(PC7)
	pcb.DXF.Signal7=()
	pcb.Skill.Signal7=()
	pcb.Resistance.Signal7=0.0(0.0)
	pcb.Capacitance.Signal7=0.0(0.0)
	pcb.EdgeCapacitance.Signal7=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffffbe06(ffbe06)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Signal8 METAL8
	pcb.CIF.Signal8=PC8(PC8)
	pcb.DXF.Signal8=()
	pcb.Skill.Signal8=()
	pcb.Resistance.Signal8=0.0(0.0)
	pcb.Capacitance.Signal8=0.0(0.0)
	pcb.EdgeCapacitance.Signal8=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff00ffff(ffff)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Power1 METAL1
	pcb.CIF.Power1=PN1(PN1)
	pcb.DXF.Power1=()
	pcb.Skill.Power1=()
	pcb.Resistance.Power1=0.0(0.0)
	pcb.Capacitance.Power1=0.0(0.0)
	pcb.EdgeCapacitance.Power1=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=1(1)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Power2 METAL2
	pcb.CIF.Power2=PN2(PN2)
	pcb.DXF.Power2=()
	pcb.Skill.Power2=()
	pcb.Resistance.Power2=0.0(0.0)
	pcb.Capacitance.Power2=0.0(0.0)
	pcb.EdgeCapacitance.Power2=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=2(2)
	color=ffff0000(ff0000)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Power3 METAL3
	pcb.CIF.Power3=PN3(PN3)
	pcb.DXF.Power3=()
	pcb.Skill.Power3=()
	pcb.Resistance.Power3=0.0(0.0)
	pcb.Capacitance.Power3=0.0(0.0)
	pcb.EdgeCapacitance.Power3=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=3(3)
	color=ff00ff00(ff00)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Power4 METAL4
	pcb.CIF.Power4=PN4(PN4)
	pcb.DXF.Power4=()
	pcb.Skill.Power4=()
	pcb.Resistance.Power4=0.0(0.0)
	pcb.Capacitance.Power4=0.0(0.0)
	pcb.EdgeCapacitance.Power4=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=4(4)
	color=ff0000ff(ff)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Power5 METAL5
	pcb.CIF.Power5=PN5(PN5)
	pcb.DXF.Power5=()
	pcb.Skill.Power5=()
	pcb.Resistance.Power5=0.0(0.0)
	pcb.Capacitance.Power5=0.0(0.0)
	pcb.EdgeCapacitance.Power5=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=5(5)
	color=ffffff00(ffff00)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Power6 METAL6
	pcb.CIF.Power6=PN6(PN6)
	pcb.DXF.Power6=()
	pcb.Skill.Power6=()
	pcb.Resistance.Power6=0.0(0.0)
	pcb.Capacitance.Power6=0.0(0.0)
	pcb.EdgeCapacitance.Power6=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffffff00(ffff00)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Power7 METAL7
	pcb.CIF.Power7=PN7(PN7)
	pcb.DXF.Power7=()
	pcb.Skill.Power7=()
	pcb.Resistance.Power7=0.0(0.0)
	pcb.Capacitance.Power7=0.0(0.0)
	pcb.EdgeCapacitance.Power7=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffffbe06(ffbe06)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Power8 METAL8
	pcb.CIF.Power8=PN8(PN8)
	pcb.DXF.Power8=()
	pcb.Skill.Power8=()
	pcb.Resistance.Power8=0.0(0.0)
	pcb.Capacitance.Power8=0.0(0.0)
	pcb.EdgeCapacitance.Power8=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff00ffff(ffff)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer TopSilk ART
	pcb.CIF.TopSilk=PSSC(PSSC)
	pcb.DXF.TopSilk=()
	pcb.Skill.TopSilk=()
	pcb.Resistance.TopSilk=0.0(0.0)
	pcb.Capacitance.TopSilk=0.0(0.0)
	pcb.EdgeCapacitance.TopSilk=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffe6e6e6(e6e6e6)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer BottomSilk ART
	pcb.CIF.BottomSilk=PSSS(PSSS)
	pcb.DXF.BottomSilk=()
	pcb.Skill.BottomSilk=()
	pcb.Resistance.BottomSilk=0.0(0.0)
	pcb.Capacitance.BottomSilk=0.0(0.0)
	pcb.EdgeCapacitance.BottomSilk=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff646464(646464)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer TopSolder METAL1
	pcb.CIF.TopSolder=PSMC(PSMC)
	pcb.DXF.TopSolder=()
	pcb.Skill.TopSolder=()
	pcb.Resistance.TopSolder=0.0(0.0)
	pcb.Capacitance.TopSolder=0.0(0.0)
	pcb.EdgeCapacitance.TopSolder=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffafffaf(afffaf)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer BottomSolder METAL8
	pcb.CIF.BottomSolder=PSMS(PSMS)
	pcb.DXF.BottomSolder=()
	pcb.Skill.BottomSolder=()
	pcb.Resistance.BottomSolder=0.0(0.0)
	pcb.Capacitance.BottomSolder=0.0(0.0)
	pcb.EdgeCapacitance.BottomSolder=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff599f55(599f55)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Drill CONTACT1 CONMETAL
	pcb.CIF.Drill=PD(PD)
	pcb.DXF.Drill=()
	pcb.Skill.Drill=()
	pcb.Resistance.Drill=0.0(0.0)
	pcb.Capacitance.Drill=0.0(0.0)
	pcb.EdgeCapacitance.Drill=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff020f9f(20f9f)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer DrillNonPlated ART
	pcb.CIF.DrillNonPlated=PDNP(PDNP)
	pcb.DXF.DrillNonPlated=()
	pcb.Skill.DrillNonPlated=()
	pcb.Resistance.DrillNonPlated=0.0(0.0)
	pcb.Capacitance.DrillNonPlated=0.0(0.0)
	pcb.EdgeCapacitance.DrillNonPlated=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff9696ff(9696ff)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Drawing ART
	pcb.CIF.Drawing=PF(PF)
	pcb.DXF.Drawing=()
	pcb.Skill.Drawing=()
	pcb.Resistance.Drawing=0.0(0.0)
	pcb.Capacitance.Drawing=0.0(0.0)
	pcb.EdgeCapacitance.Drawing=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffff9696(ff9696)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
ArcProto Signal-1 metal-1
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForSignal-1INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForSignal-1INpcb=45
	DefaultRigidForSignal-1INpcb=false
	DefaultFixedAngleForSignal-1INpcb=true
	DefaultExtendedForSignal-1INpcb=true
	DefaultDirectionalForSignal-1INpcb=false
		arcLayer layer=Signal1 style=FILLED extend=0.0
ArcProto Signal-2 metal-2
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForSignal-2INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForSignal-2INpcb=45
	DefaultRigidForSignal-2INpcb=false
	DefaultFixedAngleForSignal-2INpcb=true
	DefaultExtendedForSignal-2INpcb=true
	DefaultDirectionalForSignal-2INpcb=false
		arcLayer layer=Signal2 style=FILLED extend=0.0
ArcProto Signal-3 metal-3
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForSignal-3INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForSignal-3INpcb=45
	DefaultRigidForSignal-3INpcb=false
	DefaultFixedAngleForSignal-3INpcb=true
	DefaultExtendedForSignal-3INpcb=true
	DefaultDirectionalForSignal-3INpcb=false
		arcLayer layer=Signal3 style=FILLED extend=0.0
ArcProto Signal-4 metal-4
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForSignal-4INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForSignal-4INpcb=45
	DefaultRigidForSignal-4INpcb=false
	DefaultFixedAngleForSignal-4INpcb=true
	DefaultExtendedForSignal-4INpcb=true
	DefaultDirectionalForSignal-4INpcb=false
		arcLayer layer=Signal4 style=FILLED extend=0.0
ArcProto Signal-5 metal-5
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForSignal-5INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForSignal-5INpcb=45
	DefaultRigidForSignal-5INpcb=false
	DefaultFixedAngleForSignal-5INpcb=true
	DefaultExtendedForSignal-5INpcb=true
	DefaultDirectionalForSignal-5INpcb=false
		arcLayer layer=Signal5 style=FILLED extend=0.0
ArcProto Signal-6 metal-6
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForSignal-6INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForSignal-6INpcb=45
	DefaultRigidForSignal-6INpcb=false
	DefaultFixedAngleForSignal-6INpcb=true
	DefaultExtendedForSignal-6INpcb=true
	DefaultDirectionalForSignal-6INpcb=false
		arcLayer layer=Signal6 style=FILLED extend=0.0
ArcProto Signal-7 metal-7
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForSignal-7INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForSignal-7INpcb=45
	DefaultRigidForSignal-7INpcb=false
	DefaultFixedAngleForSignal-7INpcb=true
	DefaultExtendedForSignal-7INpcb=true
	DefaultDirectionalForSignal-7INpcb=false
		arcLayer layer=Signal7 style=FILLED extend=0.0
ArcProto Signal-8 metal-8
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForSignal-8INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForSignal-8INpcb=45
	DefaultRigidForSignal-8INpcb=false
	DefaultFixedAngleForSignal-8INpcb=true
	DefaultExtendedForSignal-8INpcb=true
	DefaultDirectionalForSignal-8INpcb=false
		arcLayer layer=Signal8 style=FILLED extend=0.0
ArcProto Power-1 metal-1
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPower-1INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForPower-1INpcb=45
	DefaultRigidForPower-1INpcb=false
	DefaultFixedAngleForPower-1INpcb=true
	DefaultExtendedForPower-1INpcb=true
	DefaultDirectionalForPower-1INpcb=false
		arcLayer layer=Power1 style=FILLED extend=0.0
ArcProto Power-2 metal-2
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPower-2INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForPower-2INpcb=45
	DefaultRigidForPower-2INpcb=false
	DefaultFixedAngleForPower-2INpcb=true
	DefaultExtendedForPower-2INpcb=true
	DefaultDirectionalForPower-2INpcb=false
		arcLayer layer=Power2 style=FILLED extend=0.0
ArcProto Power-3 metal-3
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPower-3INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForPower-3INpcb=45
	DefaultRigidForPower-3INpcb=false
	DefaultFixedAngleForPower-3INpcb=true
	DefaultExtendedForPower-3INpcb=true
	DefaultDirectionalForPower-3INpcb=false
		arcLayer layer=Power3 style=FILLED extend=0.0
ArcProto Power-4 metal-4
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPower-4INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForPower-4INpcb=45
	DefaultRigidForPower-4INpcb=false
	DefaultFixedAngleForPower-4INpcb=true
	DefaultExtendedForPower-4INpcb=true
	DefaultDirectionalForPower-4INpcb=false
		arcLayer layer=Power4 style=FILLED extend=0.0
ArcProto Power-5 metal-5
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPower-5INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForPower-5INpcb=45
	DefaultRigidForPower-5INpcb=false
	DefaultFixedAngleForPower-5INpcb=true
	DefaultExtendedForPower-5INpcb=true
	DefaultDirectionalForPower-5INpcb=false
		arcLayer layer=Power5 style=FILLED extend=0.0
ArcProto Power-6 metal-6
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPower-6INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForPower-6INpcb=45
	DefaultRigidForPower-6INpcb=false
	DefaultFixedAngleForPower-6INpcb=true
	DefaultExtendedForPower-6INpcb=true
	DefaultDirectionalForPower-6INpcb=false
		arcLayer layer=Power6 style=FILLED extend=0.0
ArcProto Power-7 metal-7
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPower-7INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForPower-7INpcb=45
	DefaultRigidForPower-7INpcb=false
	DefaultFixedAngleForPower-7INpcb=true
	DefaultExtendedForPower-7INpcb=true
	DefaultDirectionalForPower-7INpcb=false
		arcLayer layer=Power7 style=FILLED extend=0.0
ArcProto Power-8 metal-8
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPower-8INpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForPower-8INpcb=45
	DefaultRigidForPower-8INpcb=false
	DefaultFixedAngleForPower-8INpcb=true
	DefaultExtendedForPower-8INpcb=true
	DefaultDirectionalForPower-8INpcb=false
		arcLayer layer=Power8 style=FILLED extend=0.0
ArcProto Top-Silk nonelectrical
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForTop-SilkINpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForTop-SilkINpcb=45
	DefaultRigidForTop-SilkINpcb=false
	DefaultFixedAngleForTop-SilkINpcb=true
	DefaultExtendedForTop-SilkINpcb=true
	DefaultDirectionalForTop-SilkINpcb=false
		arcLayer layer=TopSilk style=FILLED extend=0.0
ArcProto Bottom-Silk nonelectrical
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForBottom-SilkINpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForBottom-SilkINpcb=45
	DefaultRigidForBottom-SilkINpcb=false
	DefaultFixedAngleForBottom-SilkINpcb=true
	DefaultExtendedForBottom-SilkINpcb=true
	DefaultDirectionalForBottom-SilkINpcb=false
		arcLayer layer=BottomSilk style=FILLED extend=0.0
ArcProto Top-Solder nonelectrical
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForTop-SolderINpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForTop-SolderINpcb=45
	DefaultRigidForTop-SolderINpcb=false
	DefaultFixedAngleForTop-SolderINpcb=true
	DefaultExtendedForTop-SolderINpcb=true
	DefaultDirectionalForTop-SolderINpcb=false
		arcLayer layer=TopSolder style=FILLED extend=0.0
ArcProto Bottom-Solder nonelectrical
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForBottom-SolderINpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForBottom-SolderINpcb=45
	DefaultRigidForBottom-SolderINpcb=false
	DefaultFixedAngleForBottom-SolderINpcb=true
	DefaultExtendedForBottom-SolderINpcb=true
	DefaultDirectionalForBottom-SolderINpcb=false
		arcLayer layer=BottomSolder style=FILLED extend=0.0
ArcProto Drawing nonelectrical
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForDrawingINpcb=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForDrawingINpcb=45
	DefaultRigidForDrawingINpcb=false
	DefaultFixedAngleForDrawingINpcb=true
	DefaultExtendedForDrawingINpcb=true
	DefaultDirectionalForDrawingINpcb=false
		arcLayer layer=Drawing style=FILLED extend=0.0
PrimitiveNode Signal-1-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-1-PinINpcb=0.625
	DefaultExtendYForSignal-1-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal1 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port signal-1 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-1
		portArc Power-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-2-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-2-PinINpcb=0.625
	DefaultExtendYForSignal-2-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal2 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port signal-2 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-2
		portArc Power-2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-3-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-3-PinINpcb=0.625
	DefaultExtendYForSignal-3-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal3 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port signal-3 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-3
		portArc Power-3
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-4-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-4-PinINpcb=0.625
	DefaultExtendYForSignal-4-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal4 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port signal-4 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-4
		portArc Power-4
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-5-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-5-PinINpcb=0.625
	DefaultExtendYForSignal-5-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal5 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port signal-5 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-5
		portArc Power-5
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-6-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-6-PinINpcb=0.625
	DefaultExtendYForSignal-6-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal6 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port signal-6 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-6
		portArc Power-6
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-7-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-7-PinINpcb=0.625
	DefaultExtendYForSignal-7-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal7 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port signal-7 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-7
		portArc Power-7
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-8-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-8-PinINpcb=0.625
	DefaultExtendYForSignal-8-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal8 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port signal-8 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-8
		portArc Power-8
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-1-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-1-PinINpcb=0.625
	DefaultExtendYForPower-1-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power1 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port power-1 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-1
		portArc Power-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-2-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-2-PinINpcb=0.625
	DefaultExtendYForPower-2-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power2 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port power-2 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-2
		portArc Power-2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-3-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-3-PinINpcb=0.625
	DefaultExtendYForPower-3-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power3 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port power-3 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-3
		portArc Power-3
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-4-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-4-PinINpcb=0.625
	DefaultExtendYForPower-4-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power4 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port power-4 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-4
		portArc Power-4
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-5-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-5-PinINpcb=0.625
	DefaultExtendYForPower-5-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power5 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port power-5 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-5
		portArc Power-5
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-6-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-6-PinINpcb=0.625
	DefaultExtendYForPower-6-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power6 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port power-6 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-6
		portArc Power-6
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-7-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-7-PinINpcb=0.625
	DefaultExtendYForPower-7-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power7 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port power-7 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-7
		portArc Power-7
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-8-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-8-PinINpcb=0.625
	DefaultExtendYForPower-8-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power8 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port power-8 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-8
		portArc Power-8
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Top-Silk-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForTop-Silk-PinINpcb=0.625
	DefaultExtendYForTop-Silk-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=TopSilk port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port top-silk angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Top-Silk
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Bottom-Silk-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForBottom-Silk-PinINpcb=0.625
	DefaultExtendYForBottom-Silk-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=BottomSilk port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port bottom-silk angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Bottom-Silk
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Top-Solder-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForTop-Solder-PinINpcb=0.625
	DefaultExtendYForTop-Solder-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=TopSolder port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port top-solder angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Top-Solder
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Bottom-Solder-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForBottom-Solder-PinINpcb=0.625
	DefaultExtendYForBottom-Solder-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=BottomSolder port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port bottom-solder angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Bottom-Solder
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Drill-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForDrill-PinINpcb=0.625
	DefaultExtendYForDrill-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Drill port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port drill angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Signal-1
		portArc Signal-2
		portArc Signal-3
		portArc Signal-4
		portArc Signal-5
		portArc Signal-6
		portArc Signal-7
		portArc Signal-8
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode NonPlated-Drill-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForNonPlated-Drill-PinINpcb=0.625
	DefaultExtendYForNonPlated-Drill-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=DrillNonPlated port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port nondrill angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Engineering-Drawing-Pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForEngineering-Drawing-PinINpcb=0.625
	DefaultExtendYForEngineering-Drawing-PinINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Drawing port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port engineering angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Drawing
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-1-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-1-NodeINpcb=0.625
	DefaultExtendYForSignal-1-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port signal-1 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-1
		portArc Power-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-2-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-2-NodeINpcb=0.625
	DefaultExtendYForSignal-2-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port signal-2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-2
		portArc Power-2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-3-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-3-NodeINpcb=0.625
	DefaultExtendYForSignal-3-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal3 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port signal-3 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-3
		portArc Power-3
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-4-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-4-NodeINpcb=0.625
	DefaultExtendYForSignal-4-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal4 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port signal-4 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-4
		portArc Power-4
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-5-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-5-NodeINpcb=0.625
	DefaultExtendYForSignal-5-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal5 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port signal-5 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-5
		portArc Power-5
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-6-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-6-NodeINpcb=0.625
	DefaultExtendYForSignal-6-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal6 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port signal-6 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-6
		portArc Power-6
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-7-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-7-NodeINpcb=0.625
	DefaultExtendYForSignal-7-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal7 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port signal-7 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-7
		portArc Power-7
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Signal-8-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSignal-8-NodeINpcb=0.625
	DefaultExtendYForSignal-8-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Signal8 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port signal-8 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-8
		portArc Power-8
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-1-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-1-NodeINpcb=0.625
	DefaultExtendYForPower-1-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port power-1 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-1
		portArc Power-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-2-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-2-NodeINpcb=0.625
	DefaultExtendYForPower-2-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port power-2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-2
		portArc Power-2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-3-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-3-NodeINpcb=0.625
	DefaultExtendYForPower-3-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power3 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port power-3 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-3
		portArc Power-3
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-4-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-4-NodeINpcb=0.625
	DefaultExtendYForPower-4-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power4 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port power-4 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-4
		portArc Power-4
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-5-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-5-NodeINpcb=0.625
	DefaultExtendYForPower-5-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power5 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port power-5 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-5
		portArc Power-5
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-6-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-6-NodeINpcb=0.625
	DefaultExtendYForPower-6-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power6 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port power-6 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-6
		portArc Power-6
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-7-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-7-NodeINpcb=0.625
	DefaultExtendYForPower-7-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power7 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port power-7 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-7
		portArc Power-7
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power-8-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPower-8-NodeINpcb=0.625
	DefaultExtendYForPower-8-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Power8 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port power-8 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Signal-8
		portArc Power-8
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Top-Silk-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForTop-Silk-NodeINpcb=0.625
	DefaultExtendYForTop-Silk-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=TopSilk port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port top-silk angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Top-Silk
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Bottom-Silk-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForBottom-Silk-NodeINpcb=0.625
	DefaultExtendYForBottom-Silk-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=BottomSilk port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port bottom-silk angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Bottom-Silk
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Top-Solder-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForTop-Solder-NodeINpcb=0.625
	DefaultExtendYForTop-Solder-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=TopSolder port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port top-solder angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Top-Solder
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Bottom-Solder-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForBottom-Solder-NodeINpcb=0.625
	DefaultExtendYForBottom-Solder-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=BottomSolder port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port bottom-solder angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Bottom-Solder
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Engineering-Drawing-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForEngineering-Drawing-NodeINpcb=0.625
	DefaultExtendYForEngineering-Drawing-NodeINpcb=0.625
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Drawing port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port engineering angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Drawing
		portArc Universal
		portArc Invisible
		portArc Unrouted
Foundry NONE
	pcb.GDS.Signal1=()
	pcb.GDS.Signal2=()
	pcb.GDS.Signal3=()
	pcb.GDS.Signal4=()
	pcb.GDS.Signal5=()
	pcb.GDS.Signal6=()
	pcb.GDS.Signal7=()
	pcb.GDS.Signal8=()
	pcb.GDS.Power1=()
	pcb.GDS.Power2=()
	pcb.GDS.Power3=()
	pcb.GDS.Power4=()
	pcb.GDS.Power5=()
	pcb.GDS.Power6=()
	pcb.GDS.Power7=()
	pcb.GDS.Power8=()
	pcb.GDS.TopSilk=()
	pcb.GDS.BottomSilk=()
	pcb.GDS.TopSolder=()
	pcb.GDS.BottomSolder=()
	pcb.GDS.Drill=()
	pcb.GDS.DrillNonPlated=()
	pcb.GDS.Drawing=()
 menu 0 0 arc Signal-1
 menu 0 1 arc Power-1
 menu 0 2 nodeInst Signal-1-Pin:pin:
 menu 0 3 nodeInst Power-1-Pin:pin:
 menu 1 0 arc Signal-2
 menu 1 1 arc Power-2
 menu 1 2 nodeInst Signal-2-Pin:pin:
 menu 1 3 nodeInst Power-2-Pin:pin:
 menu 2 0 arc Signal-3
 menu 2 1 arc Power-3
 menu 2 2 nodeInst Signal-3-Pin:pin:
 menu 2 3 nodeInst Power-3-Pin:pin:
 menu 3 0 arc Signal-4
 menu 3 1 arc Power-4
 menu 3 2 nodeInst Signal-4-Pin:pin:
 menu 3 3 nodeInst Power-4-Pin:pin:
 menu 4 0 arc Signal-5
 menu 4 1 arc Power-5
 menu 4 2 nodeInst Signal-5-Pin:pin:
 menu 4 3 nodeInst Power-5-Pin:pin:
 menu 5 0 arc Signal-6
 menu 5 1 arc Power-6
 menu 5 2 nodeInst Signal-6-Pin:pin:
 menu 5 3 nodeInst Power-6-Pin:pin:
 menu 6 0 arc Signal-7
 menu 6 1 arc Power-7
 menu 6 2 nodeInst Signal-7-Pin:pin:
 menu 6 3 nodeInst Power-7-Pin:pin:
 menu 7 0 arc Signal-8
 menu 7 1 arc Power-8
 menu 7 2 nodeInst Signal-8-Pin:pin:
 menu 7 3 nodeInst Power-8-Pin:pin:
 menu 8 0 arc Top-Silk
 menu 8 1 nodeInst Top-Silk-Pin:pin:
 menu 8 2 arc Bottom-Silk
 menu 8 3 nodeInst Bottom-Silk-Pin:pin:
 menu 9 0 arc Top-Solder
 menu 9 1 nodeInst Top-Solder-Pin:pin:
 menu 9 2 arc Bottom-Solder
 menu 9 3 nodeInst Bottom-Solder-Pin:pin:
 menu 10 0 arc Drawing
 menu 10 1 nodeInst Drill-Pin:pin:
 menu 10 2 nodeInst NonPlated-Drill-Pin:pin:
 menu 10 3 nodeInst Engineering-Drawing-Pin:pin:
 menu 11 0 Pure
 menu 11 1 Misc.
 menu 11 2 Cell
    <Foundry name="NONE">
    </Foundry>
