Technology rcmos
class com.sun.electric.technology.Technology
shortName=Round CMOS
techDesc=Complementary MOS (round, from MOSIS, P-Well, double metal)
Bits:  NONEGATEDARCS
isScaleRelevant=truercmos.Scale=2000.0(2000.0)
rcmos.Foundry=NONE(NONE)
rcmos.NumMetalLayers=2(2)
rcmos.MininumResistance=10.0(10.0)
rcmos.GateLengthSubtraction=0.0(0.0)
rcmos.Gate Inclusion=false(false)
rcmos.Ground Net Inclusion=false(false)
rcmos.MaxSeriesResistance=10.0(10.0)
rcmos.LogicalEffort.GateCapacitance=0.4(0.4)
rcmos.LogicalEffort.WireRatio=0.16(0.16)
rcmos.LogicalEffort.DiffAlpha=0.7(0.7)
ResolutionValueForrcmos=0.0
TRANSPARENT_1=ff60d1ff
TRANSPARENT_2=ffff9bc0
TRANSPARENT_3=ff6be260
TRANSPARENT_4=fff0ddb5
TRANSPARENT_5=ffe05fff
Layer Metal-1 METAL1
	rcmos.CIF.Metal-1=CMF(CMF)
	rcmos.DXF.Metal-1=()
	rcmos.Skill.Metal-1=()
	rcmos.Resistance.Metal-1=0.0(0.0)
	rcmos.Capacitance.Metal-1=0.0(0.0)
	rcmos.EdgeCapacitance.Metal-1=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=1(1)
	color=ff60d1ff(60d1ff)
	opacity=0.8(0.8)
	foreground=true
	pattern 2222 0 8888 0 2222 0 8888 0 2222 0 8888 0 2222 0 8888 0
	distance3D=16.5
	thickness3D=2.65
	mode3D=NONE
	factor3D=0.2
Layer Metal-2 METAL2
	rcmos.CIF.Metal-2=CMS(CMS)
	rcmos.DXF.Metal-2=()
	rcmos.Skill.Metal-2=()
	rcmos.Resistance.Metal-2=0.0(0.0)
	rcmos.Capacitance.Metal-2=0.0(0.0)
	rcmos.EdgeCapacitance.Metal-2=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=5(5)
	color=ffe05fff(e05fff)
	opacity=0.8(0.8)
	foreground=true
	pattern 1010 2020 4040 8080 101 202 404 808 1010 2020 4040 8080 101 202 404 808
	distance3D=22.15
	thickness3D=2.65
	mode3D=NONE
	factor3D=0.2
Layer Polysilicon POLY1
	rcmos.CIF.Polysilicon=CPG(CPG)
	rcmos.DXF.Polysilicon=()
	rcmos.Skill.Polysilicon=()
	rcmos.Resistance.Polysilicon=0.0(0.0)
	rcmos.Capacitance.Polysilicon=0.0(0.0)
	rcmos.EdgeCapacitance.Polysilicon=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=2(2)
	color=ffff9bc0(ff9bc0)
	opacity=0.8(0.8)
	foreground=true
	pattern 808 404 202 101 8080 4040 2020 1010 808 404 202 101 8080 4040 2020 1010
	distance3D=14.75
	thickness3D=1.0
	mode3D=NONE
	factor3D=0.2
Layer S-Active DIFF
	rcmos.CIF.S-Active=CAA(CAA)
	rcmos.DXF.S-Active=()
	rcmos.Skill.S-Active=()
	rcmos.Resistance.S-Active=0.0(0.0)
	rcmos.Capacitance.S-Active=0.0(0.0)
	rcmos.EdgeCapacitance.S-Active=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=3(3)
	color=ff6be260(6be260)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 303 4848 303 0 3030 8484 3030 0 303 4848 303 0 3030 8484 3030
	distance3D=9.0
	thickness3D=4.0
	mode3D=NONE
	factor3D=0.2
Layer D-Active DIFF
	rcmos.CIF.D-Active=CAA(CAA)
	rcmos.DXF.D-Active=()
	rcmos.Skill.D-Active=()
	rcmos.Resistance.D-Active=0.0(0.0)
	rcmos.Capacitance.D-Active=0.0(0.0)
	rcmos.EdgeCapacitance.D-Active=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=3(3)
	color=ff6be260(6be260)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 303 4848 303 0 3030 8484 3030 0 303 4848 303 0 3030 8484 3030
	distance3D=9.0
	thickness3D=4.0
	mode3D=NONE
	factor3D=0.2
Layer Select IMPLANTP
	rcmos.CIF.Select=CSG(CSG)
	rcmos.DXF.Select=()
	rcmos.Skill.Select=()
	rcmos.Resistance.Select=0.0(0.0)
	rcmos.Capacitance.Select=0.0(0.0)
	rcmos.EdgeCapacitance.Select=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=0(0)
	color=ffffff00(ffff00)
	opacity=0.8(0.8)
	foreground=true
	pattern 1010 2020 4040 8080 101 202 404 808 1010 2020 4040 8080 101 202 404 808
	distance3D=8.0
	thickness3D=5.0
	mode3D=NONE
	factor3D=0.2
Layer Well WELLP
	rcmos.CIF.Well=CWG(CWG)
	rcmos.DXF.Well=()
	rcmos.Skill.Well=()
	rcmos.Resistance.Well=0.0(0.0)
	rcmos.Capacitance.Well=0.0(0.0)
	rcmos.EdgeCapacitance.Well=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=4(4)
	color=fff0ddb5(f0ddb5)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 c0 0 0 0 c0 0 0 0 c0 0 0 0 c0 0 0
	distance3D=0.0
	thickness3D=13.0
	mode3D=NONE
	factor3D=0.2
Layer Contact-Cut CONTACT1
	rcmos.CIF.Contact-Cut=CC(CC)
	rcmos.DXF.Contact-Cut=()
	rcmos.Skill.Contact-Cut=()
	rcmos.Resistance.Contact-Cut=0.0(0.0)
	rcmos.Capacitance.Contact-Cut=0.0(0.0)
	rcmos.EdgeCapacitance.Contact-Cut=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=13.0
	thickness3D=3.5
	mode3D=NONE
	factor3D=0.2
Layer Via CONTACT2
	rcmos.CIF.Via=CVA(CVA)
	rcmos.DXF.Via=()
	rcmos.Skill.Via=()
	rcmos.Resistance.Via=0.0(0.0)
	rcmos.Capacitance.Via=0.0(0.0)
	rcmos.EdgeCapacitance.Via=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=19.15
	thickness3D=3.0
	mode3D=NONE
	factor3D=0.2
Layer Passivation OVERGLASS
	rcmos.CIF.Passivation=COG(COG)
	rcmos.DXF.Passivation=()
	rcmos.Skill.Passivation=()
	rcmos.Resistance.Passivation=0.0(0.0)
	rcmos.Capacitance.Passivation=0.0(0.0)
	rcmos.EdgeCapacitance.Passivation=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=0(0)
	color=ff646464(646464)
	opacity=0.8(0.8)
	foreground=true
	pattern 1c1c 3e3e 3636 3e3e 1c1c 0 0 0 1c1c 3e3e 3636 3e3e 1c1c 0 0 0
	distance3D=19.15
	thickness3D=5.0
	mode3D=NONE
	factor3D=0.2
Layer Poly-Cut CONTACT1
	rcmos.CIF.Poly-Cut=CCP(CCP)
	rcmos.DXF.Poly-Cut=()
	rcmos.Skill.Poly-Cut=()
	rcmos.Resistance.Poly-Cut=0.0(0.0)
	rcmos.Capacitance.Poly-Cut=0.0(0.0)
	rcmos.EdgeCapacitance.Poly-Cut=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=15.75
	thickness3D=0.75
	mode3D=NONE
	factor3D=0.2
Layer Active-Cut CONTACT1
	rcmos.CIF.Active-Cut=CCA(CCA)
	rcmos.DXF.Active-Cut=()
	rcmos.Skill.Active-Cut=()
	rcmos.Resistance.Active-Cut=0.0(0.0)
	rcmos.Capacitance.Active-Cut=0.0(0.0)
	rcmos.EdgeCapacitance.Active-Cut=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=13.0
	thickness3D=3.5
	mode3D=NONE
	factor3D=0.2
ArcProto Metal-1 metal-1
	isWipable=false
	isCurvable=true
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForMetal-1INrcmos=0.0
	baseExtend=1.5
	defaultLambdaBaseWidth=3.0
	diskOffset1=1.5
	diskOffset2=1.5
	DefaultAngleForMetal-1INrcmos=45
	DefaultRigidForMetal-1INrcmos=false
	DefaultFixedAngleForMetal-1INrcmos=true
	DefaultExtendedForMetal-1INrcmos=false
	DefaultDirectionalForMetal-1INrcmos=false
		arcLayer layer=Metal-1 style=FILLED extend=1.5
ArcProto Metal-2 metal-2
	isWipable=false
	isCurvable=true
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForMetal-2INrcmos=0.0
	baseExtend=1.5
	defaultLambdaBaseWidth=3.0
	diskOffset1=1.5
	diskOffset2=1.5
	DefaultAngleForMetal-2INrcmos=0
	DefaultRigidForMetal-2INrcmos=false
	DefaultFixedAngleForMetal-2INrcmos=false
	DefaultExtendedForMetal-2INrcmos=false
	DefaultDirectionalForMetal-2INrcmos=false
		arcLayer layer=Metal-2 style=FILLED extend=1.5
ArcProto Polysilicon poly-1
	isWipable=false
	isCurvable=true
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPolysiliconINrcmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=1.0
	diskOffset2=1.0
	DefaultAngleForPolysiliconINrcmos=0
	DefaultRigidForPolysiliconINrcmos=false
	DefaultFixedAngleForPolysiliconINrcmos=false
	DefaultExtendedForPolysiliconINrcmos=false
	DefaultDirectionalForPolysiliconINrcmos=false
		arcLayer layer=Polysilicon style=FILLED extend=1.0
ArcProto S-Active n-diffusion
	isWipable=false
	isCurvable=true
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForS-ActiveINrcmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=3.0
	diskOffset2=1.0
	DefaultAngleForS-ActiveINrcmos=0
	DefaultRigidForS-ActiveINrcmos=false
	DefaultFixedAngleForS-ActiveINrcmos=false
	DefaultExtendedForS-ActiveINrcmos=false
	DefaultDirectionalForS-ActiveINrcmos=false
		arcLayer layer=S-Active style=FILLED extend=1.0
		arcLayer layer=Select style=FILLED extend=3.0
ArcProto D-Active p-diffusion
	isWipable=false
	isCurvable=true
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForD-ActiveINrcmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=5.0
	diskOffset2=1.0
	DefaultAngleForD-ActiveINrcmos=0
	DefaultRigidForD-ActiveINrcmos=false
	DefaultFixedAngleForD-ActiveINrcmos=false
	DefaultExtendedForD-ActiveINrcmos=false
	DefaultDirectionalForD-ActiveINrcmos=false
		arcLayer layer=D-Active style=FILLED extend=1.0
		arcLayer layer=Well style=FILLED extend=5.0
ArcProto Substrate-Active substrate-diffusion
	isWipable=false
	isCurvable=true
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForSubstrate-ActiveINrcmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=1.0
	diskOffset2=1.0
	DefaultAngleForSubstrate-ActiveINrcmos=0
	DefaultRigidForSubstrate-ActiveINrcmos=false
	DefaultFixedAngleForSubstrate-ActiveINrcmos=false
	DefaultExtendedForSubstrate-ActiveINrcmos=false
	DefaultDirectionalForSubstrate-ActiveINrcmos=false
		arcLayer layer=D-Active style=FILLED extend=1.0
		arcLayer layer=S-Active style=FILLED extend=1.0
ArcProto Well-Active well-diffusion
	isWipable=false
	isCurvable=true
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForWell-ActiveINrcmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=3.0
	diskOffset2=1.0
	DefaultAngleForWell-ActiveINrcmos=0
	DefaultRigidForWell-ActiveINrcmos=false
	DefaultFixedAngleForWell-ActiveINrcmos=false
	DefaultExtendedForWell-ActiveINrcmos=false
	DefaultDirectionalForWell-ActiveINrcmos=false
		arcLayer layer=D-Active style=FILLED extend=1.0
		arcLayer layer=S-Active style=FILLED extend=1.0
		arcLayer layer=Well style=FILLED extend=3.0
		arcLayer layer=Select style=FILLED extend=3.0
ArcProto S-Transistor n-diffusion
	isWipable=false
	isCurvable=true
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForS-TransistorINrcmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=3.0
	diskOffset2=1.0
	DefaultAngleForS-TransistorINrcmos=0
	DefaultRigidForS-TransistorINrcmos=false
	DefaultFixedAngleForS-TransistorINrcmos=false
	DefaultExtendedForS-TransistorINrcmos=false
	DefaultDirectionalForS-TransistorINrcmos=false
		arcLayer layer=D-Active style=FILLED extend=1.0
		arcLayer layer=Polysilicon style=FILLED extend=1.0
		arcLayer layer=Select style=FILLED extend=3.0
ArcProto D-Transistor p-diffusion
	isWipable=false
	isCurvable=true
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForD-TransistorINrcmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=5.0
	diskOffset2=1.0
	DefaultAngleForD-TransistorINrcmos=0
	DefaultRigidForD-TransistorINrcmos=false
	DefaultFixedAngleForD-TransistorINrcmos=false
	DefaultExtendedForD-TransistorINrcmos=false
	DefaultDirectionalForD-TransistorINrcmos=false
		arcLayer layer=D-Active style=FILLED extend=1.0
		arcLayer layer=Polysilicon style=FILLED extend=1.0
		arcLayer layer=Well style=FILLED extend=5.0
PrimitiveNode Metal-1-Pin pin NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	baseRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	DefaultExtendXForMetal-1-PinINrcmos=0.0
	DefaultExtendYForMetal-1-PinINrcmos=0.0
	diskOffset1=1.5,1.5
	diskOffset2=1.5,1.5
	layers:
	layer=Metal-1 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port metal-1 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Metal-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-Bend90 unknown CURVEPIN
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	baseRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	minNodeSize w=10.0 h=10.0 rule=
	DefaultExtendXForMetal-1-Bend90INrcmos=0.0
	DefaultExtendYForMetal-1-Bend90INrcmos=0.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Metal-1 port=0 style=FILLED repr=0
		point xm=0.0 xa=6.5 ym=0.0 ya=-5.0
		point xm=0.0 xa=6.485 ym=0.0 ya=-4.435
		point xm=0.0 xa=6.445 ym=0.0 ya=-3.8725
		point xm=0.0 xa=6.375 ym=0.0 ya=-3.3125
		point xm=0.0 xa=6.28 ym=0.0 ya=-2.755
		point xm=0.0 xa=6.155 ym=0.0 ya=-2.205
		point xm=0.0 xa=6.005 ym=0.0 ya=-1.6625
		point xm=0.0 xa=5.8275 ym=0.0 ya=-1.125
		point xm=0.0 xa=5.625 ym=0.0 ya=-0.6
		point xm=0.0 xa=5.395 ym=0.0 ya=-0.0825
		point xm=0.0 xa=5.1425 ym=0.0 ya=0.42
		point xm=0.0 xa=4.865 ym=0.0 ya=0.9125
		point xm=0.0 xa=4.5625 ym=0.0 ya=1.39
		point xm=0.0 xa=4.2375 ym=0.0 ya=1.85
		point xm=0.0 xa=3.89 ym=0.0 ya=2.295
		point xm=0.0 xa=3.52 ym=0.0 ya=2.7225
		point xm=0.0 xa=3.1325 ym=0.0 ya=3.1325
		point xm=0.0 xa=2.7225 ym=0.0 ya=3.52
		point xm=0.0 xa=2.295 ym=0.0 ya=3.89
		point xm=0.0 xa=1.85 ym=0.0 ya=4.2375
		point xm=0.0 xa=1.39 ym=0.0 ya=4.5625
		point xm=0.0 xa=0.9125 ym=0.0 ya=4.865
		point xm=0.0 xa=0.42 ym=0.0 ya=5.1425
		point xm=0.0 xa=-0.0825 ym=0.0 ya=5.395
		point xm=0.0 xa=-0.6 ym=0.0 ya=5.625
		point xm=0.0 xa=-1.125 ym=0.0 ya=5.8275
		point xm=0.0 xa=-1.6625 ym=0.0 ya=6.005
		point xm=0.0 xa=-2.205 ym=0.0 ya=6.155
		point xm=0.0 xa=-2.755 ym=0.0 ya=6.28
		point xm=0.0 xa=-3.3125 ym=0.0 ya=6.375
		point xm=0.0 xa=-3.8725 ym=0.0 ya=6.445
		point xm=0.0 xa=-4.435 ym=0.0 ya=6.485
		point xm=0.0 xa=-5.0 ym=0.0 ya=6.5
		point xm=0.0 xa=-5.0 ym=0.0 ya=3.5
		point xm=0.0 xa=-4.5825 ym=0.0 ya=3.49
		point xm=0.0 xa=-4.1675 ym=0.0 ya=3.46
		point xm=0.0 xa=-3.7525 ym=0.0 ya=3.4075
		point xm=0.0 xa=-3.3425 ym=0.0 ya=3.3375
		point xm=0.0 xa=-2.935 ym=0.0 ya=3.245
		point xm=0.0 xa=-2.5325 ym=0.0 ya=3.135
		point xm=0.0 xa=-2.135 ym=0.0 ya=3.0025
		point xm=0.0 xa=-1.7475 ym=0.0 ya=2.8525
		point xm=0.0 xa=-1.365 ym=0.0 ya=2.685
		point xm=0.0 xa=-0.9925 ym=0.0 ya=2.495
		point xm=0.0 xa=-0.63 ym=0.0 ya=2.29
		point xm=0.0 xa=-0.2775 ym=0.0 ya=2.0675
		point xm=0.0 xa=0.0625 ym=0.0 ya=1.8275
		point xm=0.0 xa=0.3925 ym=0.0 ya=1.57
		point xm=0.0 xa=0.7075 ym=0.0 ya=1.2975
		point xm=0.0 xa=1.01 ym=0.0 ya=1.01
		point xm=0.0 xa=1.2975 ym=0.0 ya=0.7075
		point xm=0.0 xa=1.57 ym=0.0 ya=0.3925
		point xm=0.0 xa=1.8275 ym=0.0 ya=0.0625
		point xm=0.0 xa=2.0675 ym=0.0 ya=-0.2775
		point xm=0.0 xa=2.29 ym=0.0 ya=-0.63
		point xm=0.0 xa=2.495 ym=0.0 ya=-0.9925
		point xm=0.0 xa=2.685 ym=0.0 ya=-1.365
		point xm=0.0 xa=2.8525 ym=0.0 ya=-1.7475
		point xm=0.0 xa=3.0025 ym=0.0 ya=-2.135
		point xm=0.0 xa=3.135 ym=0.0 ya=-2.5325
		point xm=0.0 xa=3.245 ym=0.0 ya=-2.935
		point xm=0.0 xa=3.3375 ym=0.0 ya=-3.3425
		point xm=0.0 xa=3.4075 ym=0.0 ya=-3.7525
		point xm=0.0 xa=3.46 ym=0.0 ya=-4.1675
		point xm=0.0 xa=3.49 ym=0.0 ya=-4.5825
		point xm=0.0 xa=3.5 ym=0.0 ya=-5.0
	port c1 angle=270 range=90 topology=0 unknown
		lm=-0.5 la=10.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=-10.0
		isolated=false negatable=false
		portArc Metal-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port c2 angle=180 range=90 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=-10.0 bm=-0.5 ba=10.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Metal-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-Bend45 unknown CURVEPIN
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	baseRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	minNodeSize w=10.0 h=10.0 rule=
	DefaultExtendXForMetal-1-Bend45INrcmos=0.0
	DefaultExtendYForMetal-1-Bend45INrcmos=0.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Metal-1 port=0 style=FILLED repr=0
		point xm=0.0 xa=6.5 ym=0.0 ya=-5.0
		point xm=0.0 xa=6.485 ym=0.0 ya=-4.435
		point xm=0.0 xa=6.445 ym=0.0 ya=-3.8725
		point xm=0.0 xa=6.375 ym=0.0 ya=-3.3125
		point xm=0.0 xa=6.28 ym=0.0 ya=-2.755
		point xm=0.0 xa=6.155 ym=0.0 ya=-2.205
		point xm=0.0 xa=6.005 ym=0.0 ya=-1.6625
		point xm=0.0 xa=5.8275 ym=0.0 ya=-1.125
		point xm=0.0 xa=5.625 ym=0.0 ya=-0.6
		point xm=0.0 xa=5.395 ym=0.0 ya=-0.0825
		point xm=0.0 xa=5.1425 ym=0.0 ya=0.42
		point xm=0.0 xa=4.865 ym=0.0 ya=0.9125
		point xm=0.0 xa=4.5625 ym=0.0 ya=1.39
		point xm=0.0 xa=4.2375 ym=0.0 ya=1.85
		point xm=0.0 xa=3.89 ym=0.0 ya=2.295
		point xm=0.0 xa=3.52 ym=0.0 ya=2.7225
		point xm=0.0 xa=3.1325 ym=0.0 ya=3.1325
		point xm=0.0 xa=1.01 ym=0.0 ya=1.01
		point xm=0.0 xa=1.2975 ym=0.0 ya=0.7075
		point xm=0.0 xa=1.57 ym=0.0 ya=0.3925
		point xm=0.0 xa=1.8275 ym=0.0 ya=0.0625
		point xm=0.0 xa=2.0675 ym=0.0 ya=-0.2775
		point xm=0.0 xa=2.29 ym=0.0 ya=-0.63
		point xm=0.0 xa=2.495 ym=0.0 ya=-0.9925
		point xm=0.0 xa=2.685 ym=0.0 ya=-1.365
		point xm=0.0 xa=2.8525 ym=0.0 ya=-1.7475
		point xm=0.0 xa=3.0025 ym=0.0 ya=-2.135
		point xm=0.0 xa=3.135 ym=0.0 ya=-2.5325
		point xm=0.0 xa=3.245 ym=0.0 ya=-2.935
		point xm=0.0 xa=3.3375 ym=0.0 ya=-3.3425
		point xm=0.0 xa=3.4075 ym=0.0 ya=-3.7525
		point xm=0.0 xa=3.46 ym=0.0 ya=-4.1675
		point xm=0.0 xa=3.49 ym=0.0 ya=-4.5825
		point xm=0.0 xa=3.5 ym=0.0 ya=-5.0
	port c1 angle=270 range=90 topology=0 unknown
		lm=-0.5 la=10.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=-10.0
		isolated=false negatable=false
		portArc Metal-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port c2 angle=135 range=90 topology=0 unknown
		lm=-0.5 la=7.07 rm=0.5 ra=-2.93 bm=-0.5 ba=7.07 tm=0.5 ta=-2.93
		isolated=false negatable=false
		portArc Metal-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-2-Pin pin NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	baseRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	DefaultExtendXForMetal-2-PinINrcmos=0.0
	DefaultExtendYForMetal-2-PinINrcmos=0.0
	diskOffset1=1.5,1.5
	diskOffset2=1.5,1.5
	layers:
	layer=Metal-2 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port metal-2 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Metal-2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Polysilicon-Pin pin NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForPolysilicon-PinINrcmos=0.0
	DefaultExtendYForPolysilicon-PinINrcmos=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Polysilicon port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port polysilicon angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode S-Active-Pin pin NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForS-Active-PinINrcmos=0.0
	DefaultExtendYForS-Active-PinINrcmos=0.0
	diskOffset1=3.0,3.0
	diskOffset2=1.0,1.0
	layers:
	layer=S-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.0 ya=0.0
	layer=Select port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port s-active angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc S-Active
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode D-Active-Pin pin NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[4.0,4.0] Y:[4.0,4.0]}
	fullRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForD-Active-PinINrcmos=0.0
	DefaultExtendYForD-Active-PinINrcmos=0.0
	diskOffset1=5.0,5.0
	diskOffset2=1.0,1.0
	layers:
	layer=D-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-4.0 ym=0.0 ya=0.0
	layer=Well port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port d-active angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc D-Active
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Substrate-Active-Pin pin NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForSubstrate-Active-PinINrcmos=0.0
	DefaultExtendYForSubstrate-Active-PinINrcmos=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=D-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=S-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port active angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Substrate-Active
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Well-Active-Pin pin NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForWell-Active-PinINrcmos=0.0
	DefaultExtendYForWell-Active-PinINrcmos=0.0
	diskOffset1=3.0,3.0
	diskOffset2=1.0,1.0
	layers:
	layer=D-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.0 ya=0.0
	layer=S-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.0 ya=0.0
	layer=Well port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Select port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-1.0 ym=0.0 ya=0.0
	port active angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Well-Active
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode S-Transistor pin
	specialType=0 numMultiCuts=0
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForS-TransistorINrcmos=0.0
	DefaultExtendYForS-TransistorINrcmos=0.0
	diskOffset1=3.0,3.0
	diskOffset2=1.0,1.0
	layers:
	layer=S-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.0 ya=0.0
	layer=Polysilicon port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.0 ya=0.0
	layer=Select port=-1 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port s-trans angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc S-Transistor
		portArc S-Active
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode D-Transistor pin
	specialType=0 numMultiCuts=0
	SizeOffset {X:[4.0,4.0] Y:[4.0,4.0]}
	fullRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForD-TransistorINrcmos=0.0
	DefaultExtendYForD-TransistorINrcmos=0.0
	diskOffset1=5.0,5.0
	diskOffset2=1.0,1.0
	layers:
	layer=D-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-4.0 ym=0.0 ya=0.0
	layer=Polysilicon port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-4.0 ym=0.0 ya=0.0
	layer=Well port=-1 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port d-trans angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc D-Transistor
		portArc D-Active
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-S-Active-Con contact NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForMetal-1-S-Active-ConINrcmos=0.0
	DefaultExtendYForMetal-1-S-Active-ConINrcmos=0.0
	diskOffset1=5.0,5.0
	diskOffset2=3.0,3.0
	layers:
	layer=Metal-1 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-3.0 ym=0.0 ya=0.0
	layer=S-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.0 ya=0.0
	layer=Select port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Active-Cut port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=1.0 ym=0.0 ya=0.0
	port metal-1-s-act angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc S-Active
		portArc Metal-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-D-Active-Con contact NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[4.0,4.0] Y:[4.0,4.0]}
	fullRectangle=ERectangle[x=-7.0,y=-7.0,w=14.0,h=14.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForMetal-1-D-Active-ConINrcmos=0.0
	DefaultExtendYForMetal-1-D-Active-ConINrcmos=0.0
	diskOffset1=7.0,7.0
	diskOffset2=3.0,3.0
	layers:
	layer=Metal-1 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-5.0 ym=0.0 ya=0.0
	layer=D-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-4.0 ym=0.0 ya=0.0
	layer=Well port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Active-Cut port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=1.0 ym=0.0 ya=0.0
	port metal-1-d-act angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc D-Active
		portArc Metal-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-Polysilicon-Con contact NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForMetal-1-Polysilicon-ConINrcmos=0.0
	DefaultExtendYForMetal-1-Polysilicon-ConINrcmos=0.0
	diskOffset1=3.0,3.0
	diskOffset2=3.0,3.0
	layers:
	layer=Metal-1 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-1.0 ym=0.0 ya=0.0
	layer=Polysilicon port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Poly-Cut port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=1.0 ym=0.0 ya=0.0
	port metal-1-polysilicon angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Metal-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-Metal-2-Con contact NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForMetal-1-Metal-2-ConINrcmos=0.0
	DefaultExtendYForMetal-1-Metal-2-ConINrcmos=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Metal-1 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Metal-2 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Via port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=1.0 ym=0.0 ya=0.0
	port metal-1-metal-2 angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Metal-1
		portArc Metal-2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-Well-Con well NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForMetal-1-Well-ConINrcmos=0.0
	DefaultExtendYForMetal-1-Well-ConINrcmos=0.0
	diskOffset1=5.0,5.0
	diskOffset2=3.0,3.0
	layers:
	layer=Metal-1 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-5.0 ym=0.0 ya=0.0
	layer=S-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.0 ya=0.0
	layer=Well port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Select port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.0 ya=0.0
	layer=Active-Cut port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=1.0 ym=0.0 ya=0.0
	port metal-1-well angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Metal-1
		portArc Well-Active
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-Substrate-Con well NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForMetal-1-Substrate-ConINrcmos=0.0
	DefaultExtendYForMetal-1-Substrate-ConINrcmos=0.0
	diskOffset1=3.0,3.0
	diskOffset2=3.0,3.0
	layers:
	layer=Metal-1 port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-1.0 ym=0.0 ya=0.0
	layer=S-Active port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Active-Cut port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=1.0 ym=0.0 ya=0.0
	port metal-1-substrate angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Metal-1
		portArc Substrate-Active
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForMetal-1-NodeINrcmos=2.0
	DefaultExtendYForMetal-1-NodeINrcmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Metal-1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal-1 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Metal-1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-2-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForMetal-2-NodeINrcmos=2.0
	DefaultExtendYForMetal-2-NodeINrcmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Metal-2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal-2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Metal-2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Polysilicon-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPolysilicon-NodeINrcmos=2.0
	DefaultExtendYForPolysilicon-NodeINrcmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port polysilicon angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Active-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForActive-NodeINrcmos=2.0
	DefaultExtendYForActive-NodeINrcmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=S-Active port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port active angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc S-Active
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode D-Active-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForD-Active-NodeINrcmos=2.0
	DefaultExtendYForD-Active-NodeINrcmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=D-Active port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port active angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc D-Active
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Select-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForSelect-NodeINrcmos=2.0
	DefaultExtendYForSelect-NodeINrcmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Select port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port select angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Well-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForWell-NodeINrcmos=3.0
	DefaultExtendYForWell-NodeINrcmos=3.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Well port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port well angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Cut-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForCut-NodeINrcmos=1.0
	DefaultExtendYForCut-NodeINrcmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Contact-Cut port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port cut angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Via-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForVia-NodeINrcmos=1.0
	DefaultExtendYForVia-NodeINrcmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Via port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port via angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Passivation-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPassivation-NodeINrcmos=4.0
	DefaultExtendYForPassivation-NodeINrcmos=4.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Passivation port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port passivation angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Poly-Cut-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPoly-Cut-NodeINrcmos=1.0
	DefaultExtendYForPoly-Cut-NodeINrcmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Poly-Cut port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port polycut angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Active-Cut-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForActive-Cut-NodeINrcmos=1.0
	DefaultExtendYForActive-Cut-NodeINrcmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Active-Cut port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port activecut angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
Foundry NONE
	rcmos.GDS.Metal-1=()
	rcmos.GDS.Metal-2=()
	rcmos.GDS.Polysilicon=()
	rcmos.GDS.S-Active=()
	rcmos.GDS.D-Active=()
	rcmos.GDS.Select=()
	rcmos.GDS.Well=()
	rcmos.GDS.Contact-Cut=()
	rcmos.GDS.Via=()
	rcmos.GDS.Passivation=()
	rcmos.GDS.Poly-Cut=()
	rcmos.GDS.Active-Cut=()
 menu 0 0 arc S-Transistor
 menu 0 1 nodeInst S-Transistor:pin:
 menu 0 2 Pure
 menu 1 0 arc D-Transistor
 menu 1 1 nodeInst D-Transistor:pin:
 menu 1 2 Misc.
 menu 2 0 arc Well-Active
 menu 2 1 nodeInst Well-Active-Pin:pin:
 menu 2 2 node Metal-1-Well-Con
 menu 3 0 arc S-Active
 menu 3 1 nodeInst S-Active-Pin:pin:
 menu 3 2 node Metal-1-S-Active-Con
 menu 4 0 arc D-Active
 menu 4 1 nodeInst D-Active-Pin:pin:
 menu 4 2 node Metal-1-D-Active-Con
 menu 5 0 arc Substrate-Active
 menu 5 1 nodeInst Substrate-Active-Pin:pin:
 menu 5 2 node Metal-1-Substrate-Con
 menu 6 0 arc Polysilicon
 menu 6 1 nodeInst Polysilicon-Pin:pin:
 menu 6 2 node Metal-1-Polysilicon-Con
 menu 7 0 arc Metal-1
 menu 7 1 nodeInst Metal-1-Pin:pin: nodeInst Metal-1-Bend90:pin: nodeInst Metal-1-Bend45:pin:
 menu 7 2 node Metal-1-Metal-2-Con
 menu 8 0 arc Metal-2
 menu 8 1 nodeInst Metal-2-Pin:pin:
 menu 8 2 Cell
    <Foundry name="NONE">
    </Foundry>
