Technology efido
class com.sun.electric.technology.Technology
shortName=null
techDesc=Digital Filters
Bits:  NONEGATEDARCS
isScaleRelevant=falseefido.Scale=10000.0(10000.0)
efido.Foundry=NONE(NONE)
efido.NumMetalLayers=0(0)
efido.MininumResistance=10.0(10.0)
efido.GateLengthSubtraction=0.0(0.0)
efido.Gate Inclusion=false(false)
efido.Ground Net Inclusion=false(false)
efido.MaxSeriesResistance=10.0(10.0)
efido.LogicalEffort.GateCapacitance=0.4(0.4)
efido.LogicalEffort.WireRatio=0.16(0.16)
efido.LogicalEffort.DiffAlpha=0.7(0.7)
ResolutionValueForefido=0.0
TRANSPARENT_1=ffff0000
TRANSPARENT_2=ff0000ff
TRANSPARENT_3=ff009b50
TRANSPARENT_4=ff000000
TRANSPARENT_5=ff000000
Layer Node ART NONELEC
	efido.CIF.Node=()
	efido.DXF.Node=()
	efido.Skill.Node=()
	efido.Resistance.Node=0.0(0.0)
	efido.Capacitance.Node=0.0(0.0)
	efido.EdgeCapacitance.Node=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=1(1)
	color=ffff0000(ff0000)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Arc UNKNOWN
	efido.CIF.Arc=()
	efido.DXF.Arc=()
	efido.Skill.Arc=()
	efido.Resistance.Arc=0.0(0.0)
	efido.Capacitance.Arc=0.0(0.0)
	efido.EdgeCapacitance.Arc=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=2(2)
	color=ff0000ff(ff)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Outpad OVERGLASS
	efido.CIF.Outpad=()
	efido.DXF.Outpad=()
	efido.Skill.Outpad=()
	efido.Resistance.Outpad=0.0(0.0)
	efido.Capacitance.Outpad=0.0(0.0)
	efido.EdgeCapacitance.Outpad=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=3(3)
	color=ff009b50(9b50)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
ArcProto wire metal-1
	isWipable=false
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForwireINefido=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForwireINefido=45
	DefaultRigidForwireINefido=false
	DefaultFixedAngleForwireINefido=true
	DefaultExtendedForwireINefido=true
	DefaultDirectionalForwireINefido=false
		arcLayer layer=Arc style=CLOSED extend=0.0
ArcProto bus bus
	isWipable=false
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForbusINefido=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=1.0
	diskOffset2=1.0
	DefaultAngleForbusINefido=45
	DefaultRigidForbusINefido=false
	DefaultFixedAngleForbusINefido=true
	DefaultExtendedForbusINefido=true
	DefaultDirectionalForbusINefido=false
		arcLayer layer=Arc style=CLOSED extend=1.0
PrimitiveNode wire_pin pin NSQUARE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-0.5,y=-0.5,w=1.0,h=1.0]
	baseRectangle=ERectangle[x=-0.5,y=-0.5,w=1.0,h=1.0]
	DefaultExtendXForwire_pinINefido=0.0
	DefaultExtendYForwire_pinINefido=0.0
	diskOffset1=0.5,0.5
	diskOffset2=0.5,0.5
	layers:
	layer=Arc port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port wire angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode bus_pin pin
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForbus_pinINefido=0.0
	DefaultExtendYForbus_pinINefido=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Node port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port bus angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode adder unknown NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForadderINefido=0.0
	DefaultExtendYForadderINefido=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Node port=-1 style=OPENED repr=0
		point xm=0.25 xa=0.0 ym=0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=5 style=OPENED repr=0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=-1 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=5 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.1 ya=0.0
	port in1 angle=270 range=15 topology=4 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in2 angle=225 range=15 topology=0 unknown
		lm=-0.3535534 la=0.0 rm=-0.3535534 ra=0.0 bm=0.3535534 ba=0.0 tm=0.3535534 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in3 angle=180 range=15 topology=1 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in4 angle=135 range=15 topology=2 unknown
		lm=-0.3535534 la=0.0 rm=-0.3535534 ra=0.0 bm=-0.3535534 ba=0.0 tm=-0.3535534 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in5 angle=90 range=15 topology=3 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port out angle=0 range=45 topology=5 unknown
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode multiplier unknown NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXFormultiplierINefido=0.0
	DefaultExtendYFormultiplierINefido=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Node port=-1 style=OPENED repr=0
		point xm=0.25 xa=0.0 ym=0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=-1 style=OPENED repr=0
		point xm=-0.25 xa=0.0 ym=0.25 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=-1 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=5 style=OPENED repr=0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=5 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.1 ya=0.0
	port in1 angle=270 range=15 topology=4 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in2 angle=225 range=15 topology=0 unknown
		lm=-0.3535534 la=0.0 rm=-0.3535534 ra=0.0 bm=0.3535534 ba=0.0 tm=0.3535534 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in3 angle=180 range=15 topology=1 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in4 angle=135 range=15 topology=2 unknown
		lm=-0.3535534 la=0.0 rm=-0.3535534 ra=0.0 bm=-0.3535534 ba=0.0 tm=-0.3535534 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in5 angle=90 range=15 topology=3 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port out angle=0 range=45 topology=5 unknown
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode timedelay unknown
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXFortimedelayINefido=0.0
	DefaultExtendYFortimedelayINefido=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Node port=-1 style=OPENED repr=0
		point xm=-0.25 xa=0.0 ym=0.25 ya=0.0
		point xm=0.25 xa=0.0 ym=0.25 ya=0.0
	layer=Node port=-1 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=1 style=OPENED repr=0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=-1 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=1 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.1 ya=0.0
	port in angle=180 range=15 topology=0 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port out angle=0 range=45 topology=1 unknown
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode multiplexer unknown
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXFormultiplexerINefido=0.0
	DefaultExtendYFormultiplexerINefido=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Node port=-1 style=OPENED repr=0
		point xm=-0.2 xa=0.0 ym=-0.05 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.1 xa=0.0 ym=-0.3 ya=0.0
	layer=Node port=1 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.25 ya=0.0
	layer=Node port=-1 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.25 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=-1 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port in1 angle=270 range=15 topology=1 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.25 ba=0.0 tm=0.25 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in2 angle=135 range=15 topology=0 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=-0.25 ba=0.0 tm=-0.25 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port out angle=0 range=45 topology=2 unknown
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode subtractor unknown NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForsubtractorINefido=0.0
	DefaultExtendYForsubtractorINefido=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Node port=-1 style=OPENED repr=0
		point xm=-0.25 xa=0.0 ym=0.0 ya=0.0
		point xm=0.25 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=5 style=OPENED repr=0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=5 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=-1 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port in1 angle=270 range=15 topology=4 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in2 angle=225 range=15 topology=0 unknown
		lm=-0.3535534 la=0.0 rm=-0.3535534 ra=0.0 bm=0.3535534 ba=0.0 tm=0.3535534 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in3 angle=180 range=15 topology=1 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in4 angle=135 range=15 topology=2 unknown
		lm=-0.3535534 la=0.0 rm=-0.3535534 ra=0.0 bm=-0.3535534 ba=0.0 tm=-0.3535534 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in5 angle=90 range=15 topology=3 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port out angle=0 range=45 topology=5 unknown
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode divider unknown NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXFordividerINefido=0.0
	DefaultExtendYFordividerINefido=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Node port=-1 style=OPENED repr=0
		point xm=-0.05 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=-1 style=OPENED repr=0
		point xm=-0.25 xa=0.0 ym=0.0 ya=0.0
		point xm=0.25 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=-1 style=OPENED repr=0
		point xm=-0.05 xa=0.0 ym=0.25 ya=0.0
		point xm=0.05 xa=0.0 ym=0.25 ya=0.0
	layer=Node port=4 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=4 style=OPENED repr=0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=-1 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port in1 angle=270 range=15 topology=4 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in2 angle=225 range=15 topology=0 unknown
		lm=-0.3535534 la=0.0 rm=-0.3535534 ra=0.0 bm=0.3535534 ba=0.0 tm=0.3535534 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in3 angle=180 range=15 topology=1 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in4 angle=135 range=15 topology=2 unknown
		lm=-0.3535534 la=0.0 rm=-0.3535534 ra=0.0 bm=-0.3535534 ba=0.0 tm=-0.3535534 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port in5 angle=90 range=15 topology=3 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port out angle=0 range=45 topology=5 unknown
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode padin connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForpadinINefido=0.0
	DefaultExtendYForpadinINefido=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Node port=0 style=CROSSED repr=1
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.25 xa=0.0 ym=0.25 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port out angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode padout connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForpadoutINefido=0.0
	DefaultExtendYForpadoutINefido=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Outpad port=0 style=CROSSED repr=1
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.25 xa=0.0 ym=0.25 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port in angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
Foundry NONE
	efido.GDS.Node=()
	efido.GDS.Arc=()
	efido.GDS.Outpad=()
 menu 0 0 arc wire
 menu 0 1 node multiplier
 menu 1 0 arc bus
 menu 1 1 node timedelay
 menu 2 0 Cell
 menu 2 1 node multiplexer
 menu 3 0 Misc.
 menu 3 1 node subtractor
 menu 4 0 Pure
 menu 4 1 node divider
 menu 5 0 nodeInst wire_pin:pin:
 menu 5 1 node padin
 menu 6 0 nodeInst bus_pin:pin:
 menu 6 1 node padout
 menu 7 0 node adder
    <Foundry name="NONE">
    </Foundry>
