Technology schematic
class com.sun.electric.technology.technologies.Schematics
shortName=Schematics
techDesc=Schematic Capture
Bits:  NONSTANDARD STATICTECHNOLOGY
isScaleRelevant=falseschematic.Scale=2000.0(2000.0)
schematic.Foundry=NONE(NONE)
schematic.NumMetalLayers=1(1)
schematic.MininumResistance=10.0(10.0)
schematic.GateLengthSubtraction=0.0(0.0)
schematic.Gate Inclusion=false(false)
schematic.Ground Net Inclusion=false(false)
schematic.MaxSeriesResistance=10.0(10.0)
schematic.LogicalEffort.GateCapacitance=0.4(0.4)
schematic.LogicalEffort.WireRatio=0.16(0.16)
schematic.LogicalEffort.DiffAlpha=0.7(0.7)
ResolutionValueForschematic=0.0
Layer Arc METAL1
	schematic.CIF.Arc=()
	schematic.DXF.Arc=()
	schematic.Skill.Arc=()
	schematic.Resistance.Arc=0.0(0.0)
	schematic.Capacitance.Arc=0.0(0.0)
	schematic.EdgeCapacitance.Arc=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff0000ff(ff)
	opacity=0.8(0.8)
	foreground=true
	pattern ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Bus BUS
	schematic.CIF.Bus=()
	schematic.DXF.Bus=()
	schematic.Skill.Bus=()
	schematic.Resistance.Bus=0.0(0.0)
	schematic.Capacitance.Bus=0.0(0.0)
	schematic.EdgeCapacitance.Bus=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=0(0)
	color=ff00ff00(ff00)
	opacity=0.8(0.8)
	foreground=true
	pattern aaaa 5555 aaaa 5555 aaaa 5555 aaaa 5555 aaaa 5555 aaaa 5555 aaaa 5555 aaaa 5555
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Node ART
	schematic.CIF.Node=()
	schematic.DXF.Node=()
	schematic.Skill.Node=()
	schematic.Resistance.Node=0.0(0.0)
	schematic.Capacitance.Node=0.0(0.0)
	schematic.EdgeCapacitance.Node=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffff0000(ff0000)
	opacity=0.8(0.8)
	foreground=true
	pattern ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Text ART
	schematic.CIF.Text=()
	schematic.DXF.Text=()
	schematic.Skill.Text=()
	schematic.Resistance.Text=0.0(0.0)
	schematic.Capacitance.Text=0.0(0.0)
	schematic.EdgeCapacitance.Text=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff ffff
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
ArcProto wire metal-1
	isWipable=false
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForwireINschematic=0.0
	baseExtend=0.0
	defaultLambdaBaseWidth=0.0
	diskOffset1=0.0
	diskOffset2=0.0
	DefaultAngleForwireINschematic=45
	DefaultRigidForwireINschematic=false
	DefaultFixedAngleForwireINschematic=true
	DefaultExtendedForwireINschematic=true
	DefaultDirectionalForwireINschematic=false
		arcLayer layer=Arc style=FILLED extend=0.0
ArcProto bus bus
	isWipable=false
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForbusINschematic=0.0
	baseExtend=0.5
	defaultLambdaBaseWidth=1.0
	diskOffset1=0.5
	diskOffset2=0.5
	DefaultAngleForbusINschematic=45
	DefaultRigidForbusINschematic=false
	DefaultFixedAngleForbusINschematic=true
	DefaultExtendedForbusINschematic=false
	DefaultDirectionalForbusINschematic=false
		arcLayer layer=Bus style=FILLED extend=0.5
PrimitiveNode Wire_Pin pin NSQUARE CANBEZEROSIZE WIPEON1OR2
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-0.25,y=-0.25,w=0.5,h=0.5]
	baseRectangle=ERectangle[x=-0.25,y=-0.25,w=0.5,h=0.5]
	DefaultExtendXForWire_PinINschematic=0.0
	DefaultExtendYForWire_PinINschematic=0.0
	diskOffset1=0.25,0.25
	diskOffset2=0.25,0.25
	layers:
	layer=Arc port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port wire angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Bus_Pin pin NSQUARE CANBEZEROSIZE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForBus_PinINschematic=0.0
	DefaultExtendYForBus_PinINschematic=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Bus port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Arc port=0 style=DISC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	port bus angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Wire_Con connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForWire_ConINschematic=0.0
	DefaultExtendYForWire_ConINschematic=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Text port=0 style=TEXTCENT repr=0
		message="J" td=20000000000 colorIndex=0 disp=true
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
	port wire angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.5 rm=0.5 ra=-0.5 bm=-0.5 ba=0.5 tm=0.5 ta=-0.5
		isolated=true negatable=false
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Buffer buffer
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,1.0] Y:[0.25,0.25]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-3.0,y=-2.75,w=5.0,h=5.5]
	DefaultExtendXForBufferINschematic=0.0
	DefaultExtendYForBufferINschematic=0.0
	diskOffset1=3.0,3.0
	diskOffset2=2.5,2.75
	layers:
	layer=Node port=0 style=CLOSED repr=0
		point xm=0.5 xa=-1.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.5 ya=-0.25
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.25
	port a angle=180 range=45 topology=0 input
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port c angle=270 range=45 topology=1 input
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=2.0 tm=-0.5 ta=2.0
		isolated=false negatable=true
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port y angle=0 range=45 topology=2 output
		lm=0.5 la=-1.0 rm=0.5 ra=-1.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode And AND-gate
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.5] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-4.0,y=-3.0,w=8.0,h=6.0]
	baseRectangle=ERectangle[x=-4.0,y=-3.0,w=7.5,h=6.0]
	autoGrowth (0.0,4.0)
	DefaultExtendXForAndINschematic=0.0
	DefaultExtendYForAndINschematic=0.0
	diskOffset1=4.0,3.0
	diskOffset2=3.75,3.0
	layers:
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=0.0 xa=0.5 ym=0.0 ya=0.0
		point xm=0.0 xa=0.5 ym=0.0 ya=3.0
		point xm=0.0 xa=0.5 ym=0.0 ya=-3.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.5 ym=0.0 ya=3.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=3.0
		point xm=0.0 xa=-4.0 ym=0.5 ya=0.0
		point xm=0.0 xa=-4.0 ym=-0.5 ya=0.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=-3.0
		point xm=0.0 xa=0.5 ym=0.0 ya=-3.0
	port a angle=180 range=45 topology=0 input
		lm=0.0 la=-4.0 rm=0.0 ra=-4.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=true negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port y angle=0 range=45 topology=1 output
		lm=0.0 la=3.5 rm=0.0 ra=3.5 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port yt angle=0 range=45 topology=2 output
		lm=0.0 la=2.75 rm=0.0 ra=2.75 bm=0.0 ba=2.0 tm=0.0 ta=2.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port yc angle=0 range=45 topology=3 output
		lm=0.0 la=2.75 rm=0.0 ra=2.75 bm=0.0 ba=-2.0 tm=0.0 ta=-2.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Or OR-gate
	specialType=0 numMultiCuts=0
	SizeOffset {X:[1.0,0.5] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-5.0,y=-3.0,w=10.0,h=6.0]
	baseRectangle=ERectangle[x=-4.0,y=-3.0,w=8.5,h=6.0]
	autoGrowth (0.0,4.0)
	DefaultExtendXForOrINschematic=0.0
	DefaultExtendYForOrINschematic=0.0
	diskOffset1=5.0,3.0
	diskOffset2=4.25,3.0
	layers:
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=0.0 xa=-9.0 ym=0.0 ya=0.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=3.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=-3.0
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=0.0 xa=-0.75 ym=0.0 ya=-3.0
		point xm=0.0 xa=-0.75 ym=0.0 ya=3.0
		point xm=0.0 xa=4.5 ym=0.0 ya=0.0
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=0.0 xa=-0.75 ym=0.0 ya=3.0
		point xm=0.0 xa=4.5 ym=0.0 ya=0.0
		point xm=0.0 xa=-0.75 ym=0.0 ya=-3.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.0 xa=-4.0 ym=0.5 ya=0.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=3.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=3.0
		point xm=0.0 xa=-0.75 ym=0.0 ya=3.0
		point xm=0.0 xa=-4.0 ym=-0.5 ya=0.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=-3.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=-3.0
		point xm=0.0 xa=-0.75 ym=0.0 ya=-3.0
	port a angle=180 range=45 topology=0 input
		lm=0.0 la=-4.0 rm=0.0 ra=-3.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=true negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port y angle=0 range=45 topology=1 output
		lm=0.0 la=4.5 rm=0.0 ra=4.5 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port yt angle=0 range=45 topology=2 output
		lm=0.0 la=2.65 rm=0.0 ra=2.65 bm=0.0 ba=2.0 tm=0.0 ta=2.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port yc angle=0 range=45 topology=3 output
		lm=0.0 la=2.65 rm=0.0 ra=2.65 bm=0.0 ba=-2.0 tm=0.0 ta=-2.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Xor XOR-gate
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.5] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-5.0,y=-3.0,w=10.0,h=6.0]
	baseRectangle=ERectangle[x=-5.0,y=-3.0,w=9.5,h=6.0]
	autoGrowth (0.0,4.0)
	DefaultExtendXForXorINschematic=0.0
	DefaultExtendYForXorINschematic=0.0
	diskOffset1=5.0,3.0
	diskOffset2=4.75,3.0
	layers:
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=0.0 xa=-9.0 ym=0.0 ya=0.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=3.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=-3.0
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=0.0 xa=-0.75 ym=0.0 ya=-3.0
		point xm=0.0 xa=-0.75 ym=0.0 ya=3.0
		point xm=0.0 xa=4.5 ym=0.0 ya=0.0
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=0.0 xa=-0.75 ym=0.0 ya=3.0
		point xm=0.0 xa=4.5 ym=0.0 ya=0.0
		point xm=0.0 xa=-0.75 ym=0.0 ya=-3.0
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=0.0 xa=-10.0 ym=0.0 ya=0.0
		point xm=0.0 xa=-5.0 ym=0.0 ya=3.0
		point xm=0.0 xa=-5.0 ym=0.0 ya=-3.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.0 xa=-4.0 ym=0.5 ya=0.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=3.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=3.0
		point xm=0.0 xa=-0.75 ym=0.0 ya=3.0
		point xm=0.0 xa=-4.0 ym=-0.5 ya=0.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=-3.0
		point xm=0.0 xa=-4.0 ym=0.0 ya=-3.0
		point xm=0.0 xa=-0.75 ym=0.0 ya=-3.0
	port a angle=180 range=45 topology=0 input
		lm=0.0 la=-4.0 rm=0.0 ra=-3.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=true negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port y angle=0 range=45 topology=1 output
		lm=0.0 la=4.5 rm=0.0 ra=4.5 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port yt angle=0 range=45 topology=2 output
		lm=0.0 la=2.65 rm=0.0 ra=2.65 bm=0.0 ba=2.0 tm=0.0 ta=2.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port yc angle=0 range=45 topology=3 output
		lm=0.0 la=2.65 rm=0.0 ra=2.65 bm=0.0 ba=-2.0 tm=0.0 ta=-2.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
MultiFunction PrimitiveNode Flip-Flop flip-flop-RS-MS
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-5.0,w=6.0,h=10.0]
	baseRectangle=ERectangle[x=-3.0,y=-5.0,w=6.0,h=10.0]
	DefaultExtendXForFlip-FlopINschematic=0.0
	DefaultExtendYForFlip-FlopINschematic=0.0
	diskOffset1=3.0,5.0
	diskOffset2=3.0,5.0
	layers:
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="R" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="S" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	port i1 angle=180 range=45 topology=0 input
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.3 ba=0.0 tm=0.3 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port i2 angle=180 range=45 topology=1 input
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=-0.3 ba=0.0 tm=-0.3 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port q angle=0 range=45 topology=2 output
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=0.3 ba=0.0 tm=0.3 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port qb angle=0 range=45 topology=3 output
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.3 ba=0.0 tm=-0.3 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port ck angle=180 range=45 topology=4 input
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port preset angle=90 range=45 topology=5 input
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port clear angle=270 range=45 topology=6 input
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	techBits=0 flip-flop-RS-MS
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="R" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="S" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=1 flip-flop-JK-MS
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="J" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="K" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=2 flip-flop-D-MS
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="D" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="E" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=3 flip-flop-T-MS
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="T" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=4 flip-flop-RS-P
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="R" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="S" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=5 flip-flop-JK-P
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="J" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="K" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=6 flip-flop-D-P
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="D" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="E" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=7 flip-flop-T-P
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="T" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=8 flip-flop-RS-N
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="R" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="S" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=9 flip-flop-JK-N
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="J" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="K" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=10 flip-flop-D-N
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="D" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="E" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
	techBits=11 flip-flop-T-N
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.1 xa=0.0 ym=-0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="T" td=10000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=-0.35 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="Q" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="QB" td=10000000000 colorIndex=0 disp=true
		point xm=0.5 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="PR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="CLR" td=10000000000 colorIndex=0 disp=true
		point xm=-0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
PrimitiveNode Mux multiplexor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.5,0.5] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-4.0,y=-5.0,w=8.0,h=10.0]
	baseRectangle=ERectangle[x=-3.5,y=-5.0,w=7.0,h=10.0]
	autoGrowth (0.0,4.0)
	DefaultExtendXForMuxINschematic=0.0
	DefaultExtendYForMuxINschematic=0.0
	diskOffset1=4.0,5.0
	diskOffset2=3.5,5.0
	layers:
	layer=Node port=0 style=CLOSED repr=0
		point xm=0.4 xa=0.0 ym=0.375 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.4 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.4 xa=0.0 ym=0.5 ya=0.0
	port a angle=180 range=45 topology=0 input
		lm=-0.4 la=0.0 rm=-0.4 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=true negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port s angle=270 range=45 topology=2 input
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.4375 ba=0.0 tm=-0.4375 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port y angle=0 range=45 topology=1 output
		lm=0.4 la=0.0 rm=0.4 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Bbox unknown
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	baseRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	DefaultExtendXForBboxINschematic=0.0
	DefaultExtendYForBboxINschematic=0.0
	diskOffset1=5.0,5.0
	diskOffset2=5.0,5.0
	layers:
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port a angle=0 range=45 topology=0 unknown
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=true negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port b angle=90 range=45 topology=1 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=true negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port c angle=180 range=45 topology=2 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=true negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port d angle=270 range=45 topology=3 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=true negatable=true
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Switch unknown
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.5,0.5] Y:[0.5,0.5]}
	fullRectangle=ERectangle[x=-3.0,y=-1.0,w=6.0,h=2.0]
	baseRectangle=ERectangle[x=-2.5,y=-0.5,w=5.0,h=1.0]
	autoGrowth (0.0,4.0)
	DefaultExtendXForSwitchINschematic=0.0
	DefaultExtendYForSwitchINschematic=0.0
	diskOffset1=3.0,1.0
	diskOffset2=2.5,0.5
	layers:
	layer=Node port=0 style=DISC repr=0
		point xm=0.5 xa=-1.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-1.25 ym=0.0 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=-1.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=1.0 ym=0.0 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=-1.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=1.0 ym=0.0 ya=1.0
	port a angle=180 range=90 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=true negatable=false
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port y angle=0 range=90 topology=1 unknown
		lm=0.5 la=-1.0 rm=0.5 ra=-1.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Off-Page connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-1.0,w=4.0,h=2.0]
	baseRectangle=ERectangle[x=-2.0,y=-1.0,w=4.0,h=2.0]
	DefaultExtendXForOff-PageINschematic=0.0
	DefaultExtendYForOff-PageINschematic=0.0
	diskOffset1=2.0,1.0
	diskOffset2=2.0,1.0
	layers:
	layer=Node port=0 style=CLOSED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
	port a angle=180 range=45 topology=0 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port y angle=0 range=45 topology=0 unknown
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Power power NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	baseRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	DefaultExtendXForPowerINschematic=0.0
	DefaultExtendYForPowerINschematic=0.0
	diskOffset1=1.5,1.5
	diskOffset2=1.5,1.5
	layers:
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.375 ya=0.0
	port vdd angle=0 range=180 topology=0 power
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Ground ground
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.5,y=-2.0,w=3.0,h=4.0]
	baseRectangle=ERectangle[x=-1.5,y=-2.0,w=3.0,h=4.0]
	DefaultExtendXForGroundINschematic=0.0
	DefaultExtendYForGroundINschematic=0.0
	diskOffset1=1.5,2.0
	diskOffset2=1.5,2.0
	layers:
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.375 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.375 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	port gnd angle=90 range=90 topology=0 ground
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Source source NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForSourceINschematic=0.0
	DefaultExtendYForSourceINschematic=0.0
	diskOffset1=3.0,3.0
	diskOffset2=3.0,3.0
	layers:
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.15 xa=0.0 ym=0.3 ya=0.0
		point xm=0.15 xa=0.0 ym=0.3 ya=0.0
		point xm=0.0 xa=0.0 ym=0.15 ya=0.0
		point xm=0.0 xa=0.0 ym=0.45 ya=0.0
	port plus angle=90 range=45 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port minus angle=270 range=45 topology=1 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
MultiFunction PrimitiveNode Transistor transistor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,1.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=3.0]
	DefaultExtendXForTransistorINschematic=0.0
	DefaultExtendYForTransistorINschematic=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,1.5
	layers:
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	port g angle=0 range=180 topology=0 input
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=-1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port s angle=180 range=90 topology=1 bidirectional
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port d angle=0 range=90 topology=2 bidirectional
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	techBits=0 nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=1 depletion-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=FILLED repr=1
		point xm=-0.375 xa=0.0 ym=-0.375 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=2 pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=3 NPN-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.4375 ya=0.0
	techBits=4 PNP-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.25 xa=0.0 ym=-0.1875 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.25 ya=0.0
	techBits=5 n-type-JFET-transistor
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.0625 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0625 xa=0.0 ym=0.0 ya=0.0
	techBits=6 p-type-JFET-transistor
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.0625 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0625 xa=0.0 ym=0.0 ya=0.0
	techBits=7 depletion-mesfet
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=8 enhancement-mesfet
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=9 depletion-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=FILLED repr=1
		point xm=-0.375 xa=0.0 ym=-0.375 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=10 native-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=11 native-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=12 floating-gate-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.1875 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.1875 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=13 floating-gate-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.1875 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.1875 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=14 low-threshold-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.195 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.195 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.195 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=15 low-threshold-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.195 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.195 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=-0.07 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.195 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.05499999999999999 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=16 high-threshold-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.05499999999999999 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.05499999999999999 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.05499999999999999 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=17 high-threshold-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.05499999999999999 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.05499999999999999 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.07 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.05499999999999999 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.195 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=18 high-voltage-1-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.125 ya=0.0
		point xm=0.4 xa=0.0 ym=0.125 ya=0.0
	techBits=19 high-voltage-1-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.125 ya=0.0
		point xm=0.4 xa=0.0 ym=0.125 ya=0.0
	techBits=20 high-voltage-2-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.125 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.125 ya=0.0
	techBits=21 high-voltage-2-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.125 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.125 ya=0.0
	techBits=22 high-voltage-3-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.25000000000000006 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.20000000000000007 xa=0.0 ym=0.075 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.15000000000000008 xa=0.0 ym=0.125 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.125 ya=0.0
	techBits=23 high-voltage-3-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.25000000000000006 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.20000000000000007 xa=0.0 ym=0.075 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.15000000000000008 xa=0.0 ym=0.125 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.125 ya=0.0
	techBits=24 native-high-voltage-1-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.125 ya=0.0
		point xm=0.4 xa=0.0 ym=0.125 ya=0.0
	techBits=25 native-high-voltage-1-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.125 ya=0.0
		point xm=0.4 xa=0.0 ym=0.125 ya=0.0
	techBits=26 native-high-voltage-2-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.125 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.125 ya=0.0
	techBits=27 native-high-voltage-2-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.125 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.125 ya=0.0
	techBits=28 native-high-voltage-3-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.25000000000000006 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.20000000000000007 xa=0.0 ym=0.075 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.15000000000000008 xa=0.0 ym=0.125 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.125 ya=0.0
	techBits=29 native-high-voltage-3-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.25000000000000006 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.20000000000000007 xa=0.0 ym=0.075 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.15000000000000008 xa=0.0 ym=0.125 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.125 ya=0.0
	techBits=30 carbon-nanotube-nMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.3125 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.3125 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	techBits=31 carbon-nanotube-pMOS-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.3125 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.3125 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
MultiFunction PrimitiveNode Resistor resistor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[1.0,1.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-0.5,w=6.0,h=1.0]
	baseRectangle=ERectangle[x=-2.0,y=-0.5,w=4.0,h=1.0]
	DefaultExtendXForResistorINschematic=0.0
	DefaultExtendYForResistorINschematic=0.0
	diskOffset1=3.0,0.5
	diskOffset2=2.0,0.5
	layers:
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	port a angle=180 range=90 topology=0 unknown
		lm=-0.3333333333 la=0.0 rm=-0.3333333333 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port b angle=0 range=90 topology=1 unknown
		lm=0.3333333333 la=0.0 rm=0.3333333333 ra=0.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	techBits=0 resistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	techBits=1 n-type-poly-resistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="N" td=20000000000 colorIndex=0 disp=true
		point xm=0.2 xa=0.0 ym=0.0 ya=0.0
		point xm=0.2 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
	techBits=2 p-type-poly-resistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="P" td=20000000000 colorIndex=0 disp=true
		point xm=0.2 xa=0.0 ym=0.0 ya=0.0
		point xm=0.2 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
	techBits=3 n-type-well-resistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="N" td=20000000000 colorIndex=0 disp=true
		point xm=0.2 xa=0.0 ym=0.0 ya=0.0
		point xm=0.2 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=OPENEDT2 repr=0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
	techBits=4 p-type-well-resistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="P" td=20000000000 colorIndex=0 disp=true
		point xm=0.2 xa=0.0 ym=0.0 ya=0.0
		point xm=0.2 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=OPENEDT2 repr=0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
	techBits=5 n-type-active-resistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="N" td=20000000000 colorIndex=0 disp=true
		point xm=0.2 xa=0.0 ym=0.0 ya=0.0
		point xm=0.2 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=OPENEDT3 repr=0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
	techBits=6 p-type-active-resistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="P" td=20000000000 colorIndex=0 disp=true
		point xm=0.2 xa=0.0 ym=0.0 ya=0.0
		point xm=0.2 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=OPENEDT3 repr=0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.5 ya=0.0
	techBits=7 n-type-no-silicide-poly-resistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="US-N" td=20000000000 colorIndex=0 disp=true
		point xm=0.2 xa=0.0 ym=0.0 ya=0.0
		point xm=0.2 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
	techBits=8 p-type-no-silicide-poly-resistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="US-P" td=20000000000 colorIndex=0 disp=true
		point xm=0.2 xa=0.0 ym=0.0 ya=0.0
		point xm=0.2 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
	techBits=9 hi-res-poly2-resistor
	layer=Node port=0 style=OPENEDT3 repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	techBits=10 resistor-bias
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.3333333333 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.15 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.05 xa=0.0 ym=0.5 ya=0.0
		point xm=0.05 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.15 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3333333333 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=DISC repr=0
		point xm=3.0 xa=-19.85 ym=0.0 ya=0.25
		point xm=3.0 xa=-19.975 ym=0.0 ya=0.25
MultiFunction PrimitiveNode Capacitor capacitor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.5,y=-2.0,w=3.0,h=4.0]
	baseRectangle=ERectangle[x=-1.5,y=-2.0,w=3.0,h=4.0]
	DefaultExtendXForCapacitorINschematic=0.0
	DefaultExtendYForCapacitorINschematic=0.0
	diskOffset1=1.5,2.0
	diskOffset2=1.5,2.0
	layers:
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	port a angle=90 range=90 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port b angle=270 range=90 topology=1 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	techBits=0 capacitor
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	techBits=1 electrolytic-capacitor
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.1 xa=0.0 ym=-0.3 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.2 ya=0.0
		point xm=0.2 xa=0.0 ym=-0.4 ya=0.0
	techBits=2 poly2-capacitor
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=0.1 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.1 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENEDT3 repr=0
		point xm=-0.5 xa=0.0 ym=0.1 ya=0.0
		point xm=0.5 xa=0.0 ym=0.1 ya=0.0
MultiFunction PrimitiveNode Diode diode
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-2.0,w=2.0,h=4.0]
	baseRectangle=ERectangle[x=-1.0,y=-2.0,w=2.0,h=4.0]
	DefaultExtendXForDiodeINschematic=0.0
	DefaultExtendYForDiodeINschematic=0.0
	diskOffset1=1.0,2.0
	diskOffset2=1.0,2.0
	layers:
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.25 ya=0.0
		point xm=0.5 xa=0.0 ym=0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=FILLED repr=0
		point xm=-0.5 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.25 ya=0.0
	port a angle=90 range=90 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port b angle=270 range=90 topology=1 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	techBits=0 diode
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.25 ya=0.0
		point xm=0.5 xa=0.0 ym=0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=FILLED repr=0
		point xm=-0.5 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.25 ya=0.0
	techBits=1 zener-diode
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.375 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.25 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.25 ya=0.0
		point xm=0.5 xa=0.0 ym=0.25 ya=0.0
		point xm=0.5 xa=0.0 ym=0.25 ya=0.0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=FILLED repr=0
		point xm=-0.5 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.25 ya=0.0
PrimitiveNode Inductor inductor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-2.0,w=2.0,h=4.0]
	baseRectangle=ERectangle[x=-1.0,y=-2.0,w=2.0,h=4.0]
	DefaultExtendXForInductorINschematic=0.0
	DefaultExtendYForInductorINschematic=0.0
	diskOffset1=1.0,2.0
	diskOffset2=1.0,2.0
	layers:
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=-0.25 xa=0.0 ym=0.16666666665 ya=0.0
		point xm=0.0 xa=0.0 ym=0.16666666665 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=-0.25 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=-0.25 xa=0.0 ym=-0.16666666665 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.16666666665 ya=0.0
	port a angle=90 range=90 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port b angle=270 range=90 topology=1 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Josephson-Junction josephson-junction-transistor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForJosephson-JunctionINschematic=0.0
	DefaultExtendYForJosephson-JunctionINschematic=0.0
	diskOffset1=3.0,3.0
	diskOffset2=3.0,3.0
	layers:
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=5.0 ym=0.5 ya=-5.0
		point xm=0.5 xa=-5.0 ym=-0.5 ya=5.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=5.0 ym=-0.5 ya=5.0
		point xm=0.5 xa=-5.0 ym=0.5 ya=-5.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=1.0 ym=0.5 ya=-0.75
		point xm=0.0 xa=1.25 ym=0.5 ya=-0.75
	port s angle=90 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=6.0 tm=-0.5 ta=6.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port d angle=270 range=180 topology=1 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=-6.0 tm=0.5 ta=-6.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Meter meter NSQUARE
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForMeterINschematic=0.0
	DefaultExtendYForMeterINschematic=0.0
	diskOffset1=3.0,3.0
	diskOffset2=3.0,3.0
	layers:
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=TEXTBOX repr=0
		message="V" td=20000000000 colorIndex=0 disp=true
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port a angle=90 range=45 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port b angle=270 range=45 topology=1 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Well well
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-1.0,w=4.0,h=2.0]
	baseRectangle=ERectangle[x=-2.0,y=-1.0,w=4.0,h=2.0]
	DefaultExtendXForWellINschematic=0.0
	DefaultExtendYForWellINschematic=0.0
	diskOffset1=2.0,1.0
	diskOffset2=2.0,1.0
	layers:
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	port well angle=90 range=90 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Substrate substrate
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	baseRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	DefaultExtendXForSubstrateINschematic=0.0
	DefaultExtendYForSubstrateINschematic=0.0
	diskOffset1=1.5,1.5
	diskOffset2=1.5,1.5
	layers:
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	port substrate angle=90 range=90 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
MultiFunction PrimitiveNode Two-Port transmission-line
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-5.0,y=-3.0,w=10.0,h=6.0]
	baseRectangle=ERectangle[x=-5.0,y=-3.0,w=10.0,h=6.0]
	DefaultExtendXForTwo-PortINschematic=0.0
	DefaultExtendYForTwo-PortINschematic=0.0
	diskOffset1=5.0,3.0
	diskOffset2=5.0,3.0
	layers:
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.4 xa=0.0 ym=0.5 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.4 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=-0.4 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.4 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.3333333333 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.175 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.225 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.29166666665 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.375 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.175 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.225 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.2 xa=0.0 ym=0.29166666665 ya=0.0
		point xm=0.2 xa=0.0 ym=0.375 ya=0.0
	port a angle=180 range=90 topology=0 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=0.3333333333 ba=0.0 tm=0.3333333333 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port b angle=180 range=90 topology=1 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=-0.3333333333 ba=0.0 tm=-0.3333333333 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port x angle=0 range=90 topology=2 unknown
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=0.3333333333 ba=0.0 tm=0.3333333333 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port y angle=0 range=90 topology=3 unknown
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.3333333333 ba=0.0 tm=-0.3333333333 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	techBits=0 vccs
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.4 xa=0.0 ym=0.5 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.15 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.15 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.3 xa=0.0 ym=0.15 ya=0.0
		point xm=0.225 xa=0.0 ym=0.0 ya=0.0
		point xm=0.225 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.15 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.15 ya=0.0
		point xm=0.375 xa=0.0 ym=0.0 ya=0.0
		point xm=0.375 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3 xa=0.0 ym=0.15 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.19166666665 xa=0.0 ym=0.16666666665 ya=0.0
		point xm=0.19166666665 xa=0.0 ym=-0.16666666665 ya=0.0
		point xm=0.19166666665 xa=0.0 ym=-0.16666666665 ya=0.0
		point xm=0.16666666665 xa=0.0 ym=-0.083333333 ya=0.0
		point xm=0.19166666665 xa=0.0 ym=-0.16666666665 ya=0.0
		point xm=0.21666666665 xa=0.0 ym=-0.083333333 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.175 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.225 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.29166666665 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.375 ya=0.0
	techBits=1 ccvs
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.4 xa=0.0 ym=0.5 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENEDT1 repr=0
		point xm=-0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.3333333333 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.15 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.15 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3 xa=0.0 ym=0.15 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.175 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.225 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.29166666665 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.375 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.175 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.225 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.2 xa=0.0 ym=0.29166666665 ya=0.0
		point xm=0.2 xa=0.0 ym=0.375 ya=0.0
	techBits=2 vcvs
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.4 xa=0.0 ym=0.5 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.15 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.15 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.3 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3 xa=0.0 ym=0.15 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.175 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.225 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.29166666665 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.375 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.175 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.225 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.2 xa=0.0 ym=0.29166666665 ya=0.0
		point xm=0.2 xa=0.0 ym=0.375 ya=0.0
	techBits=3 cccs
	layer=Node port=0 style=CLOSED repr=1
		point xm=-0.4 xa=0.0 ym=0.5 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENEDT1 repr=0
		point xm=-0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.3333333333 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=0.15 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.15 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.3 xa=0.0 ym=0.15 ya=0.0
		point xm=0.225 xa=0.0 ym=0.0 ya=0.0
		point xm=0.225 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.15 ya=0.0
		point xm=0.3 xa=0.0 ym=-0.15 ya=0.0
		point xm=0.375 xa=0.0 ym=0.0 ya=0.0
		point xm=0.375 xa=0.0 ym=0.0 ya=0.0
		point xm=0.3 xa=0.0 ym=0.15 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.19166666665 xa=0.0 ym=0.16666666665 ya=0.0
		point xm=0.19166666665 xa=0.0 ym=-0.16666666665 ya=0.0
		point xm=0.19166666665 xa=0.0 ym=-0.16666666665 ya=0.0
		point xm=0.16666666665 xa=0.0 ym=-0.083333333 ya=0.0
		point xm=0.19166666665 xa=0.0 ym=-0.16666666665 ya=0.0
		point xm=0.21666666665 xa=0.0 ym=-0.083333333 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.175 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.225 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.29166666665 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.375 ya=0.0
	techBits=4 transmission-line
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.4 xa=0.0 ym=0.5 ya=0.0
		point xm=0.4 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.4 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.4 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.4 xa=0.0 ym=0.5 ya=0.0
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=-0.8 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.4 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.4 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLEARC repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.4 xa=0.0 ym=0.5 ya=0.0
		point xm=0.4 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.4 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=-0.4 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.5 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.45 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.3333333333 ya=0.0
		point xm=0.45 xa=0.0 ym=-0.3333333333 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.175 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.225 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.29166666665 ya=0.0
		point xm=-0.2 xa=0.0 ym=0.375 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.2583333333 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.3083333333 xa=0.0 ym=0.3333333333 ya=0.0
		point xm=0.2833333333 xa=0.0 ym=0.29166666665 ya=0.0
		point xm=0.2833333333 xa=0.0 ym=0.375 ya=0.0
MultiFunction PrimitiveNode 4-Port-Transistor 4-port-transistor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,1.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=3.0]
	DefaultExtendXFor4-Port-TransistorINschematic=0.0
	DefaultExtendYFor4-Port-TransistorINschematic=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,1.5
	layers:
	layer=Node port=0 style=VECTORS repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	port g angle=0 range=180 topology=0 input
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=-1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port s angle=180 range=90 topology=1 bidirectional
		lm=-0.5 la=0.0 rm=-0.5 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port d angle=0 range=90 topology=2 bidirectional
		lm=0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port b angle=270 range=90 topology=3 input
		lm=-0.25 la=0.0 rm=-0.25 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
	techBits=0 nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=1 depletion-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=FILLED repr=1
		point xm=-0.375 xa=0.0 ym=-0.375 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.4375 ya=0.0
	techBits=2 pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=3 NPN-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.4375 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	techBits=4 PNP-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.25 xa=0.0 ym=-0.1875 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	techBits=5 n-type-JFET-4-port-transistor
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.0625 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0625 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=6 p-type-JFET-4-port-transistor
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.0625 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0625 xa=0.0 ym=0.0 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.25 ya=0.0
	techBits=7 4-port-depletion-mesfet
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.25 ya=0.0
	techBits=8 4-port-enhancement-mesfet
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.4375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.125 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.25 ya=0.0
	techBits=9 depletion-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=FILLED repr=1
		point xm=-0.375 xa=0.0 ym=-0.375 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.4375 ya=0.0
	techBits=10 native-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=11 native-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=12 floating-gate-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.1875 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.1875 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=13 floating-gate-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.1875 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.1875 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=14 low-threshold-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.195 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.195 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.195 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=15 low-threshold-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.195 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.195 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=-0.07 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.195 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.05499999999999999 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=16 high-threshold-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.05499999999999999 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.05499999999999999 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.05499999999999999 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=17 high-threshold-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.05499999999999999 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.05499999999999999 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.07 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.05499999999999999 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.195 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=18 high-voltage-1-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.125 ya=0.0
		point xm=0.4 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=19 high-voltage-1-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.125 ya=0.0
		point xm=0.4 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=20 high-voltage-2-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.125 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=21 high-voltage-2-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.125 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=22 high-voltage-3-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.25000000000000006 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.20000000000000007 xa=0.0 ym=0.075 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.15000000000000008 xa=0.0 ym=0.125 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=23 high-voltage-3-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.25000000000000006 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.20000000000000007 xa=0.0 ym=0.075 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.15000000000000008 xa=0.0 ym=0.125 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=24 native-high-voltage-1-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.125 ya=0.0
		point xm=0.4 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=25 native-high-voltage-1-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.125 ya=0.0
		point xm=0.4 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=26 native-high-voltage-2-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.125 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=27 native-high-voltage-2-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.125 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=28 native-high-voltage-3-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.25000000000000006 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.20000000000000007 xa=0.0 ym=0.075 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.15000000000000008 xa=0.0 ym=0.125 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=29 native-high-voltage-3-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.5 xa=0.0 ym=0.125 ya=0.0
		point xm=0.45 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.45 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.45 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.4 xa=0.0 ym=0.075 ya=0.0
		point xm=0.4 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.35000000000000003 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.35000000000000003 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.30000000000000004 xa=0.0 ym=0.075 ya=0.0
		point xm=0.30000000000000004 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.25000000000000006 xa=0.0 ym=0.024999999999999994 ya=0.0
		point xm=0.25000000000000006 xa=0.0 ym=0.225 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.20000000000000007 xa=0.0 ym=0.075 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.175 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.15000000000000008 xa=0.0 ym=0.125 ya=0.0
		point xm=0.20000000000000007 xa=0.0 ym=0.125 ya=0.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.175 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3333333333 xa=0.0 ym=-0.375 ya=0.0
	techBits=30 carbon-nanotube-nMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.3125 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.3125 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.4375 ya=0.0
	techBits=31 carbon-nanotube-pMOS-4-port-transistor
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.25 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.3125 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.25 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.3125 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.125 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.0625 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=-0.125 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=-0.0625 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.1875 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.17783121635129678 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.2139156081756484 ya=0.0
		point xm=-0.3125 xa=0.0 ym=-0.28608439182435164 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.3221687836487032 ya=0.0
		point xm=-0.1875 xa=0.0 ym=-0.28608439182435164 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=-0.375 xa=0.0 ym=-0.125 ya=0.0
		point xm=0.375 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=CIRCLE repr=0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.125 ya=0.0
	layer=Node port=0 style=OPENED repr=0
		point xm=0.0 xa=0.0 ym=0.125 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=-1.0
	layer=Node port=0 style=VECTORS repr=0
		point xm=-0.25 xa=0.0 ym=-0.375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.2 xa=0.0 ym=-0.4375 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.3 xa=0.0 ym=-0.4375 ya=0.0
PrimitiveNode Global-Signal connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	baseRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	DefaultExtendXForGlobal-SignalINschematic=0.0
	DefaultExtendYForGlobal-SignalINschematic=0.0
	diskOffset1=1.5,1.5
	diskOffset2=1.5,1.5
	layers:
	layer=Node port=0 style=CLOSED repr=0
		point xm=-0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
	layer=Node port=0 style=CLOSED repr=0
		point xm=-0.45 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.45 ya=0.0
		point xm=0.45 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=-0.45 ya=0.0
	port global angle=270 range=90 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Global-Partition connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-1.0,w=4.0,h=2.0]
	baseRectangle=ERectangle[x=-2.0,y=-1.0,w=4.0,h=2.0]
	DefaultExtendXForGlobal-PartitionINschematic=0.0
	DefaultExtendYForGlobal-PartitionINschematic=0.0
	diskOffset1=2.0,1.0
	diskOffset2=2.0,1.0
	layers:
	layer=Node port=0 style=CLOSED repr=0
		point xm=-0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=-0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=0.25 xa=0.0 ym=0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.0 ya=0.0
		point xm=0.25 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.25 xa=0.0 ym=-0.5 ya=0.0
	layer=Text port=0 style=TEXTCENT repr=0
		message="GP" td=20000000000 colorIndex=0 disp=true
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
		point xm=0.0 xa=0.0 ym=0.0 ya=0.0
	port top angle=90 range=90 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bottom angle=270 range=90 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=0.0 tm=-0.5 ta=0.0
		isolated=false negatable=false
		portArc wire
		portArc bus
		portArc Universal
		portArc Invisible
		portArc Unrouted
Foundry NONE
	schematic.GDS.Arc=()
	schematic.GDS.Bus=()
	schematic.GDS.Node=()
	schematic.GDS.Text=()
 menu 0 0 arc wire
 menu 0 1 arc bus
 menu 1 0 nodeInst Wire_Pin:pin:
 menu 1 1 nodeInst Bus_Pin:pin:
 menu 2 0 Spice
 menu 2 1 Cell
 menu 3 0 node Off-Page
 menu 3 1 node Wire_Con
 menu 4 0 nodeInst Global-Signal:connection::Global:true nodeInst Global-Partition:connection::Partition:true
 menu 4 1 Misc.
 menu 5 0 node Power
 menu 5 1 node Ground
 menu 6 0 nodeInst Resistor:resistor::Normal:true nodeInst Resistor:n-type-poly-resistor::N-Poly:true nodeInst Resistor:p-type-poly-resistor::P-Poly:true nodeInst Resistor:n-type-well-resistor::N-Well:true nodeInst Resistor:p-type-well-resistor::P-Well:true nodeInst Resistor:n-type-active-resistor::N-Active:true nodeInst Resistor:p-type-active-resistor::P-Active:true nodeInst Resistor:n-type-no-silicide-poly-resistor::NoS-N-Poly:true nodeInst Resistor:p-type-no-silicide-poly-resistor::NoS-P-Poly:true nodeInst Resistor:hi-res-poly2-resistor::Hi-Res-Poly2:true nodeInst Resistor:resistor-bias::Bias:true
 menu 6 1 nodeInst Inductor:inductor::Induct:true nodeInst Josephson-Junction:josephson-junction-transistor::JJ:true
 menu 7 0 nodeInst Capacitor:capacitor::Normal:true nodeInst Capacitor:electrolytic-capacitor::Electro:true nodeInst Capacitor:poly2-capacitor::P1-P2:true
 menu 7 1 nodeInst Diode:diode::Normal:true nodeInst Diode:zener-diode::Zener:true
 menu 8 0 nodeInst 4-Port-Transistor:nMOS-4-port-transistor:R:nMOS:true nodeInst 4-Port-Transistor:pMOS-4-port-transistor:R:pMOS:true nodeInst 4-Port-Transistor:depletion-nMOS-4-port-transistor:R:nMOS D:true nodeInst 4-Port-Transistor:depletion-pMOS-4-port-transistor:R:pMOS D:true nodeInst 4-Port-Transistor:native-nMOS-4-port-transistor:R:nMOS NT:true nodeInst 4-Port-Transistor:native-pMOS-4-port-transistor:R:pMOS NT:true nodeInst 4-Port-Transistor:floating-gate-nMOS-4-port-transistor:R:nMOS FG:true nodeInst 4-Port-Transistor:floating-gate-pMOS-4-port-transistor:R:pMOS FG:true nodeInst 4-Port-Transistor:carbon-nanotube-nMOS-4-port-transistor:R:nMOS CN:true nodeInst 4-Port-Transistor:carbon-nanotube-pMOS-4-port-transistor:R:pMOS CN:true nodeInst 4-Port-Transistor:low-threshold-nMOS-4-port-transistor:R:nMOS VTL:true nodeInst 4-Port-Transistor:low-threshold-pMOS-4-port-transistor:R:pMOS VTL:true nodeInst 4-Port-Transistor:high-threshold-nMOS-4-port-transistor:R:nMOS VTH:true nodeInst 4-Port-Transistor:high-threshold-pMOS-4-port-transistor:R:pMOS -VTH:true nodeInst 4-Port-Transistor:high-voltage-1-nMOS-4-port-transistor:R:nMOS HV1:true nodeInst 4-Port-Transistor:high-voltage-1-pMOS-4-port-transistor:R:pMOS HV1:true nodeInst 4-Port-Transistor:high-voltage-2-nMOS-4-port-transistor:R:nMOS HV2:true nodeInst 4-Port-Transistor:high-voltage-2-pMOS-4-port-transistor:R:pMOS HV2:true nodeInst 4-Port-Transistor:high-voltage-3-nMOS-4-port-transistor:R:nMOS HV3:true nodeInst 4-Port-Transistor:high-voltage-3-pMOS-4-port-transistor:R:pMOS HV3:true nodeInst 4-Port-Transistor:native-high-voltage-1-nMOS-4-port-transistor:R:nMOS NT/HV1:true nodeInst 4-Port-Transistor:native-high-voltage-1-pMOS-4-port-transistor:R:pMOS NT/HV1:true nodeInst 4-Port-Transistor:native-high-voltage-2-nMOS-4-port-transistor:R:nMOS NT/HV2:true nodeInst 4-Port-Transistor:native-high-voltage-2-pMOS-4-port-transistor:R:pMOS NT/HV2:true nodeInst 4-Port-Transistor:native-high-voltage-3-nMOS-4-port-transistor:R:nMOS NT/HV3:true nodeInst 4-Port-Transistor:native-high-voltage-3-pMOS-4-port-transistor:R:pMOS NT/HV3:true nodeInst 4-Port-Transistor:NPN-4-port-transistor:R:NPN:true nodeInst 4-Port-Transistor:PNP-4-port-transistor:R:PNP:true nodeInst 4-Port-Transistor:4-port-depletion-mesfet:R:DMES:true nodeInst 4-Port-Transistor:4-port-enhancement-mesfet:R:EMES:true nodeInst 4-Port-Transistor:p-type-JFET-4-port-transistor:R:pJFET:true nodeInst 4-Port-Transistor:p-type-JFET-4-port-transistor:R:nJFET:true
 menu 8 1 nodeInst Transistor:pMOS-transistor:R
 menu 9 0 nodeInst Transistor:nMOS-transistor:R:nMOS:true nodeInst Transistor:pMOS-transistor:R:pMOS:true nodeInst Transistor:depletion-nMOS-transistor:R:nMOS D:true nodeInst Transistor:depletion-pMOS-transistor:R:pMOS D:true nodeInst Transistor:native-nMOS-transistor:R:nMOS NT:true nodeInst Transistor:native-pMOS-transistor:R:pMOS NT:true nodeInst Transistor:floating-gate-nMOS-transistor:R:nMOS FG:true nodeInst Transistor:floating-gate-pMOS-transistor:R:pMOS FG:true nodeInst Transistor:carbon-nanotube-nMOS-transistor:R:nMOS CN:true nodeInst Transistor:carbon-nanotube-pMOS-transistor:R:pMOS CN:true nodeInst Transistor:low-threshold-nMOS-transistor:R:nMOS VTL:true nodeInst Transistor:low-threshold-pMOS-transistor:R:pMOS VTL:true nodeInst Transistor:high-threshold-nMOS-transistor:R:nMOS VTH:true nodeInst Transistor:high-threshold-pMOS-transistor:R:pMOS VTH:true nodeInst Transistor:high-voltage-1-nMOS-transistor:R:nMOS HV1:true nodeInst Transistor:high-voltage-1-pMOS-transistor:R:pMOS HV1:true nodeInst Transistor:high-voltage-2-nMOS-transistor:R:nMOS HV2:true nodeInst Transistor:high-voltage-2-pMOS-transistor:R:pMOS HV2:true nodeInst Transistor:high-voltage-3-nMOS-transistor:R:nMOS HV3:true nodeInst Transistor:high-voltage-3-pMOS-transistor:R:pMOS HV3:true nodeInst Transistor:native-high-voltage-1-nMOS-transistor:R:nMOS NT/HV1:true nodeInst Transistor:native-high-voltage-1-pMOS-transistor:R:pMOS NT/HV1:true nodeInst Transistor:native-high-voltage-2-nMOS-transistor:R:nMOS NT/HV2:true nodeInst Transistor:native-high-voltage-2-pMOS-transistor:R:pMOS NT/HV2:true nodeInst Transistor:native-high-voltage-3-nMOS-transistor:R:nMOS NT/HV3:true nodeInst Transistor:native-high-voltage-3-pMOS-transistor:R:pMOS NT/HV3:true nodeInst Transistor:NPN-transistor:R:NPN:true nodeInst Transistor:PNP-transistor:R:PNP:true nodeInst Transistor:depletion-mesfet:R:DMES:true nodeInst Transistor:enhancement-mesfet:R:EMES:true nodeInst Transistor:p-type-JFET-transistor:R:pJFET:true nodeInst Transistor:n-type-JFET-transistor:R:nJFET:true
 menu 9 1 nodeInst Transistor:nMOS-transistor:R
 menu 10 0 node Switch
 menu 10 1 nodeInst Flip-Flop:flip-flop-RS-MS::RS M/S:true nodeInst Flip-Flop:flip-flop-RS-P::RS pos:true nodeInst Flip-Flop:flip-flop-RS-N::RS neg:true - nodeInst Flip-Flop:flip-flop-JK-MS::JK M/S:true nodeInst Flip-Flop:flip-flop-JK-P::JK pos:true nodeInst Flip-Flop:flip-flop-JK-N::JK neg:true - nodeInst Flip-Flop:flip-flop-D-MS::D M/S:true nodeInst Flip-Flop:flip-flop-D-P::D pos:true nodeInst Flip-Flop:flip-flop-D-N::D neg:true - nodeInst Flip-Flop:flip-flop-T-MS::T M/S:true nodeInst Flip-Flop:flip-flop-T-P::T pos:true nodeInst Flip-Flop:flip-flop-T-N::T neg:true
 menu 11 0 node Mux
 menu 11 1 node Buffer
 menu 12 0 node Xor
 menu 12 1 node Or
 menu 13 0 node Bbox
 menu 13 1 node And
    <Foundry name="NONE">
    </Foundry>
