Technology tft
class com.sun.electric.technology.Technology
shortName=tft
techDesc=Thin Film
Bits:  NONEGATEDARCS
isScaleRelevant=truetft.Scale=5000.0(5000.0)
tft.Foundry=NONE(NONE)
tft.NumMetalLayers=2(2)
tft.MininumResistance=0.0(0.0)
tft.GateLengthSubtraction=0.0(0.0)
tft.Gate Inclusion=false(false)
tft.Ground Net Inclusion=false(false)
tft.MaxSeriesResistance=10.0(10.0)
tft.LogicalEffort.GateCapacitance=0.4(0.4)
tft.LogicalEffort.WireRatio=0.16(0.16)
tft.LogicalEffort.DiffAlpha=0.7(0.7)
ResolutionValueFortft=0.0
TRANSPARENT_1=ff00d1ff
TRANSPARENT_2=ffff9bc0
TRANSPARENT_3=ff6be260
TRANSPARENT_4=ffffd700
Layer Metal-1 METAL1
	tft.CIF.Metal-1=CMF(CMF)
	tft.DXF.Metal-1=()
	tft.Skill.Metal-1=()
	tft.Resistance.Metal-1=0.0(0.0)
	tft.Capacitance.Metal-1=0.0(0.0)
	tft.EdgeCapacitance.Metal-1=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=1(1)
	color=ff00d1ff(d1ff)
	opacity=0.8(0.8)
	foreground=true
	pattern ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Metal-2 METAL2
	tft.CIF.Metal-2=CMS(CMS)
	tft.DXF.Metal-2=()
	tft.Skill.Metal-2=()
	tft.Resistance.Metal-2=0.0(0.0)
	tft.Capacitance.Metal-2=0.0(0.0)
	tft.EdgeCapacitance.Metal-2=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=4(4)
	color=ffffd700(ffd700)
	opacity=0.7(0.7)
	foreground=true
	pattern 1010 2020 4040 8080 101 202 404 808 1010 2020 4040 8080 101 202 404 808
	distance3D=22.15
	thickness3D=2.65
	mode3D=NONE
	factor3D=0.0
Layer HiK POLY1
	tft.CIF.HiK=CPG(CPG)
	tft.DXF.HiK=()
	tft.Skill.HiK=()
	tft.Resistance.HiK=0.0(0.0)
	tft.Capacitance.HiK=0.0(0.0)
	tft.EdgeCapacitance.HiK=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=2(2)
	color=ffff9bc0(ff9bc0)
	opacity=0.8(0.8)
	foreground=true
	pattern 808 404 202 101 8080 4040 2020 1010 808 404 202 101 8080 4040 2020 1010
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Pent DIFFP
	tft.CIF.Pent=CSP(CSP)
	tft.DXF.Pent=()
	tft.Skill.Pent=()
	tft.Resistance.Pent=0.0(0.0)
	tft.Capacitance.Pent=0.0(0.0)
	tft.EdgeCapacitance.Pent=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=0(0)
	color=ffff00ff(ff00ff)
	opacity=0.8(0.8)
	foreground=true
	pattern e0e0 7070 3838 1c1c e0e 707 8383 c1c1 e0e0 7070 3838 1c1c e0e 707 8383 c1c1
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Via1 CONTACT1
	tft.CIF.Via1=CVA(CVA)
	tft.DXF.Via1=()
	tft.Skill.Via1=()
	tft.Resistance.Via1=0.0(0.0)
	tft.Capacitance.Via1=0.0(0.0)
	tft.EdgeCapacitance.Via1=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=Solid-Thick(Solid-Thick)
	transparent=3(3)
	color=ff6be260(6be260)
	opacity=0.5(0.5)
	foreground=true
	pattern 0 303 4848 303 0 3030 8484 3030 0 303 4848 303 0 3030 8484 3030
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Passivation OVERGLASS
	tft.CIF.Passivation=COG(COG)
	tft.DXF.Passivation=()
	tft.Skill.Passivation=()
	tft.Resistance.Passivation=0.0(0.0)
	tft.Capacitance.Passivation=0.0(0.0)
	tft.EdgeCapacitance.Passivation=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=0(0)
	color=ff666666(666666)
	opacity=0.8(0.8)
	foreground=true
	pattern 1c1c 3e3e 3636 3e3e 1c1c 0 0 0 1c1c 3e3e 3636 3e3e 1c1c 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer lay1 UNKNOWN
	tft.CIF.lay1=uk1(uk1)
	tft.DXF.lay1=()
	tft.Skill.lay1=()
	tft.Resistance.lay1=0.0(0.0)
	tft.Capacitance.lay1=0.0(0.0)
	tft.EdgeCapacitance.lay1=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=Solid(Solid)
	transparent=0(0)
	color=ffffff00(ffff00)
	opacity=1.0(1.0)
	foreground=false
	pattern ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer lay2 UNKNOWN
	tft.CIF.lay2=uk2(uk2)
	tft.DXF.lay2=()
	tft.Skill.lay2=()
	tft.Resistance.lay2=0.0(0.0)
	tft.Capacitance.lay2=0.0(0.0)
	tft.EdgeCapacitance.lay2=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=Solid(Solid)
	transparent=0(0)
	color=ff66ff00(66ff00)
	opacity=1.0(1.0)
	foreground=false
	pattern ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer lay3 UNKNOWN
	tft.CIF.lay3=uk3(uk3)
	tft.DXF.lay3=()
	tft.Skill.lay3=()
	tft.Resistance.lay3=0.0(0.0)
	tft.Capacitance.lay3=0.0(0.0)
	tft.EdgeCapacitance.lay3=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=Solid(Solid)
	transparent=0(0)
	color=ffffff66(ffff66)
	opacity=1.0(1.0)
	foreground=false
	pattern ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer lay4 UNKNOWN
	tft.CIF.lay4=uk4(uk4)
	tft.DXF.lay4=()
	tft.Skill.lay4=()
	tft.Resistance.lay4=0.0(0.0)
	tft.Capacitance.lay4=0.0(0.0)
	tft.EdgeCapacitance.lay4=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=Solid(Solid)
	transparent=0(0)
	color=ff66ff00(66ff00)
	opacity=1.0(1.0)
	foreground=false
	pattern ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0 ffff 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
ArcProto Metal_1 metal-1
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForMetal_1INtft=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=1.0
	diskOffset2=1.0
	DefaultAngleForMetal_1INtft=90
	DefaultRigidForMetal_1INtft=false
	DefaultFixedAngleForMetal_1INtft=true
	DefaultExtendedForMetal_1INtft=true
	DefaultDirectionalForMetal_1INtft=false
		arcLayer layer=Metal-1 style=FILLED extend=1.0
ArcProto Metal_2 metal-2
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForMetal_2INtft=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=1.0
	diskOffset2=1.0
	DefaultAngleForMetal_2INtft=90
	DefaultRigidForMetal_2INtft=false
	DefaultFixedAngleForMetal_2INtft=true
	DefaultExtendedForMetal_2INtft=true
	DefaultDirectionalForMetal_2INtft=false
		arcLayer layer=Metal-2 style=FILLED extend=1.0
PrimitiveNode Metal-1-Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForMetal-1-PinINtft=0.0
	DefaultExtendYForMetal-1-PinINtft=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Metal-1 port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal-1 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-2-Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForMetal-2-PinINtft=0.0
	DefaultExtendYForMetal-2-PinINtft=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Metal-2 port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal-2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-Metal-2-Con contact
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.5,y=-2.5,w=5.0,h=5.0]
	baseRectangle=ERectangle[x=-2.5,y=-2.5,w=5.0,h=5.0]
	DefaultExtendXForMetal-1-Metal-2-ConINtft=0.0
	DefaultExtendYForMetal-1-Metal-2-ConINtft=0.0
	diskOffset1=2.5,2.5
	diskOffset2=2.5,2.5
	layers:
	layer=Metal-1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Metal-2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Via1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=1.5 ym=-0.5 ya=1.5
		point xm=0.5 xa=-1.5 ym=0.5 ya=-1.5
	port metal-1-metal-2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.5 rm=0.5 ra=-1.5 bm=-0.5 ba=1.5 tm=0.5 ta=-1.5
		isolated=false negatable=false
		portArc Metal_1
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode capacitor capacitor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[3.0,3.0] Y:[3.0,3.0]}
	fullRectangle=ERectangle[x=-5.5,y=-5.5,w=11.0,h=11.0]
	baseRectangle=ERectangle[x=-2.5,y=-2.5,w=5.0,h=5.0]
	DefaultExtendXForcapacitorINtft=0.0
	DefaultExtendYForcapacitorINtft=0.0
	diskOffset1=5.5,5.5
	diskOffset2=2.5,2.5
	layers:
	layer=Metal-1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Metal-2 port=1 style=FILLED repr=1
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	layer=HiK port=0 style=FILLED repr=1
		point xm=-0.5 xa=1.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=-1.0
	layer=Via1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	port cap-met1 angle=0 range=180 topology=1 unknown
		lm=-0.5 la=5.5 rm=0.5 ra=-5.5 bm=-0.5 ba=5.5 tm=0.5 ta=-5.5
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port cap-met2-bot angle=0 range=180 topology=0 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=-0.5 ba=3.0 tm=-0.5 ta=3.0
		isolated=false negatable=false
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port cap-met2-left angle=0 range=180 topology=1 unknown
		lm=-0.5 la=3.0 rm=-0.5 ra=3.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port cap-met2-right angle=0 range=180 topology=2 unknown
		lm=0.5 la=-3.0 rm=0.5 ra=-3.0 bm=0.0 ba=0.0 tm=0.0 ta=0.0
		isolated=false negatable=false
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port cap-met2-top angle=0 range=180 topology=3 unknown
		lm=0.0 la=0.0 rm=0.0 ra=0.0 bm=0.5 ba=-3.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode P-Transistor pMOS-transistor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[3.0,3.0] Y:[5.0,5.0]}
	fullRectangle=ERectangle[x=-5.5,y=-5.5,w=11.0,h=11.0]
	baseRectangle=ERectangle[x=-2.5,y=-0.5,w=5.0,h=1.0]
	DefaultExtendXForP-TransistorINtft=0.0
	DefaultExtendYForP-TransistorINtft=0.0
	diskOffset1=5.5,5.5
	diskOffset2=2.5,0.5
	layers:
	layer=Metal-1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Metal-2 port=3 style=FILLED repr=1
		point xm=-0.5 xa=3.0 ym=0.5 ya=-5.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	layer=Metal-2 port=1 style=FILLED repr=1
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=-0.5 ya=5.0
	layer=HiK port=0 style=FILLED repr=1
		point xm=-0.5 xa=1.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=-1.0
	layer=Via1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	port trans-met1-left angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.5 rm=-0.5 ra=0.5 bm=-0.5 ba=5.5 tm=0.5 ta=-5.5
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port trans-met2-bot angle=0 range=180 topology=1 unknown
		lm=-0.5 la=5.5 rm=0.5 ra=-5.5 bm=-0.5 ba=4.0 tm=-0.5 ta=4.0
		isolated=false negatable=false
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port trans-met1-right angle=0 range=180 topology=0 unknown
		lm=-0.5 la=10.5 rm=0.5 ra=-0.5 bm=-0.5 ba=5.5 tm=0.5 ta=-5.5
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port trans-met2-top angle=0 range=180 topology=2 unknown
		lm=-0.5 la=5.5 rm=0.5 ra=-5.5 bm=0.5 ba=-4.0 tm=0.5 ta=-4.0
		isolated=false negatable=false
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-1-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForMetal-1-NodeINtft=2.0
	DefaultExtendYForMetal-1-NodeINtft=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Metal-1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal-1 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-2-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForMetal-2-NodeINtft=2.0
	DefaultExtendYForMetal-2-NodeINtft=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Metal-2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal-2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode HiK-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForHiK-NodeINtft=2.0
	DefaultExtendYForHiK-NodeINtft=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=HiK port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port polysilicon angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Pent-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPent-NodeINtft=1.0
	DefaultExtendYForPent-NodeINtft=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Pent port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port P2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Via1-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForVia1-NodeINtft=2.0
	DefaultExtendYForVia1-NodeINtft=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Via1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port active angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Passivation-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPassivation-NodeINtft=4.5
	DefaultExtendYForPassivation-NodeINtft=4.5
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Passivation port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port Passivation angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode lay1-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForlay1-NodeINtft=2.0
	DefaultExtendYForlay1-NodeINtft=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=lay1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port lay1 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode lay2-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForlay2-NodeINtft=2.0
	DefaultExtendYForlay2-NodeINtft=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=lay2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port lay2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode lay3-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForlay3-NodeINtft=2.0
	DefaultExtendYForlay3-NodeINtft=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=lay3 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port lay3 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode lay4-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForlay4-NodeINtft=2.0
	DefaultExtendYForlay4-NodeINtft=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=lay4 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port lay4 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
Foundry NONE
	tft.GDS.Metal-1=49(49)
	tft.GDS.Metal-2=51(51)
	tft.GDS.HiK=46(46)
	tft.GDS.Pent=44(44)
	tft.GDS.Via1=50(50)
	tft.GDS.Passivation=52(52)
	tft.GDS.lay1=1(1)
	tft.GDS.lay2=2(2)
	tft.GDS.lay3=3(3)
	tft.GDS.lay4=4(4)
 menu 0 0 arc Metal_1
 menu 0 1 node P-Transistor
 menu 1 0 arc Metal_2
 menu 1 1 node Metal-1-Metal-2-Con
 menu 2 0 nodeInst Metal-1-Pin:pin:
 menu 2 1 node capacitor
 menu 3 0 nodeInst Metal-2-Pin:pin:
 menu 3 1 Cell
 menu 4 0 Pure
 menu 4 1 Misc.
    <Foundry name="NONE">
        <layerGds layer="Metal-1" gds="49"/>
        <layerGds layer="Metal-2" gds="51"/>
        <layerGds layer="HiK" gds="46"/>
        <layerGds layer="Pent" gds="44"/>
        <layerGds layer="Via1" gds="50"/>
        <layerGds layer="Passivation" gds="52"/>
        <layerGds layer="lay1" gds="1"/>
        <layerGds layer="lay2" gds="2"/>
        <layerGds layer="lay3" gds="3"/>
        <layerGds layer="lay4" gds="4"/>
        <LayerRule ruleName="1.1" layerName="Metal-1" type="MINWID" when="ALL" value="2.0"/>
        <LayersRule ruleName="1.2" layerNames="{Metal-1,Metal-1}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayerRule ruleName="2.1" layerName="HiK" type="MINWID" when="ALL" value="4.0"/>
        <LayerRule ruleName="3.1" layerName="Pent" type="MINWID" when="ALL" value="4.0"/>
        <LayerRule ruleName="4.1" layerName="Via1" type="MINWID" when="ALL" value="2.0"/>
        <LayersRule ruleName="4.2" layerNames="{Via1,Via1}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayerRule ruleName="5.1" layerName="Metal-2" type="MINWID" when="ALL" value="2.0"/>
        <LayersRule ruleName="5.2" layerNames="{Metal-2,Metal-2}" type="UCONSPA" when="ALL" value="1.0"/>
        <LayerRule ruleName="6.1" layerName="Passivation" type="MINWID" when="ALL" value="9.0"/>
    </Foundry>
