Technology bicmos
class com.sun.electric.technology.Technology
shortName=null
techDesc=Bipolar/CMOS (from MOSIS, N-Well, SCE Rules)
Bits:  NONEGATEDARCS
isScaleRelevant=truebicmos.Scale=1000.0(1000.0)
bicmos.Foundry=MOSIS(MOSIS)
bicmos.NumMetalLayers=2(2)
bicmos.MininumResistance=10.0(10.0)
bicmos.GateLengthSubtraction=0.0(0.0)
bicmos.Gate Inclusion=false(false)
bicmos.Ground Net Inclusion=false(false)
bicmos.MaxSeriesResistance=10.0(10.0)
bicmos.LogicalEffort.GateCapacitance=0.4(0.4)
bicmos.LogicalEffort.WireRatio=0.16(0.16)
bicmos.LogicalEffort.DiffAlpha=0.7(0.7)
ResolutionValueForbicmos=0.0
TRANSPARENT_1=ff60d1ff
TRANSPARENT_2=ffff9bc0
TRANSPARENT_3=ff6be260
TRANSPARENT_4=ffe05fff
TRANSPARENT_5=fff0ddb5
Layer M1 METAL1
	bicmos.CIF.M1=CMF(CMF)
	bicmos.DXF.M1=()
	bicmos.Skill.M1=()
	bicmos.Resistance.M1=0.0(0.0)
	bicmos.Capacitance.M1=0.0(0.0)
	bicmos.EdgeCapacitance.M1=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=1(1)
	color=ff60d1ff(60d1ff)
	opacity=0.8(0.8)
	foreground=true
	pattern 2222 0 8888 0 2222 0 8888 0 2222 0 8888 0 2222 0 8888 0
	distance3D=11.0
	thickness3D=0.5
	mode3D=NONE
	factor3D=0.2
Layer M2 METAL2
	bicmos.CIF.M2=CMS(CMS)
	bicmos.DXF.M2=()
	bicmos.Skill.M2=()
	bicmos.Resistance.M2=0.0(0.0)
	bicmos.Capacitance.M2=0.0(0.0)
	bicmos.EdgeCapacitance.M2=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=4(4)
	color=ffe05fff(e05fff)
	opacity=0.8(0.8)
	foreground=true
	pattern 1010 2020 4040 8080 101 202 404 808 1010 2020 4040 8080 101 202 404 808
	distance3D=12.0
	thickness3D=0.5
	mode3D=NONE
	factor3D=0.2
Layer Poly1 POLY1
	bicmos.CIF.Poly1=CPG(CPG)
	bicmos.DXF.Poly1=()
	bicmos.Skill.Poly1=()
	bicmos.Resistance.Poly1=0.0(0.0)
	bicmos.Capacitance.Poly1=0.0(0.0)
	bicmos.EdgeCapacitance.Poly1=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=2(2)
	color=ffff9bc0(ff9bc0)
	opacity=0.8(0.8)
	foreground=true
	pattern 808 404 202 101 8080 4040 2020 1010 808 404 202 101 8080 4040 2020 1010
	distance3D=9.0
	thickness3D=0.5
	mode3D=NONE
	factor3D=0.2
Layer Poly2 POLY2
	bicmos.CIF.Poly2=CEL(CEL)
	bicmos.DXF.Poly2=()
	bicmos.Skill.Poly2=()
	bicmos.Resistance.Poly2=0.0(0.0)
	bicmos.Capacitance.Poly2=0.0(0.0)
	bicmos.EdgeCapacitance.Poly2=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=Solid(Solid)
	transparent=0(0)
	color=ffff00ff(ff00ff)
	opacity=0.8(0.8)
	foreground=true
	pattern e0e0 7070 3838 1c1c e0e 707 8383 c1c1 e0e0 7070 3838 1c1c e0e 707 8383 c1c1
	distance3D=10.0
	thickness3D=0.5
	mode3D=NONE
	factor3D=0.2
Layer Active DIFF
	bicmos.CIF.Active=CAA(CAA)
	bicmos.DXF.Active=()
	bicmos.Skill.Active=()
	bicmos.Resistance.Active=0.0(0.0)
	bicmos.Capacitance.Active=0.0(0.0)
	bicmos.EdgeCapacitance.Active=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=3(3)
	color=ff6be260(6be260)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 303 4848 303 0 3030 8484 3030 0 303 4848 303 0 3030 8484 3030
	distance3D=7.0
	thickness3D=2.0
	mode3D=NONE
	factor3D=0.2
Layer Poly1_Cut CONTACT1
	bicmos.CIF.Poly1_Cut=CCP(CCP)
	bicmos.DXF.Poly1_Cut=()
	bicmos.Skill.Poly1_Cut=()
	bicmos.Resistance.Poly1_Cut=0.0(0.0)
	bicmos.Capacitance.Poly1_Cut=0.0(0.0)
	bicmos.EdgeCapacitance.Poly1_Cut=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=9.5
	thickness3D=0.5
	mode3D=NONE
	factor3D=0.2
Layer Poly2_Cut CONTACT3
	bicmos.CIF.Poly2_Cut=CCE(CCE)
	bicmos.DXF.Poly2_Cut=()
	bicmos.Skill.Poly2_Cut=()
	bicmos.Resistance.Poly2_Cut=0.0(0.0)
	bicmos.Capacitance.Poly2_Cut=0.0(0.0)
	bicmos.EdgeCapacitance.Poly2_Cut=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=10.5
	thickness3D=0.5
	mode3D=NONE
	factor3D=0.2
Layer Active_Cut CONTACT1
	bicmos.CIF.Active_Cut=CCA(CCA)
	bicmos.DXF.Active_Cut=()
	bicmos.Skill.Active_Cut=()
	bicmos.Resistance.Active_Cut=0.0(0.0)
	bicmos.Capacitance.Active_Cut=0.0(0.0)
	bicmos.EdgeCapacitance.Active_Cut=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=9.0
	thickness3D=2.0
	mode3D=NONE
	factor3D=0.2
Layer Via CONTACT2
	bicmos.CIF.Via=CVA(CVA)
	bicmos.DXF.Via=()
	bicmos.Skill.Via=()
	bicmos.Resistance.Via=0.0(0.0)
	bicmos.Capacitance.Via=0.0(0.0)
	bicmos.EdgeCapacitance.Via=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=11.0
	thickness3D=0.5
	mode3D=NONE
	factor3D=0.2
Layer P_Select IMPLANTP
	bicmos.CIF.P_Select=CSP(CSP)
	bicmos.DXF.P_Select=()
	bicmos.Skill.P_Select=()
	bicmos.Resistance.P_Select=0.0(0.0)
	bicmos.Capacitance.P_Select=0.0(0.0)
	bicmos.EdgeCapacitance.P_Select=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=Solid(Solid)
	transparent=0(0)
	color=ffffff00(ffff00)
	opacity=0.8(0.8)
	foreground=true
	pattern 1010 2020 4040 8080 101 202 404 808 1010 2020 4040 8080 101 202 404 808
	distance3D=4.0
	thickness3D=5.0
	mode3D=SCREEN_DOOR
	factor3D=0.4
Layer N_Select IMPLANTN
	bicmos.CIF.N_Select=CSN(CSN)
	bicmos.DXF.N_Select=()
	bicmos.Skill.N_Select=()
	bicmos.Resistance.N_Select=0.0(0.0)
	bicmos.Capacitance.N_Select=0.0(0.0)
	bicmos.EdgeCapacitance.N_Select=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=Solid(Solid)
	transparent=0(0)
	color=ffafffaf(afffaf)
	opacity=0.8(0.8)
	foreground=true
	pattern 1010 2020 4040 8080 101 202 404 808 1010 2020 4040 8080 101 202 404 808
	distance3D=4.0
	thickness3D=5.0
	mode3D=SCREEN_DOOR
	factor3D=0.4
Layer N_Well WELLN
	bicmos.CIF.N_Well=CWN(CWN)
	bicmos.DXF.N_Well=()
	bicmos.Skill.N_Well=()
	bicmos.Resistance.N_Well=0.0(0.0)
	bicmos.Capacitance.N_Well=0.0(0.0)
	bicmos.EdgeCapacitance.N_Well=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=5(5)
	color=fff0ddb5(f0ddb5)
	opacity=0.8(0.8)
	foreground=true
	pattern 1000 20 0 0 1 200 0 0 1000 20 0 0 1 200 0 0
	distance3D=0.0
	thickness3D=9.0
	mode3D=NICEST
	factor3D=0.8
Layer Pad_Frame ART
	bicmos.CIF.Pad_Frame=XP(XP)
	bicmos.DXF.Pad_Frame=()
	bicmos.Skill.Pad_Frame=()
	bicmos.Resistance.Pad_Frame=0.0(0.0)
	bicmos.Capacitance.Pad_Frame=0.0(0.0)
	bicmos.EdgeCapacitance.Pad_Frame=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffff0000(ff0000)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=13.0
	thickness3D=1.0
	mode3D=NONE
	factor3D=0.2
Layer Transistor TRANSISTOR
	bicmos.CIF.Transistor=()
	bicmos.DXF.Transistor=()
	bicmos.Skill.Transistor=()
	bicmos.Resistance.Transistor=0.0(0.0)
	bicmos.Capacitance.Transistor=0.0(0.0)
	bicmos.EdgeCapacitance.Transistor=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffc8c8c8(c8c8c8)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer P_Base_Active DIFFP
	bicmos.CIF.P_Base_Active=CBA(CBA)
	bicmos.DXF.P_Base_Active=()
	bicmos.Skill.P_Base_Active=()
	bicmos.Resistance.P_Base_Active=0.0(0.0)
	bicmos.Capacitance.P_Base_Active=0.0(0.0)
	bicmos.EdgeCapacitance.P_Base_Active=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=Solid(Solid)
	transparent=3(3)
	color=ff6be260(6be260)
	opacity=0.8(0.8)
	foreground=true
	pattern 4444 2222 1111 8888 4444 2222 1111 888 4444 2222 1111 8888 4444 2222 1111 888
	distance3D=7.0
	thickness3D=2.0
	mode3D=NONE
	factor3D=0.2
Layer BCCD IMPLANTN
	bicmos.CIF.BCCD=CCD(CCD)
	bicmos.DXF.BCCD=()
	bicmos.Skill.BCCD=()
	bicmos.Resistance.BCCD=0.0(0.0)
	bicmos.Capacitance.BCCD=0.0(0.0)
	bicmos.EdgeCapacitance.BCCD=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=Solid(Solid)
	transparent=0(0)
	color=ffff9696(ff9696)
	opacity=0.8(0.8)
	foreground=true
	pattern 8888 0 2222 0 8888 0 2222 0 8888 0 2222 0 8888 0 2222 0
	distance3D=4.0
	thickness3D=5.0
	mode3D=SCREEN_DOOR
	factor3D=0.4
Layer Ohmic_Substrate SUBSTRATE
	bicmos.CIF.Ohmic_Substrate=CAA(CAA)
	bicmos.DXF.Ohmic_Substrate=()
	bicmos.Skill.Ohmic_Substrate=()
	bicmos.Resistance.Ohmic_Substrate=0.0(0.0)
	bicmos.Capacitance.Ohmic_Substrate=0.0(0.0)
	bicmos.EdgeCapacitance.Ohmic_Substrate=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=3(3)
	color=ff6be260(6be260)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=9.0
	mode3D=NICEST
	factor3D=0.8
Layer Ohmic_Well WELL
	bicmos.CIF.Ohmic_Well=CAA(CAA)
	bicmos.DXF.Ohmic_Well=()
	bicmos.Skill.Ohmic_Well=()
	bicmos.Resistance.Ohmic_Well=0.0(0.0)
	bicmos.Capacitance.Ohmic_Well=0.0(0.0)
	bicmos.EdgeCapacitance.Ohmic_Well=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=3(3)
	color=ff6be260(6be260)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
Layer Passivation OVERGLASS
	bicmos.CIF.Passivation=COG(COG)
	bicmos.DXF.Passivation=()
	bicmos.Skill.Passivation=()
	bicmos.Resistance.Passivation=0.0(0.0)
	bicmos.Capacitance.Passivation=0.0(0.0)
	bicmos.EdgeCapacitance.Passivation=0.0(0.0)
	patternedOnDisplay=true(true)
	patternedOnPrinter=true(true)
	outlined=None(None)
	transparent=0(0)
	color=ff646464(646464)
	opacity=0.8(0.8)
	foreground=true
	pattern 1c1c 3e3e 3636 3e3e 1c1c 0 0 0 1c1c 3e3e 3636 3e3e 1c1c 0 0 0
	distance3D=13.0
	thickness3D=1.0
	mode3D=NONE
	factor3D=0.2
ArcProto Metal_1 metal-1
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForMetal_1INbicmos=0.0
	baseExtend=1.5
	defaultLambdaBaseWidth=3.0
	diskOffset1=1.5
	diskOffset2=1.5
	DefaultAngleForMetal_1INbicmos=90
	DefaultRigidForMetal_1INbicmos=false
	DefaultFixedAngleForMetal_1INbicmos=true
	DefaultExtendedForMetal_1INbicmos=true
	DefaultDirectionalForMetal_1INbicmos=false
		arcLayer layer=M1 style=FILLED extend=1.5
ArcProto Metal_2 metal-2
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForMetal_2INbicmos=0.0
	baseExtend=1.5
	defaultLambdaBaseWidth=3.0
	diskOffset1=1.5
	diskOffset2=1.5
	DefaultAngleForMetal_2INbicmos=90
	DefaultRigidForMetal_2INbicmos=false
	DefaultFixedAngleForMetal_2INbicmos=true
	DefaultExtendedForMetal_2INbicmos=true
	DefaultDirectionalForMetal_2INbicmos=false
		arcLayer layer=M2 style=FILLED extend=1.5
ArcProto Polysilicon poly-1
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPolysiliconINbicmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=1.0
	diskOffset2=1.0
	DefaultAngleForPolysiliconINbicmos=90
	DefaultRigidForPolysiliconINbicmos=false
	DefaultFixedAngleForPolysiliconINbicmos=true
	DefaultExtendedForPolysiliconINbicmos=true
	DefaultDirectionalForPolysiliconINbicmos=false
		arcLayer layer=Poly1 style=FILLED extend=1.0
ArcProto Polysilicon_2 poly-2
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPolysilicon_2INbicmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=1.0
	diskOffset2=1.0
	DefaultAngleForPolysilicon_2INbicmos=90
	DefaultRigidForPolysilicon_2INbicmos=false
	DefaultFixedAngleForPolysilicon_2INbicmos=true
	DefaultExtendedForPolysilicon_2INbicmos=true
	DefaultDirectionalForPolysilicon_2INbicmos=false
		arcLayer layer=Poly2 style=FILLED extend=1.0
ArcProto Ndiff n-diffusion
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForNdiffINbicmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=3.0
	diskOffset2=1.0
	DefaultAngleForNdiffINbicmos=90
	DefaultRigidForNdiffINbicmos=false
	DefaultFixedAngleForNdiffINbicmos=true
	DefaultExtendedForNdiffINbicmos=true
	DefaultDirectionalForNdiffINbicmos=false
		arcLayer layer=Active style=FILLED extend=1.0
		arcLayer layer=N_Select style=FILLED extend=3.0
ArcProto Pdiff p-diffusion
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPdiffINbicmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=6.0
	diskOffset2=1.0
	DefaultAngleForPdiffINbicmos=90
	DefaultRigidForPdiffINbicmos=false
	DefaultFixedAngleForPdiffINbicmos=true
	DefaultExtendedForPdiffINbicmos=true
	DefaultDirectionalForPdiffINbicmos=false
		arcLayer layer=Active style=FILLED extend=1.0
		arcLayer layer=P_Select style=CLOSED extend=3.0
		arcLayer layer=N_Well style=FILLED extend=6.0
ArcProto Active diffusion
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForActiveINbicmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=1.0
	diskOffset2=1.0
	DefaultAngleForActiveINbicmos=90
	DefaultRigidForActiveINbicmos=false
	DefaultFixedAngleForActiveINbicmos=true
	DefaultExtendedForActiveINbicmos=true
	DefaultDirectionalForActiveINbicmos=false
		arcLayer layer=Active style=FILLED extend=1.0
PrimitiveNode M1_Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	baseRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	DefaultExtendXForM1_PinINbicmos=0.0
	DefaultExtendYForM1_PinINbicmos=0.0
	diskOffset1=1.5,1.5
	diskOffset2=1.5,1.5
	layers:
	layer=M1 port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal-1 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.5 rm=0.5 ra=-1.5 bm=-0.5 ba=1.5 tm=0.5 ta=-1.5
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode M2_Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	baseRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	DefaultExtendXForM2_PinINbicmos=0.0
	DefaultExtendYForM2_PinINbicmos=0.0
	diskOffset1=1.5,1.5
	diskOffset2=1.5,1.5
	layers:
	layer=M2 port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal-2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.5 rm=0.5 ra=-1.5 bm=-0.5 ba=1.5 tm=0.5 ta=-1.5
		isolated=false negatable=false
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Poly1_Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForPoly1_PinINbicmos=0.0
	DefaultExtendYForPoly1_PinINbicmos=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Poly1 port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port polysilicon angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Poly2_Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForPoly2_PinINbicmos=0.0
	DefaultExtendYForPoly2_PinINbicmos=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Poly2 port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port p2-pin angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Ndiff_Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForNdiff_PinINbicmos=0.0
	DefaultExtendYForNdiff_PinINbicmos=0.0
	diskOffset1=3.0,3.0
	diskOffset2=1.0,1.0
	layers:
	layer=Active port=0 style=CROSSED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	layer=N_Select port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port Ndiff_Pin angle=0 range=180 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=-0.5 ba=3.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Ndiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Pdiff_Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[5.0,5.0] Y:[5.0,5.0]}
	fullRectangle=ERectangle[x=-6.0,y=-6.0,w=12.0,h=12.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForPdiff_PinINbicmos=0.0
	DefaultExtendYForPdiff_PinINbicmos=0.0
	diskOffset1=6.0,6.0
	diskOffset2=1.0,1.0
	layers:
	layer=Active port=0 style=CROSSED repr=1
		point xm=-0.5 xa=5.0 ym=-0.5 ya=5.0
		point xm=0.5 xa=-5.0 ym=0.5 ya=-5.0
	layer=P_Select port=0 style=CROSSED repr=1
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	layer=N_Well port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port Pdiff_Pin angle=0 range=180 topology=0 unknown
		lm=-0.5 la=6.0 rm=0.5 ra=-6.0 bm=-0.5 ba=6.0 tm=0.5 ta=-6.0
		isolated=false negatable=false
		portArc Pdiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Active_Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForActive_PinINbicmos=0.0
	DefaultExtendYForActive_PinINbicmos=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Active port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port active angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Active
		portArc Pdiff
		portArc Ndiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode M1_Poly1_Con contact
	specialType=0 numMultiCuts=1
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForM1_Poly1_ConINbicmos=0.0
	DefaultExtendYForM1_Poly1_ConINbicmos=0.0
	diskOffset1=3.0,3.0
	diskOffset2=3.0,3.0
	layers:
	layer=M1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=1.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=-1.0
	layer=Poly1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Poly1_Cut port=0 style=FILLED repr=3
		multiSizeX=2.0 multiSizeY=2.0 multiSep=2.0 multiSpe2D=2.0
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	port metal-1-polysilicon angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode M1_Poly2_Con contact
	specialType=0 numMultiCuts=1
	SizeOffset {X:[1.0,1.0] Y:[1.0,1.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForM1_Poly2_ConINbicmos=0.0
	DefaultExtendYForM1_Poly2_ConINbicmos=0.0
	diskOffset1=3.0,3.0
	diskOffset2=2.0,2.0
	layers:
	layer=M1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=1.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=-1.0
	layer=Poly2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Poly2_Cut port=0 style=FILLED repr=3
		multiSizeX=2.0 multiSizeY=2.0 multiSep=2.0 multiSpe2D=2.0
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	port M1P2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Polysilicon_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode M1_Pdiff_Con contact
	specialType=0 numMultiCuts=1
	SizeOffset {X:[5.0,5.0] Y:[5.0,5.0]}
	fullRectangle=ERectangle[x=-8.0,y=-8.0,w=16.0,h=16.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForM1_Pdiff_ConINbicmos=0.0
	DefaultExtendYForM1_Pdiff_ConINbicmos=0.0
	diskOffset1=8.0,8.0
	diskOffset2=3.0,3.0
	layers:
	layer=M1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=6.0 ym=-0.5 ya=6.0
		point xm=0.5 xa=-6.0 ym=0.5 ya=-6.0
	layer=Active port=0 style=FILLED repr=1
		point xm=-0.5 xa=5.0 ym=-0.5 ya=5.0
		point xm=0.5 xa=-5.0 ym=0.5 ya=-5.0
	layer=Active_Cut port=0 style=FILLED repr=3
		multiSizeX=2.0 multiSizeY=2.0 multiSep=2.0 multiSpe2D=2.0
		point xm=-0.5 xa=8.0 ym=-0.5 ya=8.0
		point xm=0.5 xa=-8.0 ym=0.5 ya=-8.0
	layer=P_Select port=0 style=CLOSED repr=1
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	layer=N_Well port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port m1_pdiff angle=0 range=180 topology=0 unknown
		lm=-0.5 la=6.0 rm=0.5 ra=-6.0 bm=-0.5 ba=6.0 tm=0.5 ta=-6.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Pdiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode M1_Ndiff_Con contact
	specialType=0 numMultiCuts=1
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForM1_Ndiff_ConINbicmos=0.0
	DefaultExtendYForM1_Ndiff_ConINbicmos=0.0
	diskOffset1=5.0,5.0
	diskOffset2=3.0,3.0
	layers:
	layer=M1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	layer=Active port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	layer=Active_Cut port=0 style=FILLED repr=3
		multiSizeX=2.0 multiSizeY=2.0 multiSep=2.0 multiSpe2D=2.0
		point xm=-0.5 xa=5.0 ym=-0.5 ya=5.0
		point xm=0.5 xa=-5.0 ym=0.5 ya=-5.0
	layer=N_Select port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port M1_Ndiff angle=0 range=180 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=-0.5 ba=3.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Ndiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode M1_M2_Con contact
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForM1_M2_ConINbicmos=0.0
	DefaultExtendYForM1_M2_ConINbicmos=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=M1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=M2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Via port=0 style=CLOSED repr=1
		point xm=0.0 xa=-1.0 ym=0.0 ya=-1.0
		point xm=0.0 xa=1.0 ym=0.0 ya=1.0
	port metal-1-metal-2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.5 rm=0.5 ra=-1.5 bm=-0.5 ba=1.5 tm=0.5 ta=-1.5
		isolated=false negatable=false
		portArc Metal_1
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode PMOSFET pMOS-transistor NODESHRINK HOLDSTRACE
	specialType=1 numMultiCuts=0 5.0 0.0 1.0 2.0 0.0 1.0
	SizeOffset {X:[5.0,5.0] Y:[7.0,7.0]}
	fullRectangle=ERectangle[x=-6.0,y=-8.0,w=12.0,h=16.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForPMOSFETINbicmos=0.0
	DefaultExtendYForPMOSFETINbicmos=0.0
	diskOffset1=6.0,8.0
	diskOffset2=1.0,1.0
	layers:
	layer=Poly1 port=0 style=FILLED repr=1
		LWidth=1.0 rWidth=1.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=3.0 ym=-0.5 ya=7.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-7.0
	layer=Active port=0 style=FILLED repr=1
		LWidth=3.0 rWidth=3.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=5.0 ym=-0.5 ya=5.0
		point xm=0.5 xa=-5.0 ym=0.5 ya=-5.0
	layer=P_Select port=-1 style=FILLED repr=1
		LWidth=5.0 rWidth=5.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	layer=N_Well port=-1 style=FILLED repr=1
		LWidth=8.0 rWidth=8.0 bExtend=5.0 tExtend=5.0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	electricalLayers:
	layer=Poly1 port=0 style=FILLED repr=1
		LWidth=1.0 rWidth=1.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=3.0 ym=-0.5 ya=7.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-7.0
	layer=P_Select port=-1 style=FILLED repr=1
		LWidth=5.0 rWidth=5.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	layer=N_Well port=-1 style=FILLED repr=1
		LWidth=8.0 rWidth=8.0 bExtend=5.0 tExtend=5.0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Active port=3 style=FILLED repr=1
		LWidth=3.0 rWidth=0.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=5.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-5.0 ym=0.5 ya=-5.0
	layer=Active port=1 style=FILLED repr=1
		LWidth=0.0 rWidth=3.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=5.0 ym=-0.5 ya=5.0
		point xm=0.5 xa=-5.0 ym=0.0 ya=0.0
	port pmos_poly_lt angle=180 range=90 topology=0 unknown
		lm=-0.5 la=3.0 rm=-0.5 ra=4.0 bm=0.0 ba=-1.0 tm=0.0 ta=1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port pmos_diff_top angle=90 range=90 topology=1 unknown
		lm=0.0 la=-1.0 rm=0.0 ra=1.0 bm=0.5 ba=-6.0 tm=0.5 ta=-5.0
		isolated=false negatable=false
		portArc Pdiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port pmos_poly_rt angle=0 range=90 topology=0 unknown
		lm=0.5 la=-4.0 rm=0.5 ra=-3.0 bm=0.0 ba=-1.0 tm=0.0 ta=1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port pmos_diff_bot angle=270 range=90 topology=3 unknown
		lm=0.0 la=-1.0 rm=0.0 ra=1.0 bm=-0.5 ba=5.0 tm=-0.5 ta=6.0
		isolated=false negatable=false
		portArc Pdiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode NMOSFET nMOS-transistor NODESHRINK HOLDSTRACE
	specialType=1 numMultiCuts=0 4.0 0.0 1.0 2.0 0.0 1.0
	SizeOffset {X:[2.0,2.0] Y:[4.0,4.0]}
	fullRectangle=ERectangle[x=-3.0,y=-5.0,w=6.0,h=10.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForNMOSFETINbicmos=0.0
	DefaultExtendYForNMOSFETINbicmos=0.0
	diskOffset1=3.0,5.0
	diskOffset2=1.0,1.0
	layers:
	layer=Poly1 port=0 style=FILLED repr=1
		LWidth=1.0 rWidth=1.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=4.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-4.0
	layer=Active port=0 style=FILLED repr=1
		LWidth=3.0 rWidth=3.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	layer=N_Select port=-1 style=FILLED repr=1
		LWidth=5.0 rWidth=5.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	electricalLayers:
	layer=Poly1 port=0 style=FILLED repr=1
		LWidth=1.0 rWidth=1.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=4.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-4.0
	layer=N_Select port=-1 style=FILLED repr=1
		LWidth=5.0 rWidth=5.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Active port=3 style=FILLED repr=1
		LWidth=3.0 rWidth=0.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=2.0 ym=0.0 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	layer=Active port=1 style=FILLED repr=1
		LWidth=0.0 rWidth=3.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.0 ya=0.0
	port nmos_poly_lt angle=180 range=90 topology=0 unknown
		lm=-0.5 la=0.0 rm=-0.5 ra=1.0 bm=0.0 ba=-1.0 tm=0.0 ta=1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port nmos_diff_top angle=90 range=90 topology=1 unknown
		lm=0.0 la=-1.0 rm=0.0 ra=1.0 bm=0.5 ba=-3.0 tm=0.5 ta=-2.0
		isolated=false negatable=false
		portArc Ndiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port nmos_poly_rt angle=0 range=90 topology=0 unknown
		lm=0.5 la=-1.0 rm=0.5 ra=0.0 bm=0.0 ba=-1.0 tm=0.0 ta=1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port nmos_diff_bot angle=270 range=90 topology=3 unknown
		lm=0.0 la=-1.0 rm=0.0 ra=1.0 bm=-0.5 ba=2.0 tm=-0.5 ta=3.0
		isolated=false negatable=false
		portArc Ndiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode NPN1_transistor NPN-transistor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[22.0,16.0] Y:[8.0,8.0]}
	fullRectangle=ERectangle[x=-23.0,y=-12.0,w=46.0,h=24.0]
	baseRectangle=ERectangle[x=-1.0,y=-4.0,w=8.0,h=8.0]
	DefaultExtendXForNPN1_transistorINbicmos=0.0
	DefaultExtendYForNPN1_transistorINbicmos=0.0
	diskOffset1=23.0,12.0
	diskOffset2=4.0,4.0
	layers:
	layer=M1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=35.0 ym=-0.5 ya=10.0
		point xm=0.5 xa=-7.0 ym=0.5 ya=-10.0
	layer=M1 port=1 style=FILLED repr=1
		point xm=-0.5 xa=13.0 ym=-0.5 ya=10.0
		point xm=0.5 xa=-29.0 ym=0.5 ya=-10.0
	layer=M1 port=2 style=FILLED repr=1
		point xm=-0.5 xa=24.0 ym=-0.5 ya=10.0
		point xm=0.5 xa=-18.0 ym=0.5 ya=-10.0
	layer=M1 port=3 style=FILLED repr=1
		point xm=-0.5 xa=3.0 ym=-0.5 ya=10.0
		point xm=0.5 xa=-39.0 ym=0.5 ya=-10.0
	layer=Active port=0 style=FILLED repr=1
		point xm=-0.5 xa=34.0 ym=-0.5 ya=9.0
		point xm=0.5 xa=-6.0 ym=0.5 ya=-9.0
	layer=Active port=2 style=FILLED repr=1
		point xm=-0.5 xa=22.0 ym=-0.5 ya=8.0
		point xm=0.5 xa=-16.0 ym=0.5 ya=-8.0
	layer=Active port=1 style=FILLED repr=1
		point xm=-0.5 xa=12.0 ym=-0.5 ya=9.0
		point xm=0.5 xa=-28.0 ym=0.5 ya=-9.0
	layer=Active port=3 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=9.0
		point xm=0.5 xa=-38.0 ym=0.5 ya=-9.0
	layer=Active_Cut port=0 style=FILLED repr=1
		point xm=-0.5 xa=36.0 ym=-0.5 ya=11.0
		point xm=0.5 xa=-8.0 ym=0.5 ya=-11.0
	layer=Active_Cut port=3 style=FILLED repr=1
		point xm=-0.5 xa=4.0 ym=-0.5 ya=11.0
		point xm=0.5 xa=-40.0 ym=0.5 ya=-11.0
	layer=Active_Cut port=1 style=FILLED repr=1
		point xm=-0.5 xa=14.0 ym=-0.5 ya=11.0
		point xm=0.5 xa=-30.0 ym=0.5 ya=-11.0
	layer=Active_Cut port=2 style=FILLED repr=1
		point xm=-0.5 xa=25.0 ym=-0.5 ya=11.0
		point xm=0.5 xa=-19.0 ym=0.5 ya=-11.0
	layer=P_Select port=0 style=FILLED repr=1
		point xm=-0.5 xa=34.0 ym=-0.5 ya=9.0
		point xm=0.5 xa=-6.0 ym=0.5 ya=-9.0
	layer=P_Select port=1 style=FILLED repr=1
		point xm=-0.5 xa=12.0 ym=-0.5 ya=9.0
		point xm=0.5 xa=-28.0 ym=0.5 ya=-9.0
	layer=N_Select port=2 style=FILLED repr=1
		point xm=-0.5 xa=22.0 ym=-0.5 ya=8.0
		point xm=0.5 xa=-16.0 ym=0.5 ya=-8.0
	layer=N_Select port=3 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=7.0
		point xm=0.5 xa=-36.0 ym=0.5 ya=-7.0
	layer=N_Well port=-1 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=P_Base_Active port=-1 style=FILLED repr=1
		point xm=-0.5 xa=12.0 ym=-0.5 ya=6.0
		point xm=0.5 xa=-6.0 ym=0.5 ya=-6.0
	port B1 angle=0 range=180 topology=1 unknown
		lm=-0.5 la=14.0 rm=0.5 ra=-30.0 bm=-0.5 ba=11.0 tm=0.5 ta=-11.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port B2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=36.0 rm=0.5 ra=-8.0 bm=-0.5 ba=11.0 tm=0.5 ta=-11.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port C1 angle=0 range=180 topology=3 unknown
		lm=-0.5 la=4.0 rm=0.5 ra=-40.0 bm=-0.5 ba=11.0 tm=0.5 ta=-11.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port E1 angle=0 range=180 topology=2 unknown
		lm=-0.5 la=25.0 rm=0.5 ra=-19.0 bm=-0.5 ba=11.0 tm=0.5 ta=-11.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode NPN2_Transistor NPN-transistor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-23.0,y=-18.0,w=46.0,h=36.0]
	baseRectangle=ERectangle[x=-23.0,y=-18.0,w=46.0,h=36.0]
	DefaultExtendXForNPN2_TransistorINbicmos=0.0
	DefaultExtendYForNPN2_TransistorINbicmos=0.0
	diskOffset1=23.0,18.0
	diskOffset2=23.0,18.0
	layers:
	layer=M1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=13.0 ym=-0.5 ya=10.0
		point xm=0.5 xa=-29.0 ym=0.5 ya=-22.0
	layer=M1 port=6 style=FILLED repr=1
		point xm=-0.5 xa=35.0 ym=-0.5 ya=22.0
		point xm=0.5 xa=-7.0 ym=0.5 ya=-10.0
	layer=M1 port=1 style=FILLED repr=1
		point xm=-0.5 xa=24.0 ym=-0.5 ya=22.0
		point xm=0.5 xa=-18.0 ym=0.5 ya=-10.0
	layer=M1 port=3 style=FILLED repr=1
		point xm=-0.5 xa=3.0 ym=-0.5 ya=10.0
		point xm=0.5 xa=-39.0 ym=0.5 ya=-22.0
	layer=M1 port=2 style=FILLED repr=1
		point xm=-0.5 xa=13.0 ym=-0.5 ya=22.0
		point xm=0.5 xa=-29.0 ym=0.5 ya=-10.0
	layer=M1 port=5 style=FILLED repr=1
		point xm=-0.5 xa=24.0 ym=-0.5 ya=10.0
		point xm=0.5 xa=-18.0 ym=0.5 ya=-22.0
	layer=M1 port=7 style=FILLED repr=1
		point xm=-0.5 xa=35.0 ym=-0.5 ya=10.0
		point xm=0.5 xa=-7.0 ym=0.5 ya=-22.0
	layer=M1 port=4 style=FILLED repr=1
		point xm=-0.5 xa=3.0 ym=-0.5 ya=22.0
		point xm=0.5 xa=-39.0 ym=0.5 ya=-10.0
	layer=Active port=0 style=FILLED repr=1
		point xm=-0.5 xa=12.0 ym=-0.5 ya=9.0
		point xm=0.5 xa=-28.0 ym=0.5 ya=-21.0
	layer=Active port=6 style=FILLED repr=1
		point xm=-0.5 xa=34.0 ym=-0.5 ya=21.0
		point xm=0.5 xa=-6.0 ym=0.5 ya=-9.0
	layer=Active port=1 style=FILLED repr=1
		point xm=-0.5 xa=22.0 ym=-0.5 ya=20.0
		point xm=0.5 xa=-16.0 ym=0.5 ya=-8.0
	layer=Active port=2 style=FILLED repr=1
		point xm=-0.5 xa=12.0 ym=-0.5 ya=21.0
		point xm=0.5 xa=-28.0 ym=0.5 ya=-9.0
	layer=Active port=4 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=21.0
		point xm=0.5 xa=-38.0 ym=0.5 ya=-9.0
	layer=Active port=7 style=FILLED repr=1
		point xm=-0.5 xa=34.0 ym=-0.5 ya=9.0
		point xm=0.5 xa=-6.0 ym=0.5 ya=-21.0
	layer=Active port=5 style=FILLED repr=1
		point xm=-0.5 xa=22.0 ym=-0.5 ya=8.0
		point xm=0.5 xa=-16.0 ym=0.5 ya=-20.0
	layer=Active port=3 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=9.0
		point xm=0.5 xa=-38.0 ym=0.5 ya=-21.0
	layer=Active_Cut port=0 style=FILLED repr=1
		point xm=-0.5 xa=14.0 ym=-0.5 ya=11.0
		point xm=0.5 xa=-30.0 ym=0.5 ya=-23.0
	layer=Active_Cut port=2 style=FILLED repr=1
		point xm=-0.5 xa=14.0 ym=-0.5 ya=23.0
		point xm=0.5 xa=-30.0 ym=0.5 ya=-11.0
	layer=Active_Cut port=5 style=FILLED repr=1
		point xm=-0.5 xa=25.0 ym=-0.5 ya=11.0
		point xm=0.5 xa=-19.0 ym=0.5 ya=-23.0
	layer=Active_Cut port=6 style=FILLED repr=1
		point xm=-0.5 xa=36.0 ym=-0.5 ya=23.0
		point xm=0.5 xa=-8.0 ym=0.5 ya=-11.0
	layer=Active_Cut port=1 style=FILLED repr=1
		point xm=-0.5 xa=25.0 ym=-0.5 ya=23.0
		point xm=0.5 xa=-19.0 ym=0.5 ya=-11.0
	layer=Active_Cut port=7 style=FILLED repr=1
		point xm=-0.5 xa=36.0 ym=-0.5 ya=11.0
		point xm=0.5 xa=-8.0 ym=0.5 ya=-23.0
	layer=Active_Cut port=3 style=FILLED repr=1
		point xm=-0.5 xa=4.0 ym=-0.5 ya=11.0
		point xm=0.5 xa=-40.0 ym=0.5 ya=-23.0
	layer=Active_Cut port=4 style=FILLED repr=1
		point xm=-0.5 xa=4.0 ym=-0.5 ya=23.0
		point xm=0.5 xa=-40.0 ym=0.5 ya=-11.0
	layer=P_Select port=0 style=FILLED repr=1
		point xm=-0.5 xa=12.0 ym=-0.5 ya=9.0
		point xm=0.5 xa=-28.0 ym=0.5 ya=-21.0
	layer=P_Select port=6 style=FILLED repr=1
		point xm=-0.5 xa=34.0 ym=-0.5 ya=21.0
		point xm=0.5 xa=-6.0 ym=0.5 ya=-9.0
	layer=P_Select port=7 style=FILLED repr=1
		point xm=-0.5 xa=34.0 ym=-0.5 ya=9.0
		point xm=0.5 xa=-6.0 ym=0.5 ya=-21.0
	layer=P_Select port=2 style=FILLED repr=1
		point xm=-0.5 xa=12.0 ym=-0.5 ya=21.0
		point xm=0.5 xa=-28.0 ym=0.5 ya=-9.0
	layer=N_Select port=4 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=19.0
		point xm=0.5 xa=-36.0 ym=0.5 ya=-7.0
	layer=N_Select port=3 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=7.0
		point xm=0.5 xa=-36.0 ym=0.5 ya=-19.0
	layer=N_Select port=1 style=FILLED repr=1
		point xm=-0.5 xa=22.0 ym=-0.5 ya=20.0
		point xm=0.5 xa=-16.0 ym=0.5 ya=-8.0
	layer=N_Select port=5 style=FILLED repr=1
		point xm=-0.5 xa=22.0 ym=-0.5 ya=8.0
		point xm=0.5 xa=-16.0 ym=0.5 ya=-20.0
	layer=N_Well port=-1 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=P_Base_Active port=-1 style=FILLED repr=1
		point xm=-0.5 xa=12.0 ym=-0.5 ya=6.0
		point xm=0.5 xa=-6.0 ym=0.5 ya=-6.0
	port B1 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=14.0 rm=0.5 ra=-30.0 bm=-0.5 ba=11.0 tm=0.5 ta=-23.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port B2 angle=0 range=180 topology=7 unknown
		lm=-0.5 la=36.0 rm=0.5 ra=-8.0 bm=-0.5 ba=11.0 tm=0.5 ta=-23.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port B3 angle=0 range=180 topology=2 unknown
		lm=-0.5 la=14.0 rm=0.5 ra=-30.0 bm=-0.5 ba=23.0 tm=0.5 ta=-11.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port B4 angle=0 range=180 topology=6 unknown
		lm=-0.5 la=36.0 rm=0.5 ra=-8.0 bm=-0.5 ba=23.0 tm=0.5 ta=-11.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port C1 angle=0 range=180 topology=3 unknown
		lm=-0.5 la=4.0 rm=0.5 ra=-40.0 bm=-0.5 ba=11.0 tm=0.5 ta=-23.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port C2 angle=0 range=180 topology=4 unknown
		lm=-0.5 la=4.0 rm=0.5 ra=-40.0 bm=-0.5 ba=23.0 tm=0.5 ta=-11.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port E1 angle=0 range=180 topology=5 unknown
		lm=-0.5 la=25.0 rm=0.5 ra=-19.0 bm=-0.5 ba=11.0 tm=0.5 ta=-23.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port E2 angle=0 range=180 topology=1 unknown
		lm=-0.5 la=25.0 rm=0.5 ra=-19.0 bm=-0.5 ba=23.0 tm=0.5 ta=-11.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode M1_N_Well_Con well
	specialType=0 numMultiCuts=1
	SizeOffset {X:[3.0,3.0] Y:[3.0,3.0]}
	fullRectangle=ERectangle[x=-6.0,y=-6.0,w=12.0,h=12.0]
	baseRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	DefaultExtendXForM1_N_Well_ConINbicmos=0.0
	DefaultExtendYForM1_N_Well_ConINbicmos=0.0
	diskOffset1=6.0,6.0
	diskOffset2=3.0,3.0
	layers:
	layer=M1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=4.0 ym=-0.5 ya=4.0
		point xm=0.5 xa=-4.0 ym=0.5 ya=-4.0
	layer=Active_Cut port=0 style=FILLED repr=3
		multiSizeX=2.0 multiSizeY=2.0 multiSep=2.0 multiSpe2D=2.0
		point xm=-0.5 xa=6.0 ym=-0.5 ya=6.0
		point xm=0.5 xa=-6.0 ym=0.5 ya=-6.0
	layer=N_Select port=0 style=FILLED repr=1
		point xm=-0.5 xa=1.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=-1.0
	layer=N_Well port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Ohmic_Well port=0 style=FILLED repr=1
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	port metal-1-well angle=0 range=180 topology=0 unknown
		lm=-0.5 la=4.0 rm=0.5 ra=-4.0 bm=-0.5 ba=4.0 tm=0.5 ta=-4.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Active
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Poly1_Poly2_Cap capacitor
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-6.0,y=-6.0,w=12.0,h=12.0]
	baseRectangle=ERectangle[x=-6.0,y=-6.0,w=12.0,h=12.0]
	DefaultExtendXForPoly1_Poly2_CapINbicmos=0.0
	DefaultExtendYForPoly1_Poly2_CapINbicmos=0.0
	diskOffset1=6.0,6.0
	diskOffset2=6.0,6.0
	layers:
	layer=Poly1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Poly2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	port P1P2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=-0.5 ba=3.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Polysilicon_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port P1P2alt angle=0 range=180 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=-0.5 ba=3.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Polysilicon_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode M1_Substrate_Con unknown
	specialType=0 numMultiCuts=1
	SizeOffset {X:[3.0,3.0] Y:[3.0,3.0]}
	fullRectangle=ERectangle[x=-5.0,y=-5.0,w=10.0,h=10.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForM1_Substrate_ConINbicmos=0.0
	DefaultExtendYForM1_Substrate_ConINbicmos=0.0
	diskOffset1=5.0,5.0
	diskOffset2=2.0,2.0
	layers:
	layer=M1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=3.0 ym=-0.5 ya=3.0
		point xm=0.5 xa=-3.0 ym=0.5 ya=-3.0
	layer=Active_Cut port=0 style=FILLED repr=3
		multiSizeX=2.0 multiSizeY=2.0 multiSep=2.0 multiSpe2D=2.0
		point xm=-0.5 xa=5.0 ym=-0.5 ya=5.0
		point xm=0.5 xa=-5.0 ym=0.5 ya=-5.0
	layer=P_Select port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Ohmic_Substrate port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	port M1_Substrate angle=0 range=180 topology=0 unknown
		lm=-0.5 la=4.0 rm=0.5 ra=-4.0 bm=-0.5 ba=4.0 tm=0.5 ta=-4.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Ndiff_Node unknown
	specialType=0 numMultiCuts=0
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-4.0,y=-4.0,w=8.0,h=8.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForNdiff_NodeINbicmos=0.0
	DefaultExtendYForNdiff_NodeINbicmos=0.0
	diskOffset1=4.0,4.0
	diskOffset2=2.0,2.0
	layers:
	layer=Active port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	layer=N_Select port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port active angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Active
		portArc Pdiff
		portArc Ndiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Pdiff_Node unknown
	specialType=0 numMultiCuts=0
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-4.0,y=-4.0,w=8.0,h=8.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForPdiff_NodeINbicmos=0.0
	DefaultExtendYForPdiff_NodeINbicmos=0.0
	diskOffset1=4.0,4.0
	diskOffset2=2.0,2.0
	layers:
	layer=Active port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	layer=P_Select port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port Pdiff angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode M1_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForM1_NodeINbicmos=2.0
	DefaultExtendYForM1_NodeINbicmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=M1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal-1 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Metal_1
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode M2_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForM2_NodeINbicmos=2.0
	DefaultExtendYForM2_NodeINbicmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=M2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal-2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Metal_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Poly1_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPoly1_NodeINbicmos=2.0
	DefaultExtendYForPoly1_NodeINbicmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Poly1 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port polysilicon angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Poly2_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPoly2_NodeINbicmos=1.0
	DefaultExtendYForPoly2_NodeINbicmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Poly2 port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port P2 angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Polysilicon_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Active_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForActive_NodeINbicmos=2.0
	DefaultExtendYForActive_NodeINbicmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Active port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port active angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Active
		portArc Pdiff
		portArc Ndiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Poly1_Cut_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPoly1_Cut_NodeINbicmos=1.0
	DefaultExtendYForPoly1_Cut_NodeINbicmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Poly1_Cut port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port polycut angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Poly_2_Cut_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPoly_2_Cut_NodeINbicmos=2.0
	DefaultExtendYForPoly_2_Cut_NodeINbicmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Poly2_Cut port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port Poly_2_Cut angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Polysilicon_2
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Active_Cut_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForActive_Cut_NodeINbicmos=1.0
	DefaultExtendYForActive_Cut_NodeINbicmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Active_Cut port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port activecut angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Via_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForVia_NodeINbicmos=1.0
	DefaultExtendYForVia_NodeINbicmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Via port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port via angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode P_Select_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForP_Select_NodeINbicmos=3.0
	DefaultExtendYForP_Select_NodeINbicmos=3.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=P_Select port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port select angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode N_Select_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForN_Select_NodeINbicmos=2.0
	DefaultExtendYForN_Select_NodeINbicmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=N_Select port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port N_Select angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode N_Well_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForN_Well_NodeINbicmos=3.0
	DefaultExtendYForN_Well_NodeINbicmos=3.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=N_Well port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port well angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Pdiff
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Pad_Frame_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPad_Frame_NodeINbicmos=4.0
	DefaultExtendYForPad_Frame_NodeINbicmos=4.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Pad_Frame port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port pad-frame angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode P_Base_Active_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForP_Base_Active_NodeINbicmos=2.0
	DefaultExtendYForP_Base_Active_NodeINbicmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=P_Base_Active port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port P_Base angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode BCCD_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForBCCD_NodeINbicmos=2.0
	DefaultExtendYForBCCD_NodeINbicmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=BCCD port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port BCCD angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Ohmic_Substrate pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForOhmic_SubstrateINbicmos=2.0
	DefaultExtendYForOhmic_SubstrateINbicmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Ohmic_Substrate port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port Ohmic_Substrate angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Ohmic_Well pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForOhmic_WellINbicmos=2.0
	DefaultExtendYForOhmic_WellINbicmos=2.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Ohmic_Well port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port Ohmic_Well angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Passivation_Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPassivation_NodeINbicmos=4.0
	DefaultExtendYForPassivation_NodeINbicmos=4.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Passivation port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port passivation angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
Foundry MOSIS
	bicmos.GDS.MOSIS.M1=10(10)
	bicmos.GDS.MOSIS.M2=12(12)
	bicmos.GDS.MOSIS.Poly1=4(4)
	bicmos.GDS.MOSIS.Poly2=19(19)
	bicmos.GDS.MOSIS.Active=31(31)
	bicmos.GDS.MOSIS.Poly1_Cut=45(45)
	bicmos.GDS.MOSIS.Poly2_Cut=55(55)
	bicmos.GDS.MOSIS.Active_Cut=35(35)
	bicmos.GDS.MOSIS.Via=()
	bicmos.GDS.MOSIS.P_Select=8(8)
	bicmos.GDS.MOSIS.N_Select=7(7)
	bicmos.GDS.MOSIS.N_Well=1(1)
	bicmos.GDS.MOSIS.Pad_Frame=9(9)
	bicmos.GDS.MOSIS.Transistor=()
	bicmos.GDS.MOSIS.P_Base_Active=33(33)
	bicmos.GDS.MOSIS.BCCD=17(17)
	bicmos.GDS.MOSIS.Ohmic_Substrate=3(3)
	bicmos.GDS.MOSIS.Ohmic_Well=3(3)
	bicmos.GDS.MOSIS.Passivation=13(13)
 menu 0 0 arc Polysilicon
 menu 0 1 nodeInst Poly1_Pin:pin:
 menu 0 2 node M1_Poly1_Con
 menu 1 0 arc Polysilicon_2
 menu 1 1 nodeInst Poly2_Pin:pin:
 menu 1 2 node M1_Poly2_Con
 menu 2 0 arc Metal_1
 menu 2 1 nodeInst M1_Pin:pin:
 menu 3 0 arc Metal_2
 menu 3 1 nodeInst M2_Pin:pin:
 menu 3 2 node M1_M2_Con
 menu 4 0 arc Pdiff
 menu 4 1 nodeInst Pdiff_Pin:pin:
 menu 4 2 node M1_Pdiff_Con
 menu 5 0 arc Ndiff
 menu 5 1 nodeInst Ndiff_Pin:pin:
 menu 5 2 node M1_Ndiff_Con
 menu 6 0 arc Active
 menu 6 1 nodeInst Active_Pin:pin:
 menu 6 2 node M1_N_Well_Con
 menu 7 0 node M1_Substrate_Con
 menu 7 1 node NPN2_Transistor
 menu 7 2 node NPN1_transistor
 menu 8 0 node Poly1_Poly2_Cap
 menu 8 1 node NMOSFET
 menu 8 2 node PMOSFET
 menu 9 0 Pure
 menu 9 1 Misc.
 menu 9 2 Cell
    <Foundry name="MOSIS">
        <layerGds layer="M1" gds="10"/>
        <layerGds layer="M2" gds="12"/>
        <layerGds layer="Poly1" gds="4"/>
        <layerGds layer="Poly2" gds="19"/>
        <layerGds layer="Active" gds="31"/>
        <layerGds layer="Poly1_Cut" gds="45"/>
        <layerGds layer="Poly2_Cut" gds="55"/>
        <layerGds layer="Active_Cut" gds="35"/>
        <layerGds layer="P_Select" gds="8"/>
        <layerGds layer="N_Select" gds="7"/>
        <layerGds layer="N_Well" gds="1"/>
        <layerGds layer="Pad_Frame" gds="9"/>
        <layerGds layer="P_Base_Active" gds="33"/>
        <layerGds layer="BCCD" gds="17"/>
        <layerGds layer="Ohmic_Substrate" gds="3"/>
        <layerGds layer="Ohmic_Well" gds="3"/>
        <layerGds layer="Passivation" gds="13"/>
        <LayerRule ruleName="W_7" layerName="Active_Cut" type="MINWID" when="ALL" value="2.0"/>
        <LayerRule ruleName="W_13" layerName="Poly1_Cut" type="MINWID" when="ALL" value="2.0"/>
        <LayerRule ruleName="W_14" layerName="Poly2_Cut" type="MINWID" when="ALL" value="2.0"/>
        <LayersRule ruleName="C_3_3" layerNames="{Via,Via}" type="CONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="U_3_3" layerNames="{Via,Via}" type="UCONSPA" when="ALL" value="3.0"/>
        <LayersRule ruleName="U_3_6" layerNames="{Via,Transistor}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="C_3_7" layerNames="{Via,Active_Cut}" type="CONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="U_3_10" layerNames="{Via,Poly1}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="U_3_12" layerNames="{Via,Active}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="C_3_13" layerNames="{Via,Poly1_Cut}" type="CONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="C_7_7" layerNames="{Active_Cut,Active_Cut}" type="CONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="U_7_12" layerNames="{Active_Cut,Active}" type="UCONSPA" when="ALL" value="5.0"/>
        <LayersRule ruleName="U_8_8" layerNames="{M1,M1}" type="UCONSPA" when="ALL" value="3.0"/>
        <LayersRule ruleName="U_9_9" layerNames="{M2,M2}" type="UCONSPA" when="ALL" value="4.0"/>
        <LayersRule ruleName="U_10_10" layerNames="{Poly1,Poly1}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="C_10_12" layerNames="{Poly1,Active}" type="CONSPA" when="ALL" value="1.0"/>
        <LayersRule ruleName="U_10_12" layerNames="{Poly1,Active}" type="UCONSPA" when="ALL" value="1.0"/>
        <LayersRule ruleName="U_10_13" layerNames="{Poly1,Poly1_Cut}" type="UCONSPA" when="ALL" value="4.0"/>
        <LayersRule ruleName="U_11_11" layerNames="{Poly2,Poly2}" type="UCONSPA" when="ALL" value="3.0"/>
        <LayersRule ruleName="U_12_12" layerNames="{Active,Active}" type="UCONSPA" when="ALL" value="3.0"/>
        <LayersRule ruleName="C_13_13" layerNames="{Poly1_Cut,Poly1_Cut}" type="CONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="C_14_14" layerNames="{Poly2_Cut,Poly2_Cut}" type="CONSPA" when="ALL" value="2.0"/>
    </Foundry>
