Technology nmos
class com.sun.electric.technology.Technology
shortName=nMOS
techDesc=nMOS (Mead & Conway abstract rules)
Bits:  NONEGATEDARCS
isScaleRelevant=truenmos.Scale=2000.0(2000.0)
nmos.Foundry=NONE(NONE)
nmos.NumMetalLayers=1(1)
nmos.MininumResistance=50.0(50.0)
nmos.GateLengthSubtraction=0.0(0.0)
nmos.Gate Inclusion=false(false)
nmos.Ground Net Inclusion=false(false)
nmos.MaxSeriesResistance=10.0(10.0)
nmos.LogicalEffort.GateCapacitance=0.4(0.4)
nmos.LogicalEffort.WireRatio=0.16(0.16)
nmos.LogicalEffort.DiffAlpha=0.7(0.7)
ResolutionValueFornmos=0.0
TRANSPARENT_1=ff0000c8
TRANSPARENT_2=ffdc0078
TRANSPARENT_3=ff46fa46
TRANSPARENT_4=fffafa00
TRANSPARENT_5=ffb4b4b4
Layer Metal METAL1
	nmos.CIF.Metal=NM(NM)
	nmos.DXF.Metal=()
	nmos.Skill.Metal=()
	nmos.Resistance.Metal=0.03(0.03)
	nmos.Capacitance.Metal=0.03(0.03)
	nmos.EdgeCapacitance.Metal=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=1(1)
	color=ff0000c8(c8)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 2222 8888 0 0 2222 8888 0 0 2222 8888 0 0 2222 8888
	distance3D=11.0
	thickness3D=0.5
	mode3D=NONE
	factor3D=0.2
Layer Polysilicon POLY1
	nmos.CIF.Polysilicon=NP(NP)
	nmos.DXF.Polysilicon=()
	nmos.Skill.Polysilicon=()
	nmos.Resistance.Polysilicon=50.0(50.0)
	nmos.Capacitance.Polysilicon=0.04(0.04)
	nmos.EdgeCapacitance.Polysilicon=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=2(2)
	color=ffdc0078(dc0078)
	opacity=0.8(0.8)
	foreground=true
	pattern 1111 8888 4444 2222 1111 8888 4444 2222 1111 8888 4444 2222 1111 8888 4444 2222
	distance3D=9.0
	thickness3D=0.5
	mode3D=NONE
	factor3D=0.2
Layer Diffusion DIFF
	nmos.CIF.Diffusion=ND(ND)
	nmos.DXF.Diffusion=()
	nmos.Skill.Diffusion=()
	nmos.Resistance.Diffusion=10.0(10.0)
	nmos.Capacitance.Diffusion=0.1(0.1)
	nmos.EdgeCapacitance.Diffusion=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=3(3)
	color=ff46fa46(46fa46)
	opacity=0.8(0.8)
	foreground=true
	pattern 4444 1111 4444 1111 4444 1111 4444 1111 4444 1111 4444 1111 4444 1111 4444 1111
	distance3D=7.0
	thickness3D=2.0
	mode3D=NONE
	factor3D=0.2
Layer Implant IMPLANT DEPLETION HEAVY
	nmos.CIF.Implant=NI(NI)
	nmos.DXF.Implant=()
	nmos.Skill.Implant=()
	nmos.Resistance.Implant=0.0(0.0)
	nmos.Capacitance.Implant=0.0(0.0)
	nmos.EdgeCapacitance.Implant=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=4(4)
	color=fffafa00(fafa00)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 1111 0 0 0 1111 0 0 0 1111 0 0 0 1111 0
	distance3D=4.0
	thickness3D=5.0
	mode3D=SCREEN_DOOR
	factor3D=0.4
Layer Contact-Cut CONTACT1
	nmos.CIF.Contact-Cut=NC(NC)
	nmos.DXF.Contact-Cut=()
	nmos.Skill.Contact-Cut=()
	nmos.Resistance.Contact-Cut=0.0(0.0)
	nmos.Capacitance.Contact-Cut=0.0(0.0)
	nmos.EdgeCapacitance.Contact-Cut=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffb48200(b48200)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=9.0
	thickness3D=2.0
	mode3D=NONE
	factor3D=0.2
Layer Buried-Contact IMPLANT
	nmos.CIF.Buried-Contact=NB(NB)
	nmos.DXF.Buried-Contact=()
	nmos.Skill.Buried-Contact=()
	nmos.Resistance.Buried-Contact=0.0(0.0)
	nmos.Capacitance.Buried-Contact=0.0(0.0)
	nmos.EdgeCapacitance.Buried-Contact=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=5(5)
	color=ffb4b4b4(b4b4b4)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 2222 4444 8888 0 2222 4444 8888 0 2222 4444 8888 0 2222 4444 8888
	distance3D=4.0
	thickness3D=5.0
	mode3D=SCREEN_DOOR
	factor3D=0.4
Layer Overglass OVERGLASS
	nmos.CIF.Overglass=NG(NG)
	nmos.DXF.Overglass=()
	nmos.Skill.Overglass=()
	nmos.Resistance.Overglass=0.0(0.0)
	nmos.Capacitance.Overglass=0.0(0.0)
	nmos.EdgeCapacitance.Overglass=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 2222 5555 2222 0 2222 5555 2222 0 2222 5555 2222 0 2222 5555 2222
	distance3D=13.0
	thickness3D=2.0
	mode3D=NONE
	factor3D=0.2
Layer Light-Implant IMPLANT DEPLETION LIGHT
	nmos.CIF.Light-Implant=NJ(NJ)
	nmos.DXF.Light-Implant=()
	nmos.Skill.Light-Implant=()
	nmos.Resistance.Light-Implant=0.0(0.0)
	nmos.Capacitance.Light-Implant=0.0(0.0)
	nmos.EdgeCapacitance.Light-Implant=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff965a00(965a00)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 cccc 0 cccc 0 0 0 0 0 cccc 0 cccc 0 0 0 0
	distance3D=4.0
	thickness3D=5.0
	mode3D=SCREEN_DOOR
	factor3D=0.4
Layer Oversize-Contact CONTACT3
	nmos.CIF.Oversize-Contact=NO(NO)
	nmos.DXF.Oversize-Contact=()
	nmos.Skill.Oversize-Contact=()
	nmos.Resistance.Oversize-Contact=0.0(0.0)
	nmos.Capacitance.Oversize-Contact=0.0(0.0)
	nmos.EdgeCapacitance.Oversize-Contact=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=12.0
	thickness3D=1.0
	mode3D=NONE
	factor3D=0.2
Layer Hard-Enhancement IMPLANT ENHANCEMENT HEAVY
	nmos.CIF.Hard-Enhancement=NE(NE)
	nmos.DXF.Hard-Enhancement=()
	nmos.Skill.Hard-Enhancement=()
	nmos.Resistance.Hard-Enhancement=0.0(0.0)
	nmos.Capacitance.Hard-Enhancement=0.0(0.0)
	nmos.EdgeCapacitance.Hard-Enhancement=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 1010 2020 4040 8080 101 202 404 808 1010 2020 4040 8080 101 202 404 808
	distance3D=4.0
	thickness3D=5.0
	mode3D=SCREEN_DOOR
	factor3D=0.4
Layer Light-Enhancement IMPLANT ENHANCEMENT LIGHT
	nmos.CIF.Light-Enhancement=NF(NF)
	nmos.DXF.Light-Enhancement=()
	nmos.Skill.Light-Enhancement=()
	nmos.Resistance.Light-Enhancement=0.0(0.0)
	nmos.Capacitance.Light-Enhancement=0.0(0.0)
	nmos.EdgeCapacitance.Light-Enhancement=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ff000000(0)
	opacity=0.8(0.8)
	foreground=true
	pattern 4040 8080 101 202 101 8080 4040 2020 4040 8080 101 202 101 8080 4040 2020
	distance3D=4.0
	thickness3D=5.0
	mode3D=SCREEN_DOOR
	factor3D=0.4
Layer Transistor TRANSISTOR
	nmos.CIF.Transistor=()
	nmos.DXF.Transistor=()
	nmos.Skill.Transistor=()
	nmos.Resistance.Transistor=0.0(0.0)
	nmos.Capacitance.Transistor=0.0(0.0)
	nmos.EdgeCapacitance.Transistor=0.0(0.0)
	patternedOnDisplay=false(false)
	patternedOnPrinter=false(false)
	outlined=None(None)
	transparent=0(0)
	color=ffc8c8c8(c8c8c8)
	opacity=0.8(0.8)
	foreground=true
	pattern 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0
	distance3D=0.0
	thickness3D=0.0
	mode3D=NONE
	factor3D=0.0
ArcProto Metal metal-1
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForMetalINnmos=0.0
	baseExtend=1.5
	defaultLambdaBaseWidth=3.0
	diskOffset1=1.5
	diskOffset2=1.5
	DefaultAngleForMetalINnmos=90
	DefaultRigidForMetalINnmos=false
	DefaultFixedAngleForMetalINnmos=true
	DefaultExtendedForMetalINnmos=true
	DefaultDirectionalForMetalINnmos=false
		arcLayer layer=Metal style=FILLED extend=1.5
ArcProto Polysilicon poly-1
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForPolysiliconINnmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=1.0
	diskOffset2=1.0
	DefaultAngleForPolysiliconINnmos=90
	DefaultRigidForPolysiliconINnmos=false
	DefaultFixedAngleForPolysiliconINnmos=true
	DefaultExtendedForPolysiliconINnmos=true
	DefaultDirectionalForPolysiliconINnmos=false
		arcLayer layer=Polysilicon style=FILLED extend=1.0
ArcProto Diffusion diffusion
	isWipable=true
	isCurvable=false
	isSpecialArc=false
	isEdgeSelect=false
	isNotUsed=false
	isSkipSizeInPalette=false
	DefaultExtendForDiffusionINnmos=0.0
	baseExtend=1.0
	defaultLambdaBaseWidth=2.0
	diskOffset1=1.0
	diskOffset2=1.0
	DefaultAngleForDiffusionINnmos=90
	DefaultRigidForDiffusionINnmos=false
	DefaultFixedAngleForDiffusionINnmos=true
	DefaultExtendedForDiffusionINnmos=true
	DefaultDirectionalForDiffusionINnmos=false
		arcLayer layer=Diffusion style=FILLED extend=1.0
PrimitiveNode Metal-Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	baseRectangle=ERectangle[x=-1.5,y=-1.5,w=3.0,h=3.0]
	DefaultExtendXForMetal-PinINnmos=0.0
	DefaultExtendYForMetal-PinINnmos=0.0
	diskOffset1=1.5,1.5
	diskOffset2=1.5,1.5
	layers:
	layer=Metal port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.5 rm=0.5 ra=-1.5 bm=-0.5 ba=1.5 tm=0.5 ta=-1.5
		isolated=false negatable=false
		portArc Metal
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Polysilicon-Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForPolysilicon-PinINnmos=0.0
	DefaultExtendYForPolysilicon-PinINnmos=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Polysilicon port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port polysilicon angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Diffusion-Pin pin ARCSWIPE ARCSHRINK
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForDiffusion-PinINnmos=0.0
	DefaultExtendYForDiffusion-PinINnmos=0.0
	diskOffset1=1.0,1.0
	diskOffset2=1.0,1.0
	layers:
	layer=Diffusion port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port diffusion angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-Polysilicon-Con contact
	specialType=0 numMultiCuts=1
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForMetal-Polysilicon-ConINnmos=0.0
	DefaultExtendYForMetal-Polysilicon-ConINnmos=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Metal port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Contact-Cut port=0 style=CROSSED repr=3
		multiSizeX=2.0 multiSizeY=2.0 multiSep=2.0 multiSpe2D=2.0
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	port metal-poly angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Metal
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-Diffusion-Con contact
	specialType=0 numMultiCuts=1
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForMetal-Diffusion-ConINnmos=0.0
	DefaultExtendYForMetal-Diffusion-ConINnmos=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Diffusion port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Metal port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Contact-Cut port=0 style=CROSSED repr=3
		multiSizeX=2.0 multiSizeY=2.0 multiSep=2.0 multiSpe2D=2.0
		point xm=-0.5 xa=2.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=-2.0
	port metal-diff angle=0 range=180 topology=0 unknown
		lm=-0.5 la=1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Metal
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Butting-Con connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-2.0,w=6.0,h=4.0]
	baseRectangle=ERectangle[x=-3.0,y=-2.0,w=6.0,h=4.0]
	DefaultExtendXForButting-ConINnmos=0.0
	DefaultExtendYForButting-ConINnmos=0.0
	diskOffset1=3.0,2.0
	diskOffset2=3.0,2.0
	layers:
	layer=Diffusion port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.0 xa=1.0 ym=0.5 ya=0.0
	layer=Metal port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=0.0 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Contact-Cut port=0 style=CROSSED repr=1
		point xm=-0.5 xa=1.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=-1.0
	port but-diff angle=180 range=90 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=3.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Metal
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port but-poly angle=0 range=90 topology=0 unknown
		lm=0.5 la=-2.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Metal
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Buried-Con-Cross connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-2.0,w=6.0,h=4.0]
	baseRectangle=ERectangle[x=-3.0,y=-2.0,w=6.0,h=4.0]
	DefaultExtendXForBuried-Con-CrossINnmos=0.0
	DefaultExtendYForBuried-Con-CrossINnmos=0.0
	diskOffset1=3.0,2.0
	diskOffset2=3.0,2.0
	layers:
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=0.0
	layer=Diffusion port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-1.0
	layer=Buried-Contact port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port bur-diff-right angle=0 range=45 topology=0 unknown
		lm=0.5 la=-1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=2.0 tm=0.5 ta=-2.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-diff-left angle=180 range=45 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=1.0 bm=-0.5 ba=2.0 tm=0.5 ta=-2.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-bottom angle=270 range=45 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=-0.5 ba=1.0 tm=-0.5 ta=1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-top angle=90 range=45 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=0.5 ba=-1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Transistor nMOS-transistor NODESHRINK HOLDSTRACE
	specialType=1 numMultiCuts=0 3.0 1.0 1.0 2.0 1.0 1.0
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForTransistorINnmos=0.0
	DefaultExtendYForTransistorINnmos=0.0
	diskOffset1=3.0,3.0
	diskOffset2=1.0,1.0
	layers:
	layer=Polysilicon port=0 style=FILLED repr=1
		LWidth=1.0 rWidth=1.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-2.0
	layer=Diffusion port=0 style=FILLED repr=1
		LWidth=3.0 rWidth=3.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=2.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=0.0
	electricalLayers:
	layer=Polysilicon port=0 style=FILLED repr=1
		LWidth=1.0 rWidth=1.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-2.0
	layer=Diffusion port=1 style=FILLED repr=1
		LWidth=3.0 rWidth=0.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=2.0 ym=0.5 ya=-2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=0.0
	layer=Diffusion port=3 style=FILLED repr=1
		LWidth=0.0 rWidth=3.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=2.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=-2.0 ym=-0.5 ya=2.0
	port trans-poly-left angle=180 range=85 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=1.0 bm=-0.5 ba=3.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port trans-diff-top angle=90 range=85 topology=1 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=0.5 ba=-1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port trans-poly-right angle=0 range=85 topology=0 unknown
		lm=0.5 la=-1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=3.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port trans-diff-bottom angle=270 range=85 topology=3 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=-0.5 ba=1.0 tm=-0.5 ta=1.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Implant-Transistor depletion-nMOS-transistor NODESHRINK HOLDSTRACE
	specialType=1 numMultiCuts=0 4.0 1.0 1.0 2.0 1.0 1.0
	SizeOffset {X:[2.0,2.0] Y:[2.0,2.0]}
	fullRectangle=ERectangle[x=-3.0,y=-3.0,w=6.0,h=6.0]
	baseRectangle=ERectangle[x=-1.0,y=-1.0,w=2.0,h=2.0]
	DefaultExtendXForImplant-TransistorINnmos=0.0
	DefaultExtendYForImplant-TransistorINnmos=0.0
	diskOffset1=3.0,3.0
	diskOffset2=1.0,1.0
	layers:
	layer=Polysilicon port=0 style=FILLED repr=1
		LWidth=1.0 rWidth=1.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-2.0
	layer=Diffusion port=0 style=FILLED repr=1
		LWidth=3.0 rWidth=3.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=2.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=0.0
	layer=Implant port=-1 style=FILLED repr=1
		LWidth=2.5 rWidth=2.5 bExtend=1.5 tExtend=1.5
		point xm=-0.5 xa=0.5 ym=-0.5 ya=0.5
		point xm=0.5 xa=-0.5 ym=0.5 ya=-0.5
	electricalLayers:
	layer=Polysilicon port=0 style=FILLED repr=1
		LWidth=1.0 rWidth=1.0 bExtend=2.0 tExtend=2.0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=2.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-2.0
	layer=Implant port=-1 style=FILLED repr=1
		LWidth=2.5 rWidth=2.5 bExtend=1.5 tExtend=1.5
		point xm=-0.5 xa=0.5 ym=-0.5 ya=0.5
		point xm=0.5 xa=-0.5 ym=0.5 ya=-0.5
	layer=Diffusion port=1 style=FILLED repr=1
		LWidth=3.0 rWidth=0.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=2.0 ym=0.5 ya=-2.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=0.0
	layer=Diffusion port=3 style=FILLED repr=1
		LWidth=0.0 rWidth=3.0 bExtend=0.0 tExtend=0.0
		point xm=-0.5 xa=2.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=-2.0 ym=-0.5 ya=2.0
	port imp-trans-poly-left angle=180 range=85 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=1.0 bm=-0.5 ba=3.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port imp-trans-diff-top angle=90 range=85 topology=1 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=0.5 ba=-1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port imp-trans-poly-right angle=0 range=85 topology=0 unknown
		lm=0.5 la=-1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=3.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port imp-trans-diff-bottom angle=270 range=85 topology=3 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=-0.5 ba=1.0 tm=-0.5 ta=1.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Buried-Con-Cross-S connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	baseRectangle=ERectangle[x=-2.0,y=-2.0,w=4.0,h=4.0]
	DefaultExtendXForBuried-Con-Cross-SINnmos=0.0
	DefaultExtendYForBuried-Con-Cross-SINnmos=0.0
	diskOffset1=2.0,2.0
	diskOffset2=2.0,2.0
	layers:
	layer=Diffusion port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-1.0
	layer=Buried-Contact port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port bur-diff-left angle=180 range=45 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=1.0 bm=-0.5 ba=2.0 tm=0.5 ta=-2.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-bottom angle=270 range=45 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=-0.5 ta=1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-top angle=90 range=45 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-1.0 bm=0.5 ba=-1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-end-right angle=0 range=45 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-1.0 bm=-0.5 ba=2.0 tm=0.5 ta=-2.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Buried-Con-Cross-T connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.5,y=-2.0,w=5.0,h=4.0]
	baseRectangle=ERectangle[x=-2.5,y=-2.0,w=5.0,h=4.0]
	DefaultExtendXForBuried-Con-Cross-TINnmos=0.0
	DefaultExtendYForBuried-Con-Cross-TINnmos=0.0
	diskOffset1=2.5,2.0
	diskOffset2=2.5,2.0
	layers:
	layer=Diffusion port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-1.0
	layer=Buried-Contact port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=0.0
	port bur-poly-top angle=90 range=45 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-2.0 bm=0.5 ba=-1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-bottom angle=270 range=45 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-2.0 bm=-0.5 ba=1.0 tm=-0.5 ta=1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-diff-left angle=180 range=45 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=1.0 bm=-0.5 ba=2.0 tm=0.5 ta=-2.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Buried-Con-Polysurr connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.5,y=-2.0,w=5.0,h=4.0]
	baseRectangle=ERectangle[x=-2.5,y=-2.0,w=5.0,h=4.0]
	DefaultExtendXForBuried-Con-PolysurrINnmos=0.0
	DefaultExtendYForBuried-Con-PolysurrINnmos=0.0
	diskOffset1=2.5,2.0
	diskOffset2=2.5,2.0
	layers:
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Buried-Contact port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Diffusion port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=-1.0
	port bur-diff-left angle=180 range=45 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=1.0 bm=-0.5 ba=2.0 tm=0.5 ta=-2.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-3 angle=0 range=135 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-1 angle=0 range=135 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-2 angle=0 range=135 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Buried-Con-Diffsurr-I connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.5,y=-2.0,w=5.0,h=4.0]
	baseRectangle=ERectangle[x=-2.5,y=-2.0,w=5.0,h=4.0]
	DefaultExtendXForBuried-Con-Diffsurr-IINnmos=0.0
	DefaultExtendYForBuried-Con-Diffsurr-IINnmos=0.0
	diskOffset1=2.5,2.0
	diskOffset2=2.5,2.0
	layers:
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-1.0
	layer=Diffusion port=0 style=FILLED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=1.0
		point xm=-0.5 xa=0.0 ym=0.5 ya=-1.0
		point xm=-0.5 xa=1.0 ym=0.5 ya=-1.0
		point xm=-0.5 xa=1.0 ym=0.5 ya=0.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=0.0
		point xm=0.5 xa=-1.0 ym=-0.5 ya=0.0
		point xm=-0.5 xa=1.0 ym=-0.5 ya=0.0
		point xm=-0.5 xa=1.0 ym=-0.5 ya=1.0
	layer=Buried-Contact port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port bur-diff-left angle=180 range=45 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=1.0 bm=-0.5 ba=2.0 tm=0.5 ta=-2.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-right angle=0 range=45 topology=0 unknown
		lm=0.5 la=-1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=2.0 tm=0.5 ta=-2.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Buried-Con-Diffsurr-T connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-3.0,y=-2.0,w=6.0,h=4.0]
	baseRectangle=ERectangle[x=-3.0,y=-2.0,w=6.0,h=4.0]
	DefaultExtendXForBuried-Con-Diffsurr-TINnmos=0.0
	DefaultExtendYForBuried-Con-Diffsurr-TINnmos=0.0
	diskOffset1=3.0,2.0
	diskOffset2=3.0,2.0
	layers:
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=-2.0 ym=0.5 ya=0.0
	layer=Diffusion port=0 style=FILLED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.5 ya=-2.0
		point xm=-0.5 xa=1.0 ym=0.5 ya=-2.0
		point xm=-0.5 xa=1.0 ym=0.5 ya=-1.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=-1.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=-2.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-2.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	layer=Buried-Contact port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port bur-diff-left angle=180 range=45 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-top angle=90 range=45 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-3.0 bm=0.5 ba=-1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-diff-right angle=0 range=45 topology=0 unknown
		lm=0.5 la=-1.0 rm=0.5 ra=-1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Buried-Con-Diffsurr-L connection
	specialType=0 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=-2.5,y=-2.0,w=5.0,h=4.0]
	baseRectangle=ERectangle[x=-2.5,y=-2.0,w=5.0,h=4.0]
	DefaultExtendXForBuried-Con-Diffsurr-LINnmos=0.0
	DefaultExtendYForBuried-Con-Diffsurr-LINnmos=0.0
	diskOffset1=2.5,2.0
	diskOffset2=2.5,2.0
	layers:
	layer=Buried-Contact port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=-0.5 xa=2.0 ym=-0.5 ya=1.0
		point xm=0.5 xa=-1.0 ym=0.5 ya=0.0
	layer=Diffusion port=0 style=FILLED repr=0
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=-0.5 xa=0.0 ym=0.5 ya=-2.0
		point xm=-0.5 xa=1.0 ym=0.5 ya=-2.0
		point xm=-0.5 xa=1.0 ym=0.5 ya=-1.0
		point xm=0.5 xa=0.0 ym=0.5 ya=-1.0
		point xm=0.5 xa=0.0 ym=-0.5 ya=0.0
	port bur-diff-left angle=180 range=45 topology=0 unknown
		lm=-0.5 la=1.0 rm=-0.5 ra=1.0 bm=-0.5 ba=1.0 tm=0.5 ta=-3.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
	port bur-poly-top angle=90 range=45 topology=0 unknown
		lm=-0.5 la=3.0 rm=0.5 ra=-2.0 bm=0.5 ba=-1.0 tm=0.5 ta=-1.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Metal-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForMetal-NodeINnmos=1.5
	DefaultExtendYForMetal-NodeINnmos=1.5
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Metal port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port metal angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Metal
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Polysilicon-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForPolysilicon-NodeINnmos=1.0
	DefaultExtendYForPolysilicon-NodeINnmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Polysilicon port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port polysilicon angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Polysilicon
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Diffusion-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForDiffusion-NodeINnmos=1.0
	DefaultExtendYForDiffusion-NodeINnmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Diffusion port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port diffusion angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Diffusion
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Implant-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForImplant-NodeINnmos=1.0
	DefaultExtendYForImplant-NodeINnmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Implant port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port implant angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Cut-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForCut-NodeINnmos=1.0
	DefaultExtendYForCut-NodeINnmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Contact-Cut port=0 style=CROSSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port cut angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Buried-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForBuried-NodeINnmos=1.0
	DefaultExtendYForBuried-NodeINnmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Buried-Contact port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port buried angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Overglass-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForOverglass-NodeINnmos=1.0
	DefaultExtendYForOverglass-NodeINnmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Overglass port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port overglass angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Light-Implant-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForLight-Implant-NodeINnmos=1.0
	DefaultExtendYForLight-Implant-NodeINnmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Light-Implant port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port light-implant angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Oversize-Cut-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForOversize-Cut-NodeINnmos=1.0
	DefaultExtendYForOversize-Cut-NodeINnmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Oversize-Contact port=0 style=CLOSED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port oversize-contact angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Hard-Enhancement-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForHard-Enhancement-NodeINnmos=1.0
	DefaultExtendYForHard-Enhancement-NodeINnmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Hard-Enhancement port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port hard-enhancement angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
PrimitiveNode Light-Enhancement-Node pure-layer-node HOLDSTRACE
	specialType=2 numMultiCuts=0
	SizeOffset {X:[0.0,0.0] Y:[0.0,0.0]}
	fullRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	baseRectangle=ERectangle[x=0.0,y=0.0,w=0.0,h=0.0]
	DefaultExtendXForLight-Enhancement-NodeINnmos=1.0
	DefaultExtendYForLight-Enhancement-NodeINnmos=1.0
	diskOffset1=0.0,0.0
	diskOffset2=0.0,0.0
	layers:
	layer=Light-Enhancement port=0 style=FILLED repr=1
		point xm=-0.5 xa=0.0 ym=-0.5 ya=0.0
		point xm=0.5 xa=0.0 ym=0.5 ya=0.0
	port light-enhancement angle=0 range=180 topology=0 unknown
		lm=-0.5 la=0.0 rm=0.5 ra=0.0 bm=-0.5 ba=0.0 tm=0.5 ta=0.0
		isolated=false negatable=false
		portArc Universal
		portArc Invisible
		portArc Unrouted
Foundry NONE
	nmos.GDS.Metal=()
	nmos.GDS.Polysilicon=()
	nmos.GDS.Diffusion=()
	nmos.GDS.Implant=()
	nmos.GDS.Contact-Cut=()
	nmos.GDS.Buried-Contact=()
	nmos.GDS.Overglass=()
	nmos.GDS.Light-Implant=()
	nmos.GDS.Oversize-Contact=()
	nmos.GDS.Hard-Enhancement=()
	nmos.GDS.Light-Enhancement=()
	nmos.GDS.Transistor=()
SpiceHeader 1
	"*NMOS 4UM PROCESS"
	".OPTIONS DEFL=4UM DEFW=4UM DEFAS=80PM^2 DEFAD=80PM^2"
	".MODEL N NMOS LEVEL=1 VTO=1.1 KP=33UA/V^2 TOX=68NM GAMMA=.41"
	"+             LAMBDA=0.05 CGSO=0.18NF/M CGDO=0.18NF/M LD=0.4UM"
	"+             JS=.2A/M^2 CJ=.11MF/M^2"
	".MODEL D NMOS LEVEL=1 VTO=-3.4 KP=31UA/V^2 TOX=68NM GAMMA=.44"
	"+             LAMBDA=0.05 CGSO=0.18NF/M CGDO=0.18NF/M LD=0.4UM"
	"+             JS=.2A/M^2 CJ=.11MF/M^2"
	".MODEL DIFFCAP D CJO=.11MF/M^2"
SpiceHeader 3
	"*NMOS 4UM PROCESS"
	".OPTIONS DEFL=4UM DEFW=4UM DEFAS=80PM^2 DEFAD=80PM^2"
	"* RSH SET TO ZERO (MOSIS: RSH = 12)"
	".MODEL N NMOS LEVEL=3 VTO=0.849 LD=0.17U KP=2.98E-5 GAMMA=0.552"
	"+PHI=0.6 TOX=0.601E-7 NSUB=2.11E15 NSS=0 NFS=8.89E11 TPG=1 XJ=7.73E-7"
	"+UO=400 UEXP=1E-3 UCRIT=1.74E5 VMAX=1E5 NEFF=1E-2 DELTA=1.19"
	"+THETA=9.24E-3 ETA=0.77 KAPPA=3.25 RSH=0 CGSO=1.6E-10 CGDO=1.6E-10"
	"+CGBO=1.7E-10 CJ=1.1E-4 MJ=0.5 CJSW=1E-9"
	".MODEL D NMOS LEVEL=3 VTO=-3.07 LD=0.219U KP=2.76E-5 GAMMA=0.315"
	"+PHI=0.6 TOX=0.601E-7 NSUB=8.76E14 NSS=0 NFS=4.31E12 TPG=1 XJ=0.421U"
	"+UO=650 UEXP=1E-3 UCRIT=8.05E5 VMAX=1.96E5 NEFF=1E-2 DELTA=2.41"
	"+THETA=0 ETA=2.0 KAPPA=0.411 RSH=0 CGSO=1.6E-10 CGDO=1.6E-10"
	"+CGBO=1.7E-10 CJ=1.1E-4 MJ=0.5 CJSW=1E-9"
	"*MOSIS IS NOT RESPONSIBLE FOR THE FOLLOWING DIOD DATA"
	".MODEL DIFFCAP D CJO=.11MF/m^2"
 menu 0 0 arc Metal
 menu 0 1 nodeInst Metal-Pin:pin:
 menu 0 2 node Butting-Con
 menu 1 0 arc Polysilicon
 menu 1 1 nodeInst Polysilicon-Pin:pin:
 menu 1 2 node Metal-Polysilicon-Con
 menu 2 0 arc Diffusion
 menu 2 1 nodeInst Diffusion-Pin:pin:
 menu 2 2 node Metal-Diffusion-Con
 menu 3 0 node Buried-Con-Cross
 menu 3 1 node Transistor
 menu 3 2 node Implant-Transistor
 menu 4 0 node Buried-Con-Cross-S
 menu 4 1 node Buried-Con-Cross-T
 menu 4 2 node Buried-Con-Polysurr
 menu 5 0 node Buried-Con-Diffsurr-I
 menu 5 1 node Buried-Con-Diffsurr-T
 menu 5 2 node Buried-Con-Diffsurr-L
 menu 6 0 Pure
 menu 6 1 Misc.
 menu 6 2 Cell
    <Foundry name="NONE">
        <LayerRule ruleName="W_4" layerName="Contact-Cut" type="MINWID" when="ALL" value="2.0"/>
        <LayersRule ruleName="U_0_0" layerNames="{Metal,Metal}" type="UCONSPA" when="ALL" value="3.0"/>
        <LayersRule ruleName="U_1_1" layerNames="{Polysilicon,Polysilicon}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="C_1_2" layerNames="{Polysilicon,Diffusion}" type="CONSPA" when="ALL" value="0.0"/>
        <LayersRule ruleName="U_1_2" layerNames="{Polysilicon,Diffusion}" type="UCONSPA" when="ALL" value="1.0"/>
        <LayersRule ruleName="U_1_3" layerNames="{Polysilicon,Implant}" type="UCONSPA" when="ALL" value="1.0"/>
        <LayersRule ruleName="U_1_5" layerNames="{Polysilicon,Buried-Contact}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="U_2_2" layerNames="{Diffusion,Diffusion}" type="UCONSPA" when="ALL" value="3.0"/>
        <LayersRule ruleName="U_2_3" layerNames="{Diffusion,Implant}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="U_2_5" layerNames="{Diffusion,Buried-Contact}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="U_3_11" layerNames="{Implant,Transistor}" type="UCONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="C_4_4" layerNames="{Contact-Cut,Contact-Cut}" type="CONSPA" when="ALL" value="2.0"/>
        <LayersRule ruleName="U_4_11" layerNames="{Contact-Cut,Transistor}" type="UCONSPA" when="ALL" value="2.0"/>
    </Foundry>
